454531924040427
Connector_PinHeader_1.27mm
PinHeader_1x01_P1.27mm_Horizontal
Through hole angled pin header, 1x01, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x01 1.27mm single row
0
1
1
Connector_PinHeader_1.27mm
PinHeader_1x01_P1.27mm_Vertical
Through hole straight pin header, 1x01, 1.27mm pitch, single row
Through hole pin header THT 1x01 1.27mm single row
0
1
1
Connector_PinHeader_1.27mm
PinHeader_1x02_P1.27mm_Horizontal
Through hole angled pin header, 1x02, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x02 1.27mm single row
0
2
2
Connector_PinHeader_1.27mm
PinHeader_1x02_P1.27mm_Vertical
Through hole straight pin header, 1x02, 1.27mm pitch, single row
Through hole pin header THT 1x02 1.27mm single row
0
2
2
Connector_PinHeader_1.27mm
PinHeader_1x02_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x02, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x02 1.27mm single row style1 pin1 left
0
2
2
Connector_PinHeader_1.27mm
PinHeader_1x02_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x02, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x02 1.27mm single row style2 pin1 right
0
2
2
Connector_PinHeader_1.27mm
PinHeader_1x03_P1.27mm_Horizontal
Through hole angled pin header, 1x03, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x03 1.27mm single row
0
3
3
Connector_PinHeader_1.27mm
PinHeader_1x03_P1.27mm_Vertical
Through hole straight pin header, 1x03, 1.27mm pitch, single row
Through hole pin header THT 1x03 1.27mm single row
0
3
3
Connector_PinHeader_1.27mm
PinHeader_1x03_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x03, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x03 1.27mm single row style1 pin1 left
0
3
3
Connector_PinHeader_1.27mm
PinHeader_1x03_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x03, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x03 1.27mm single row style2 pin1 right
0
3
3
Connector_PinHeader_1.27mm
PinHeader_1x04_P1.27mm_Horizontal
Through hole angled pin header, 1x04, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x04 1.27mm single row
0
4
4
Connector_PinHeader_1.27mm
PinHeader_1x04_P1.27mm_Vertical
Through hole straight pin header, 1x04, 1.27mm pitch, single row
Through hole pin header THT 1x04 1.27mm single row
0
4
4
Connector_PinHeader_1.27mm
PinHeader_1x04_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x04, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x04 1.27mm single row style1 pin1 left
0
4
4
Connector_PinHeader_1.27mm
PinHeader_1x04_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x04, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x04 1.27mm single row style2 pin1 right
0
4
4
Connector_PinHeader_1.27mm
PinHeader_1x05_P1.27mm_Horizontal
Through hole angled pin header, 1x05, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x05 1.27mm single row
0
5
5
Connector_PinHeader_1.27mm
PinHeader_1x05_P1.27mm_Vertical
Through hole straight pin header, 1x05, 1.27mm pitch, single row
Through hole pin header THT 1x05 1.27mm single row
0
5
5
Connector_PinHeader_1.27mm
PinHeader_1x05_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x05, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x05 1.27mm single row style1 pin1 left
0
5
5
Connector_PinHeader_1.27mm
PinHeader_1x05_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x05, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x05 1.27mm single row style2 pin1 right
0
5
5
Connector_PinHeader_1.27mm
PinHeader_1x06_P1.27mm_Horizontal
Through hole angled pin header, 1x06, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x06 1.27mm single row
0
6
6
Connector_PinHeader_1.27mm
PinHeader_1x06_P1.27mm_Vertical
Through hole straight pin header, 1x06, 1.27mm pitch, single row
Through hole pin header THT 1x06 1.27mm single row
0
6
6
Connector_PinHeader_1.27mm
PinHeader_1x06_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x06, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x06 1.27mm single row style1 pin1 left
0
6
6
Connector_PinHeader_1.27mm
PinHeader_1x06_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x06, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x06 1.27mm single row style2 pin1 right
0
6
6
Connector_PinHeader_1.27mm
PinHeader_1x07_P1.27mm_Horizontal
Through hole angled pin header, 1x07, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x07 1.27mm single row
0
7
7
Connector_PinHeader_1.27mm
PinHeader_1x07_P1.27mm_Vertical
Through hole straight pin header, 1x07, 1.27mm pitch, single row
Through hole pin header THT 1x07 1.27mm single row
0
7
7
Connector_PinHeader_1.27mm
PinHeader_1x07_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x07, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x07 1.27mm single row style1 pin1 left
0
7
7
Connector_PinHeader_1.27mm
PinHeader_1x07_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x07, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x07 1.27mm single row style2 pin1 right
0
7
7
Connector_PinHeader_1.27mm
PinHeader_1x08_P1.27mm_Horizontal
Through hole angled pin header, 1x08, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x08 1.27mm single row
0
8
8
Connector_PinHeader_1.27mm
PinHeader_1x08_P1.27mm_Vertical
Through hole straight pin header, 1x08, 1.27mm pitch, single row
Through hole pin header THT 1x08 1.27mm single row
0
8
8
Connector_PinHeader_1.27mm
PinHeader_1x08_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x08, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x08 1.27mm single row style1 pin1 left
0
8
8
Connector_PinHeader_1.27mm
PinHeader_1x08_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x08, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x08 1.27mm single row style2 pin1 right
0
8
8
Connector_PinHeader_1.27mm
PinHeader_1x09_P1.27mm_Horizontal
Through hole angled pin header, 1x09, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x09 1.27mm single row
0
9
9
Connector_PinHeader_1.27mm
PinHeader_1x09_P1.27mm_Vertical
Through hole straight pin header, 1x09, 1.27mm pitch, single row
Through hole pin header THT 1x09 1.27mm single row
0
9
9
Connector_PinHeader_1.27mm
PinHeader_1x09_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x09, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x09 1.27mm single row style1 pin1 left
0
9
9
Connector_PinHeader_1.27mm
PinHeader_1x09_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x09, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x09 1.27mm single row style2 pin1 right
0
9
9
Connector_PinHeader_1.27mm
PinHeader_1x10_P1.27mm_Horizontal
Through hole angled pin header, 1x10, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x10 1.27mm single row
0
10
10
Connector_PinHeader_1.27mm
PinHeader_1x10_P1.27mm_Vertical
Through hole straight pin header, 1x10, 1.27mm pitch, single row
Through hole pin header THT 1x10 1.27mm single row
0
10
10
Connector_PinHeader_1.27mm
PinHeader_1x10_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x10, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x10 1.27mm single row style1 pin1 left
0
10
10
Connector_PinHeader_1.27mm
PinHeader_1x10_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x10, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x10 1.27mm single row style2 pin1 right
0
10
10
Connector_PinHeader_1.27mm
PinHeader_1x11_P1.27mm_Horizontal
Through hole angled pin header, 1x11, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x11 1.27mm single row
0
11
11
Connector_PinHeader_1.27mm
PinHeader_1x11_P1.27mm_Vertical
Through hole straight pin header, 1x11, 1.27mm pitch, single row
Through hole pin header THT 1x11 1.27mm single row
0
11
11
Connector_PinHeader_1.27mm
PinHeader_1x11_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x11, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x11 1.27mm single row style1 pin1 left
0
11
11
Connector_PinHeader_1.27mm
PinHeader_1x11_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x11, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x11 1.27mm single row style2 pin1 right
0
11
11
Connector_PinHeader_1.27mm
PinHeader_1x12_P1.27mm_Horizontal
Through hole angled pin header, 1x12, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x12 1.27mm single row
0
12
12
Connector_PinHeader_1.27mm
PinHeader_1x12_P1.27mm_Vertical
Through hole straight pin header, 1x12, 1.27mm pitch, single row
Through hole pin header THT 1x12 1.27mm single row
0
12
12
Connector_PinHeader_1.27mm
PinHeader_1x12_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x12, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x12 1.27mm single row style1 pin1 left
0
12
12
Connector_PinHeader_1.27mm
PinHeader_1x12_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x12, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x12 1.27mm single row style2 pin1 right
0
12
12
Connector_PinHeader_1.27mm
PinHeader_1x13_P1.27mm_Horizontal
Through hole angled pin header, 1x13, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x13 1.27mm single row
0
13
13
Connector_PinHeader_1.27mm
PinHeader_1x13_P1.27mm_Vertical
Through hole straight pin header, 1x13, 1.27mm pitch, single row
Through hole pin header THT 1x13 1.27mm single row
0
13
13
Connector_PinHeader_1.27mm
PinHeader_1x13_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x13, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x13 1.27mm single row style1 pin1 left
0
13
13
Connector_PinHeader_1.27mm
PinHeader_1x13_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x13, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x13 1.27mm single row style2 pin1 right
0
13
13
Connector_PinHeader_1.27mm
PinHeader_1x14_P1.27mm_Horizontal
Through hole angled pin header, 1x14, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x14 1.27mm single row
0
14
14
Connector_PinHeader_1.27mm
PinHeader_1x14_P1.27mm_Vertical
Through hole straight pin header, 1x14, 1.27mm pitch, single row
Through hole pin header THT 1x14 1.27mm single row
0
14
14
Connector_PinHeader_1.27mm
PinHeader_1x14_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x14, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x14 1.27mm single row style1 pin1 left
0
14
14
Connector_PinHeader_1.27mm
PinHeader_1x14_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x14, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x14 1.27mm single row style2 pin1 right
0
14
14
Connector_PinHeader_1.27mm
PinHeader_1x15_P1.27mm_Horizontal
Through hole angled pin header, 1x15, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x15 1.27mm single row
0
15
15
Connector_PinHeader_1.27mm
PinHeader_1x15_P1.27mm_Vertical
Through hole straight pin header, 1x15, 1.27mm pitch, single row
Through hole pin header THT 1x15 1.27mm single row
0
15
15
Connector_PinHeader_1.27mm
PinHeader_1x15_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x15, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x15 1.27mm single row style1 pin1 left
0
15
15
Connector_PinHeader_1.27mm
PinHeader_1x15_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x15, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x15 1.27mm single row style2 pin1 right
0
15
15
Connector_PinHeader_1.27mm
PinHeader_1x16_P1.27mm_Horizontal
Through hole angled pin header, 1x16, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x16 1.27mm single row
0
16
16
Connector_PinHeader_1.27mm
PinHeader_1x16_P1.27mm_Vertical
Through hole straight pin header, 1x16, 1.27mm pitch, single row
Through hole pin header THT 1x16 1.27mm single row
0
16
16
Connector_PinHeader_1.27mm
PinHeader_1x16_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x16, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x16 1.27mm single row style1 pin1 left
0
16
16
Connector_PinHeader_1.27mm
PinHeader_1x16_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x16, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x16 1.27mm single row style2 pin1 right
0
16
16
Connector_PinHeader_1.27mm
PinHeader_1x17_P1.27mm_Horizontal
Through hole angled pin header, 1x17, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x17 1.27mm single row
0
17
17
Connector_PinHeader_1.27mm
PinHeader_1x17_P1.27mm_Vertical
Through hole straight pin header, 1x17, 1.27mm pitch, single row
Through hole pin header THT 1x17 1.27mm single row
0
17
17
Connector_PinHeader_1.27mm
PinHeader_1x17_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x17, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x17 1.27mm single row style1 pin1 left
0
17
17
Connector_PinHeader_1.27mm
PinHeader_1x17_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x17, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x17 1.27mm single row style2 pin1 right
0
17
17
Connector_PinHeader_1.27mm
PinHeader_1x18_P1.27mm_Horizontal
Through hole angled pin header, 1x18, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x18 1.27mm single row
0
18
18
Connector_PinHeader_1.27mm
PinHeader_1x18_P1.27mm_Vertical
Through hole straight pin header, 1x18, 1.27mm pitch, single row
Through hole pin header THT 1x18 1.27mm single row
0
18
18
Connector_PinHeader_1.27mm
PinHeader_1x18_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x18, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x18 1.27mm single row style1 pin1 left
0
18
18
Connector_PinHeader_1.27mm
PinHeader_1x18_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x18, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x18 1.27mm single row style2 pin1 right
0
18
18
Connector_PinHeader_1.27mm
PinHeader_1x19_P1.27mm_Horizontal
Through hole angled pin header, 1x19, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x19 1.27mm single row
0
19
19
Connector_PinHeader_1.27mm
PinHeader_1x19_P1.27mm_Vertical
Through hole straight pin header, 1x19, 1.27mm pitch, single row
Through hole pin header THT 1x19 1.27mm single row
0
19
19
Connector_PinHeader_1.27mm
PinHeader_1x19_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x19, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x19 1.27mm single row style1 pin1 left
0
19
19
Connector_PinHeader_1.27mm
PinHeader_1x19_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x19, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x19 1.27mm single row style2 pin1 right
0
19
19
Connector_PinHeader_1.27mm
PinHeader_1x20_P1.27mm_Horizontal
Through hole angled pin header, 1x20, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x20 1.27mm single row
0
20
20
Connector_PinHeader_1.27mm
PinHeader_1x20_P1.27mm_Vertical
Through hole straight pin header, 1x20, 1.27mm pitch, single row
Through hole pin header THT 1x20 1.27mm single row
0
20
20
Connector_PinHeader_1.27mm
PinHeader_1x20_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x20, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x20 1.27mm single row style1 pin1 left
0
20
20
Connector_PinHeader_1.27mm
PinHeader_1x20_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x20, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x20 1.27mm single row style2 pin1 right
0
20
20
Connector_PinHeader_1.27mm
PinHeader_1x21_P1.27mm_Horizontal
Through hole angled pin header, 1x21, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x21 1.27mm single row
0
21
21
Connector_PinHeader_1.27mm
PinHeader_1x21_P1.27mm_Vertical
Through hole straight pin header, 1x21, 1.27mm pitch, single row
Through hole pin header THT 1x21 1.27mm single row
0
21
21
Connector_PinHeader_1.27mm
PinHeader_1x21_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x21, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x21 1.27mm single row style1 pin1 left
0
21
21
Connector_PinHeader_1.27mm
PinHeader_1x21_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x21, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x21 1.27mm single row style2 pin1 right
0
21
21
Connector_PinHeader_1.27mm
PinHeader_1x22_P1.27mm_Horizontal
Through hole angled pin header, 1x22, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x22 1.27mm single row
0
22
22
Connector_PinHeader_1.27mm
PinHeader_1x22_P1.27mm_Vertical
Through hole straight pin header, 1x22, 1.27mm pitch, single row
Through hole pin header THT 1x22 1.27mm single row
0
22
22
Connector_PinHeader_1.27mm
PinHeader_1x22_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x22, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x22 1.27mm single row style1 pin1 left
0
22
22
Connector_PinHeader_1.27mm
PinHeader_1x22_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x22, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x22 1.27mm single row style2 pin1 right
0
22
22
Connector_PinHeader_1.27mm
PinHeader_1x23_P1.27mm_Horizontal
Through hole angled pin header, 1x23, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x23 1.27mm single row
0
23
23
Connector_PinHeader_1.27mm
PinHeader_1x23_P1.27mm_Vertical
Through hole straight pin header, 1x23, 1.27mm pitch, single row
Through hole pin header THT 1x23 1.27mm single row
0
23
23
Connector_PinHeader_1.27mm
PinHeader_1x23_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x23, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x23 1.27mm single row style1 pin1 left
0
23
23
Connector_PinHeader_1.27mm
PinHeader_1x23_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x23, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x23 1.27mm single row style2 pin1 right
0
23
23
Connector_PinHeader_1.27mm
PinHeader_1x24_P1.27mm_Horizontal
Through hole angled pin header, 1x24, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x24 1.27mm single row
0
24
24
Connector_PinHeader_1.27mm
PinHeader_1x24_P1.27mm_Vertical
Through hole straight pin header, 1x24, 1.27mm pitch, single row
Through hole pin header THT 1x24 1.27mm single row
0
24
24
Connector_PinHeader_1.27mm
PinHeader_1x24_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x24, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x24 1.27mm single row style1 pin1 left
0
24
24
Connector_PinHeader_1.27mm
PinHeader_1x24_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x24, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x24 1.27mm single row style2 pin1 right
0
24
24
Connector_PinHeader_1.27mm
PinHeader_1x25_P1.27mm_Horizontal
Through hole angled pin header, 1x25, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x25 1.27mm single row
0
25
25
Connector_PinHeader_1.27mm
PinHeader_1x25_P1.27mm_Vertical
Through hole straight pin header, 1x25, 1.27mm pitch, single row
Through hole pin header THT 1x25 1.27mm single row
0
25
25
Connector_PinHeader_1.27mm
PinHeader_1x25_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x25, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x25 1.27mm single row style1 pin1 left
0
25
25
Connector_PinHeader_1.27mm
PinHeader_1x25_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x25, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x25 1.27mm single row style2 pin1 right
0
25
25
Connector_PinHeader_1.27mm
PinHeader_1x26_P1.27mm_Horizontal
Through hole angled pin header, 1x26, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x26 1.27mm single row
0
26
26
Connector_PinHeader_1.27mm
PinHeader_1x26_P1.27mm_Vertical
Through hole straight pin header, 1x26, 1.27mm pitch, single row
Through hole pin header THT 1x26 1.27mm single row
0
26
26
Connector_PinHeader_1.27mm
PinHeader_1x26_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x26, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x26 1.27mm single row style1 pin1 left
0
26
26
Connector_PinHeader_1.27mm
PinHeader_1x26_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x26, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x26 1.27mm single row style2 pin1 right
0
26
26
Connector_PinHeader_1.27mm
PinHeader_1x27_P1.27mm_Horizontal
Through hole angled pin header, 1x27, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x27 1.27mm single row
0
27
27
Connector_PinHeader_1.27mm
PinHeader_1x27_P1.27mm_Vertical
Through hole straight pin header, 1x27, 1.27mm pitch, single row
Through hole pin header THT 1x27 1.27mm single row
0
27
27
Connector_PinHeader_1.27mm
PinHeader_1x27_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x27, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x27 1.27mm single row style1 pin1 left
0
27
27
Connector_PinHeader_1.27mm
PinHeader_1x27_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x27, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x27 1.27mm single row style2 pin1 right
0
27
27
Connector_PinHeader_1.27mm
PinHeader_1x28_P1.27mm_Horizontal
Through hole angled pin header, 1x28, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x28 1.27mm single row
0
28
28
Connector_PinHeader_1.27mm
PinHeader_1x28_P1.27mm_Vertical
Through hole straight pin header, 1x28, 1.27mm pitch, single row
Through hole pin header THT 1x28 1.27mm single row
0
28
28
Connector_PinHeader_1.27mm
PinHeader_1x28_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x28, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x28 1.27mm single row style1 pin1 left
0
28
28
Connector_PinHeader_1.27mm
PinHeader_1x28_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x28, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x28 1.27mm single row style2 pin1 right
0
28
28
Connector_PinHeader_1.27mm
PinHeader_1x29_P1.27mm_Horizontal
Through hole angled pin header, 1x29, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x29 1.27mm single row
0
29
29
Connector_PinHeader_1.27mm
PinHeader_1x29_P1.27mm_Vertical
Through hole straight pin header, 1x29, 1.27mm pitch, single row
Through hole pin header THT 1x29 1.27mm single row
0
29
29
Connector_PinHeader_1.27mm
PinHeader_1x29_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x29, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x29 1.27mm single row style1 pin1 left
0
29
29
Connector_PinHeader_1.27mm
PinHeader_1x29_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x29, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x29 1.27mm single row style2 pin1 right
0
29
29
Connector_PinHeader_1.27mm
PinHeader_1x30_P1.27mm_Horizontal
Through hole angled pin header, 1x30, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x30 1.27mm single row
0
30
30
Connector_PinHeader_1.27mm
PinHeader_1x30_P1.27mm_Vertical
Through hole straight pin header, 1x30, 1.27mm pitch, single row
Through hole pin header THT 1x30 1.27mm single row
0
30
30
Connector_PinHeader_1.27mm
PinHeader_1x30_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x30, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x30 1.27mm single row style1 pin1 left
0
30
30
Connector_PinHeader_1.27mm
PinHeader_1x30_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x30, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x30 1.27mm single row style2 pin1 right
0
30
30
Connector_PinHeader_1.27mm
PinHeader_1x31_P1.27mm_Horizontal
Through hole angled pin header, 1x31, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x31 1.27mm single row
0
31
31
Connector_PinHeader_1.27mm
PinHeader_1x31_P1.27mm_Vertical
Through hole straight pin header, 1x31, 1.27mm pitch, single row
Through hole pin header THT 1x31 1.27mm single row
0
31
31
Connector_PinHeader_1.27mm
PinHeader_1x31_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x31, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x31 1.27mm single row style1 pin1 left
0
31
31
Connector_PinHeader_1.27mm
PinHeader_1x31_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x31, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x31 1.27mm single row style2 pin1 right
0
31
31
Connector_PinHeader_1.27mm
PinHeader_1x32_P1.27mm_Horizontal
Through hole angled pin header, 1x32, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x32 1.27mm single row
0
32
32
Connector_PinHeader_1.27mm
PinHeader_1x32_P1.27mm_Vertical
Through hole straight pin header, 1x32, 1.27mm pitch, single row
Through hole pin header THT 1x32 1.27mm single row
0
32
32
Connector_PinHeader_1.27mm
PinHeader_1x32_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x32, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x32 1.27mm single row style1 pin1 left
0
32
32
Connector_PinHeader_1.27mm
PinHeader_1x32_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x32, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x32 1.27mm single row style2 pin1 right
0
32
32
Connector_PinHeader_1.27mm
PinHeader_1x33_P1.27mm_Horizontal
Through hole angled pin header, 1x33, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x33 1.27mm single row
0
33
33
Connector_PinHeader_1.27mm
PinHeader_1x33_P1.27mm_Vertical
Through hole straight pin header, 1x33, 1.27mm pitch, single row
Through hole pin header THT 1x33 1.27mm single row
0
33
33
Connector_PinHeader_1.27mm
PinHeader_1x33_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x33, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x33 1.27mm single row style1 pin1 left
0
33
33
Connector_PinHeader_1.27mm
PinHeader_1x33_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x33, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x33 1.27mm single row style2 pin1 right
0
33
33
Connector_PinHeader_1.27mm
PinHeader_1x34_P1.27mm_Horizontal
Through hole angled pin header, 1x34, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x34 1.27mm single row
0
34
34
Connector_PinHeader_1.27mm
PinHeader_1x34_P1.27mm_Vertical
Through hole straight pin header, 1x34, 1.27mm pitch, single row
Through hole pin header THT 1x34 1.27mm single row
0
34
34
Connector_PinHeader_1.27mm
PinHeader_1x34_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x34, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x34 1.27mm single row style1 pin1 left
0
34
34
Connector_PinHeader_1.27mm
PinHeader_1x34_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x34, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x34 1.27mm single row style2 pin1 right
0
34
34
Connector_PinHeader_1.27mm
PinHeader_1x35_P1.27mm_Horizontal
Through hole angled pin header, 1x35, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x35 1.27mm single row
0
35
35
Connector_PinHeader_1.27mm
PinHeader_1x35_P1.27mm_Vertical
Through hole straight pin header, 1x35, 1.27mm pitch, single row
Through hole pin header THT 1x35 1.27mm single row
0
35
35
Connector_PinHeader_1.27mm
PinHeader_1x35_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x35, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x35 1.27mm single row style1 pin1 left
0
35
35
Connector_PinHeader_1.27mm
PinHeader_1x35_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x35, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x35 1.27mm single row style2 pin1 right
0
35
35
Connector_PinHeader_1.27mm
PinHeader_1x36_P1.27mm_Horizontal
Through hole angled pin header, 1x36, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x36 1.27mm single row
0
36
36
Connector_PinHeader_1.27mm
PinHeader_1x36_P1.27mm_Vertical
Through hole straight pin header, 1x36, 1.27mm pitch, single row
Through hole pin header THT 1x36 1.27mm single row
0
36
36
Connector_PinHeader_1.27mm
PinHeader_1x36_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x36, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x36 1.27mm single row style1 pin1 left
0
36
36
Connector_PinHeader_1.27mm
PinHeader_1x36_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x36, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x36 1.27mm single row style2 pin1 right
0
36
36
Connector_PinHeader_1.27mm
PinHeader_1x37_P1.27mm_Horizontal
Through hole angled pin header, 1x37, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x37 1.27mm single row
0
37
37
Connector_PinHeader_1.27mm
PinHeader_1x37_P1.27mm_Vertical
Through hole straight pin header, 1x37, 1.27mm pitch, single row
Through hole pin header THT 1x37 1.27mm single row
0
37
37
Connector_PinHeader_1.27mm
PinHeader_1x37_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x37, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x37 1.27mm single row style1 pin1 left
0
37
37
Connector_PinHeader_1.27mm
PinHeader_1x37_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x37, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x37 1.27mm single row style2 pin1 right
0
37
37
Connector_PinHeader_1.27mm
PinHeader_1x38_P1.27mm_Horizontal
Through hole angled pin header, 1x38, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x38 1.27mm single row
0
38
38
Connector_PinHeader_1.27mm
PinHeader_1x38_P1.27mm_Vertical
Through hole straight pin header, 1x38, 1.27mm pitch, single row
Through hole pin header THT 1x38 1.27mm single row
0
38
38
Connector_PinHeader_1.27mm
PinHeader_1x38_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x38, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x38 1.27mm single row style1 pin1 left
0
38
38
Connector_PinHeader_1.27mm
PinHeader_1x38_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x38, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x38 1.27mm single row style2 pin1 right
0
38
38
Connector_PinHeader_1.27mm
PinHeader_1x39_P1.27mm_Horizontal
Through hole angled pin header, 1x39, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x39 1.27mm single row
0
39
39
Connector_PinHeader_1.27mm
PinHeader_1x39_P1.27mm_Vertical
Through hole straight pin header, 1x39, 1.27mm pitch, single row
Through hole pin header THT 1x39 1.27mm single row
0
39
39
Connector_PinHeader_1.27mm
PinHeader_1x39_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x39, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x39 1.27mm single row style1 pin1 left
0
39
39
Connector_PinHeader_1.27mm
PinHeader_1x39_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x39, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x39 1.27mm single row style2 pin1 right
0
39
39
Connector_PinHeader_1.27mm
PinHeader_1x40_P1.27mm_Horizontal
Through hole angled pin header, 1x40, 1.27mm pitch, 4.0mm pin length, single row
Through hole angled pin header THT 1x40 1.27mm single row
0
40
40
Connector_PinHeader_1.27mm
PinHeader_1x40_P1.27mm_Vertical
Through hole straight pin header, 1x40, 1.27mm pitch, single row
Through hole pin header THT 1x40 1.27mm single row
0
40
40
Connector_PinHeader_1.27mm
PinHeader_1x40_P1.27mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x40, 1.27mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x40 1.27mm single row style1 pin1 left
0
40
40
Connector_PinHeader_1.27mm
PinHeader_1x40_P1.27mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x40, 1.27mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x40 1.27mm single row style2 pin1 right
0
40
40
Connector_PinHeader_1.27mm
PinHeader_2x01_P1.27mm_Horizontal
Through hole angled pin header, 2x01, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x01 1.27mm double row
0
2
2
Connector_PinHeader_1.27mm
PinHeader_2x01_P1.27mm_Vertical
Through hole straight pin header, 2x01, 1.27mm pitch, double rows
Through hole pin header THT 2x01 1.27mm double row
0
2
2
Connector_PinHeader_1.27mm
PinHeader_2x01_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x01, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x01 1.27mm double row
0
2
2
Connector_PinHeader_1.27mm
PinHeader_2x02_P1.27mm_Horizontal
Through hole angled pin header, 2x02, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x02 1.27mm double row
0
4
4
Connector_PinHeader_1.27mm
PinHeader_2x02_P1.27mm_Vertical
Through hole straight pin header, 2x02, 1.27mm pitch, double rows
Through hole pin header THT 2x02 1.27mm double row
0
4
4
Connector_PinHeader_1.27mm
PinHeader_2x02_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x02, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x02 1.27mm double row
0
4
4
Connector_PinHeader_1.27mm
PinHeader_2x03_P1.27mm_Horizontal
Through hole angled pin header, 2x03, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x03 1.27mm double row
0
6
6
Connector_PinHeader_1.27mm
PinHeader_2x03_P1.27mm_Vertical
Through hole straight pin header, 2x03, 1.27mm pitch, double rows
Through hole pin header THT 2x03 1.27mm double row
0
6
6
Connector_PinHeader_1.27mm
PinHeader_2x03_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x03, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x03 1.27mm double row
0
6
6
Connector_PinHeader_1.27mm
PinHeader_2x04_P1.27mm_Horizontal
Through hole angled pin header, 2x04, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x04 1.27mm double row
0
8
8
Connector_PinHeader_1.27mm
PinHeader_2x04_P1.27mm_Vertical
Through hole straight pin header, 2x04, 1.27mm pitch, double rows
Through hole pin header THT 2x04 1.27mm double row
0
8
8
Connector_PinHeader_1.27mm
PinHeader_2x04_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x04, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x04 1.27mm double row
0
8
8
Connector_PinHeader_1.27mm
PinHeader_2x05_P1.27mm_Horizontal
Through hole angled pin header, 2x05, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x05 1.27mm double row
0
10
10
Connector_PinHeader_1.27mm
PinHeader_2x05_P1.27mm_Vertical
Through hole straight pin header, 2x05, 1.27mm pitch, double rows
Through hole pin header THT 2x05 1.27mm double row
0
10
10
Connector_PinHeader_1.27mm
PinHeader_2x05_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x05 1.27mm double row
0
10
10
Connector_PinHeader_1.27mm
PinHeader_2x06_P1.27mm_Horizontal
Through hole angled pin header, 2x06, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x06 1.27mm double row
0
12
12
Connector_PinHeader_1.27mm
PinHeader_2x06_P1.27mm_Vertical
Through hole straight pin header, 2x06, 1.27mm pitch, double rows
Through hole pin header THT 2x06 1.27mm double row
0
12
12
Connector_PinHeader_1.27mm
PinHeader_2x06_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x06, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x06 1.27mm double row
0
12
12
Connector_PinHeader_1.27mm
PinHeader_2x07_P1.27mm_Horizontal
Through hole angled pin header, 2x07, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x07 1.27mm double row
0
14
14
Connector_PinHeader_1.27mm
PinHeader_2x07_P1.27mm_Vertical
Through hole straight pin header, 2x07, 1.27mm pitch, double rows
Through hole pin header THT 2x07 1.27mm double row
0
14
14
Connector_PinHeader_1.27mm
PinHeader_2x07_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x07, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x07 1.27mm double row
0
14
14
Connector_PinHeader_1.27mm
PinHeader_2x08_P1.27mm_Horizontal
Through hole angled pin header, 2x08, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x08 1.27mm double row
0
16
16
Connector_PinHeader_1.27mm
PinHeader_2x08_P1.27mm_Vertical
Through hole straight pin header, 2x08, 1.27mm pitch, double rows
Through hole pin header THT 2x08 1.27mm double row
0
16
16
Connector_PinHeader_1.27mm
PinHeader_2x08_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x08, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x08 1.27mm double row
0
16
16
Connector_PinHeader_1.27mm
PinHeader_2x09_P1.27mm_Horizontal
Through hole angled pin header, 2x09, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x09 1.27mm double row
0
18
18
Connector_PinHeader_1.27mm
PinHeader_2x09_P1.27mm_Vertical
Through hole straight pin header, 2x09, 1.27mm pitch, double rows
Through hole pin header THT 2x09 1.27mm double row
0
18
18
Connector_PinHeader_1.27mm
PinHeader_2x09_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x09, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x09 1.27mm double row
0
18
18
Connector_PinHeader_1.27mm
PinHeader_2x10_P1.27mm_Horizontal
Through hole angled pin header, 2x10, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x10 1.27mm double row
0
20
20
Connector_PinHeader_1.27mm
PinHeader_2x10_P1.27mm_Vertical
Through hole straight pin header, 2x10, 1.27mm pitch, double rows
Through hole pin header THT 2x10 1.27mm double row
0
20
20
Connector_PinHeader_1.27mm
PinHeader_2x10_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x10, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x10 1.27mm double row
0
20
20
Connector_PinHeader_1.27mm
PinHeader_2x11_P1.27mm_Horizontal
Through hole angled pin header, 2x11, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x11 1.27mm double row
0
22
22
Connector_PinHeader_1.27mm
PinHeader_2x11_P1.27mm_Vertical
Through hole straight pin header, 2x11, 1.27mm pitch, double rows
Through hole pin header THT 2x11 1.27mm double row
0
22
22
Connector_PinHeader_1.27mm
PinHeader_2x11_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x11, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x11 1.27mm double row
0
22
22
Connector_PinHeader_1.27mm
PinHeader_2x12_P1.27mm_Horizontal
Through hole angled pin header, 2x12, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x12 1.27mm double row
0
24
24
Connector_PinHeader_1.27mm
PinHeader_2x12_P1.27mm_Vertical
Through hole straight pin header, 2x12, 1.27mm pitch, double rows
Through hole pin header THT 2x12 1.27mm double row
0
24
24
Connector_PinHeader_1.27mm
PinHeader_2x12_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x12, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x12 1.27mm double row
0
24
24
Connector_PinHeader_1.27mm
PinHeader_2x13_P1.27mm_Horizontal
Through hole angled pin header, 2x13, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x13 1.27mm double row
0
26
26
Connector_PinHeader_1.27mm
PinHeader_2x13_P1.27mm_Vertical
Through hole straight pin header, 2x13, 1.27mm pitch, double rows
Through hole pin header THT 2x13 1.27mm double row
0
26
26
Connector_PinHeader_1.27mm
PinHeader_2x13_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x13, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x13 1.27mm double row
0
26
26
Connector_PinHeader_1.27mm
PinHeader_2x14_P1.27mm_Horizontal
Through hole angled pin header, 2x14, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x14 1.27mm double row
0
28
28
Connector_PinHeader_1.27mm
PinHeader_2x14_P1.27mm_Vertical
Through hole straight pin header, 2x14, 1.27mm pitch, double rows
Through hole pin header THT 2x14 1.27mm double row
0
28
28
Connector_PinHeader_1.27mm
PinHeader_2x14_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x14, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x14 1.27mm double row
0
28
28
Connector_PinHeader_1.27mm
PinHeader_2x15_P1.27mm_Horizontal
Through hole angled pin header, 2x15, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x15 1.27mm double row
0
30
30
Connector_PinHeader_1.27mm
PinHeader_2x15_P1.27mm_Vertical
Through hole straight pin header, 2x15, 1.27mm pitch, double rows
Through hole pin header THT 2x15 1.27mm double row
0
30
30
Connector_PinHeader_1.27mm
PinHeader_2x15_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x15, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x15 1.27mm double row
0
30
30
Connector_PinHeader_1.27mm
PinHeader_2x16_P1.27mm_Horizontal
Through hole angled pin header, 2x16, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x16 1.27mm double row
0
32
32
Connector_PinHeader_1.27mm
PinHeader_2x16_P1.27mm_Vertical
Through hole straight pin header, 2x16, 1.27mm pitch, double rows
Through hole pin header THT 2x16 1.27mm double row
0
32
32
Connector_PinHeader_1.27mm
PinHeader_2x16_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x16, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x16 1.27mm double row
0
32
32
Connector_PinHeader_1.27mm
PinHeader_2x17_P1.27mm_Horizontal
Through hole angled pin header, 2x17, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x17 1.27mm double row
0
34
34
Connector_PinHeader_1.27mm
PinHeader_2x17_P1.27mm_Vertical
Through hole straight pin header, 2x17, 1.27mm pitch, double rows
Through hole pin header THT 2x17 1.27mm double row
0
34
34
Connector_PinHeader_1.27mm
PinHeader_2x17_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x17, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x17 1.27mm double row
0
34
34
Connector_PinHeader_1.27mm
PinHeader_2x18_P1.27mm_Horizontal
Through hole angled pin header, 2x18, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x18 1.27mm double row
0
36
36
Connector_PinHeader_1.27mm
PinHeader_2x18_P1.27mm_Vertical
Through hole straight pin header, 2x18, 1.27mm pitch, double rows
Through hole pin header THT 2x18 1.27mm double row
0
36
36
Connector_PinHeader_1.27mm
PinHeader_2x18_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x18, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x18 1.27mm double row
0
36
36
Connector_PinHeader_1.27mm
PinHeader_2x19_P1.27mm_Horizontal
Through hole angled pin header, 2x19, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x19 1.27mm double row
0
38
38
Connector_PinHeader_1.27mm
PinHeader_2x19_P1.27mm_Vertical
Through hole straight pin header, 2x19, 1.27mm pitch, double rows
Through hole pin header THT 2x19 1.27mm double row
0
38
38
Connector_PinHeader_1.27mm
PinHeader_2x19_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x19, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x19 1.27mm double row
0
38
38
Connector_PinHeader_1.27mm
PinHeader_2x20_P1.27mm_Horizontal
Through hole angled pin header, 2x20, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x20 1.27mm double row
0
40
40
Connector_PinHeader_1.27mm
PinHeader_2x20_P1.27mm_Vertical
Through hole straight pin header, 2x20, 1.27mm pitch, double rows
Through hole pin header THT 2x20 1.27mm double row
0
40
40
Connector_PinHeader_1.27mm
PinHeader_2x20_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x20, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x20 1.27mm double row
0
40
40
Connector_PinHeader_1.27mm
PinHeader_2x21_P1.27mm_Horizontal
Through hole angled pin header, 2x21, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x21 1.27mm double row
0
42
42
Connector_PinHeader_1.27mm
PinHeader_2x21_P1.27mm_Vertical
Through hole straight pin header, 2x21, 1.27mm pitch, double rows
Through hole pin header THT 2x21 1.27mm double row
0
42
42
Connector_PinHeader_1.27mm
PinHeader_2x21_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x21, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x21 1.27mm double row
0
42
42
Connector_PinHeader_1.27mm
PinHeader_2x22_P1.27mm_Horizontal
Through hole angled pin header, 2x22, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x22 1.27mm double row
0
44
44
Connector_PinHeader_1.27mm
PinHeader_2x22_P1.27mm_Vertical
Through hole straight pin header, 2x22, 1.27mm pitch, double rows
Through hole pin header THT 2x22 1.27mm double row
0
44
44
Connector_PinHeader_1.27mm
PinHeader_2x22_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x22, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x22 1.27mm double row
0
44
44
Connector_PinHeader_1.27mm
PinHeader_2x23_P1.27mm_Horizontal
Through hole angled pin header, 2x23, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x23 1.27mm double row
0
46
46
Connector_PinHeader_1.27mm
PinHeader_2x23_P1.27mm_Vertical
Through hole straight pin header, 2x23, 1.27mm pitch, double rows
Through hole pin header THT 2x23 1.27mm double row
0
46
46
Connector_PinHeader_1.27mm
PinHeader_2x23_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x23, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x23 1.27mm double row
0
46
46
Connector_PinHeader_1.27mm
PinHeader_2x24_P1.27mm_Horizontal
Through hole angled pin header, 2x24, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x24 1.27mm double row
0
48
48
Connector_PinHeader_1.27mm
PinHeader_2x24_P1.27mm_Vertical
Through hole straight pin header, 2x24, 1.27mm pitch, double rows
Through hole pin header THT 2x24 1.27mm double row
0
48
48
Connector_PinHeader_1.27mm
PinHeader_2x24_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x24, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x24 1.27mm double row
0
48
48
Connector_PinHeader_1.27mm
PinHeader_2x25_P1.27mm_Horizontal
Through hole angled pin header, 2x25, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x25 1.27mm double row
0
50
50
Connector_PinHeader_1.27mm
PinHeader_2x25_P1.27mm_Vertical
Through hole straight pin header, 2x25, 1.27mm pitch, double rows
Through hole pin header THT 2x25 1.27mm double row
0
50
50
Connector_PinHeader_1.27mm
PinHeader_2x25_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x25, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x25 1.27mm double row
0
50
50
Connector_PinHeader_1.27mm
PinHeader_2x26_P1.27mm_Horizontal
Through hole angled pin header, 2x26, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x26 1.27mm double row
0
52
52
Connector_PinHeader_1.27mm
PinHeader_2x26_P1.27mm_Vertical
Through hole straight pin header, 2x26, 1.27mm pitch, double rows
Through hole pin header THT 2x26 1.27mm double row
0
52
52
Connector_PinHeader_1.27mm
PinHeader_2x26_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x26, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x26 1.27mm double row
0
52
52
Connector_PinHeader_1.27mm
PinHeader_2x27_P1.27mm_Horizontal
Through hole angled pin header, 2x27, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x27 1.27mm double row
0
54
54
Connector_PinHeader_1.27mm
PinHeader_2x27_P1.27mm_Vertical
Through hole straight pin header, 2x27, 1.27mm pitch, double rows
Through hole pin header THT 2x27 1.27mm double row
0
54
54
Connector_PinHeader_1.27mm
PinHeader_2x27_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x27, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x27 1.27mm double row
0
54
54
Connector_PinHeader_1.27mm
PinHeader_2x28_P1.27mm_Horizontal
Through hole angled pin header, 2x28, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x28 1.27mm double row
0
56
56
Connector_PinHeader_1.27mm
PinHeader_2x28_P1.27mm_Vertical
Through hole straight pin header, 2x28, 1.27mm pitch, double rows
Through hole pin header THT 2x28 1.27mm double row
0
56
56
Connector_PinHeader_1.27mm
PinHeader_2x28_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x28, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x28 1.27mm double row
0
56
56
Connector_PinHeader_1.27mm
PinHeader_2x29_P1.27mm_Horizontal
Through hole angled pin header, 2x29, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x29 1.27mm double row
0
58
58
Connector_PinHeader_1.27mm
PinHeader_2x29_P1.27mm_Vertical
Through hole straight pin header, 2x29, 1.27mm pitch, double rows
Through hole pin header THT 2x29 1.27mm double row
0
58
58
Connector_PinHeader_1.27mm
PinHeader_2x29_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x29, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x29 1.27mm double row
0
58
58
Connector_PinHeader_1.27mm
PinHeader_2x30_P1.27mm_Horizontal
Through hole angled pin header, 2x30, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x30 1.27mm double row
0
60
60
Connector_PinHeader_1.27mm
PinHeader_2x30_P1.27mm_Vertical
Through hole straight pin header, 2x30, 1.27mm pitch, double rows
Through hole pin header THT 2x30 1.27mm double row
0
60
60
Connector_PinHeader_1.27mm
PinHeader_2x30_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x30, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x30 1.27mm double row
0
60
60
Connector_PinHeader_1.27mm
PinHeader_2x31_P1.27mm_Horizontal
Through hole angled pin header, 2x31, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x31 1.27mm double row
0
62
62
Connector_PinHeader_1.27mm
PinHeader_2x31_P1.27mm_Vertical
Through hole straight pin header, 2x31, 1.27mm pitch, double rows
Through hole pin header THT 2x31 1.27mm double row
0
62
62
Connector_PinHeader_1.27mm
PinHeader_2x31_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x31, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x31 1.27mm double row
0
62
62
Connector_PinHeader_1.27mm
PinHeader_2x32_P1.27mm_Horizontal
Through hole angled pin header, 2x32, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x32 1.27mm double row
0
64
64
Connector_PinHeader_1.27mm
PinHeader_2x32_P1.27mm_Vertical
Through hole straight pin header, 2x32, 1.27mm pitch, double rows
Through hole pin header THT 2x32 1.27mm double row
0
64
64
Connector_PinHeader_1.27mm
PinHeader_2x32_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x32, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x32 1.27mm double row
0
64
64
Connector_PinHeader_1.27mm
PinHeader_2x33_P1.27mm_Horizontal
Through hole angled pin header, 2x33, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x33 1.27mm double row
0
66
66
Connector_PinHeader_1.27mm
PinHeader_2x33_P1.27mm_Vertical
Through hole straight pin header, 2x33, 1.27mm pitch, double rows
Through hole pin header THT 2x33 1.27mm double row
0
66
66
Connector_PinHeader_1.27mm
PinHeader_2x33_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x33, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x33 1.27mm double row
0
66
66
Connector_PinHeader_1.27mm
PinHeader_2x34_P1.27mm_Horizontal
Through hole angled pin header, 2x34, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x34 1.27mm double row
0
68
68
Connector_PinHeader_1.27mm
PinHeader_2x34_P1.27mm_Vertical
Through hole straight pin header, 2x34, 1.27mm pitch, double rows
Through hole pin header THT 2x34 1.27mm double row
0
68
68
Connector_PinHeader_1.27mm
PinHeader_2x34_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x34, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x34 1.27mm double row
0
68
68
Connector_PinHeader_1.27mm
PinHeader_2x35_P1.27mm_Horizontal
Through hole angled pin header, 2x35, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x35 1.27mm double row
0
70
70
Connector_PinHeader_1.27mm
PinHeader_2x35_P1.27mm_Vertical
Through hole straight pin header, 2x35, 1.27mm pitch, double rows
Through hole pin header THT 2x35 1.27mm double row
0
70
70
Connector_PinHeader_1.27mm
PinHeader_2x35_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x35, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x35 1.27mm double row
0
70
70
Connector_PinHeader_1.27mm
PinHeader_2x36_P1.27mm_Horizontal
Through hole angled pin header, 2x36, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x36 1.27mm double row
0
72
72
Connector_PinHeader_1.27mm
PinHeader_2x36_P1.27mm_Vertical
Through hole straight pin header, 2x36, 1.27mm pitch, double rows
Through hole pin header THT 2x36 1.27mm double row
0
72
72
Connector_PinHeader_1.27mm
PinHeader_2x36_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x36, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x36 1.27mm double row
0
72
72
Connector_PinHeader_1.27mm
PinHeader_2x37_P1.27mm_Horizontal
Through hole angled pin header, 2x37, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x37 1.27mm double row
0
74
74
Connector_PinHeader_1.27mm
PinHeader_2x37_P1.27mm_Vertical
Through hole straight pin header, 2x37, 1.27mm pitch, double rows
Through hole pin header THT 2x37 1.27mm double row
0
74
74
Connector_PinHeader_1.27mm
PinHeader_2x37_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x37, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x37 1.27mm double row
0
74
74
Connector_PinHeader_1.27mm
PinHeader_2x38_P1.27mm_Horizontal
Through hole angled pin header, 2x38, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x38 1.27mm double row
0
76
76
Connector_PinHeader_1.27mm
PinHeader_2x38_P1.27mm_Vertical
Through hole straight pin header, 2x38, 1.27mm pitch, double rows
Through hole pin header THT 2x38 1.27mm double row
0
76
76
Connector_PinHeader_1.27mm
PinHeader_2x38_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x38, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x38 1.27mm double row
0
76
76
Connector_PinHeader_1.27mm
PinHeader_2x39_P1.27mm_Horizontal
Through hole angled pin header, 2x39, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x39 1.27mm double row
0
78
78
Connector_PinHeader_1.27mm
PinHeader_2x39_P1.27mm_Vertical
Through hole straight pin header, 2x39, 1.27mm pitch, double rows
Through hole pin header THT 2x39 1.27mm double row
0
78
78
Connector_PinHeader_1.27mm
PinHeader_2x39_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x39, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x39 1.27mm double row
0
78
78
Connector_PinHeader_1.27mm
PinHeader_2x40_P1.27mm_Horizontal
Through hole angled pin header, 2x40, 1.27mm pitch, 4.0mm pin length, double rows
Through hole angled pin header THT 2x40 1.27mm double row
0
80
80
Connector_PinHeader_1.27mm
PinHeader_2x40_P1.27mm_Vertical
Through hole straight pin header, 2x40, 1.27mm pitch, double rows
Through hole pin header THT 2x40 1.27mm double row
0
80
80
Connector_PinHeader_1.27mm
PinHeader_2x40_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x40, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x40 1.27mm double row
0
80
80
