#MicroXplorer Configuration settings - do not modify
ADC1.AWD1FilteringConfig=ADC_AWD_FILTERING_2SAMPLES
ADC1.AWD1HighThreshold=4090
ADC1.AWD1ITMode=DISABLE
ADC1.AWD1LowThreshold=5
ADC1.Channel-2\#ChannelRegularConversion=ADC_CHANNEL_VOPAMP1
ADC1.ContinuousConvMode=ENABLE
ADC1.DMAContinuousRequests=ENABLE
ADC1.EnableAnalogWatchDog1=true
ADC1.IPParameters=Rank-2\#ChannelRegularConversion,Channel-2\#ChannelRegularConversion,SamplingTime-2\#ChannelRegularConversion,OffsetNumber-2\#ChannelRegularConversion,NbrOfConversionFlag,OversamplingMode,ContinuousConvMode,DMAContinuousRequests,master,EnableAnalogWatchDog1,WatchdogChannel,AWD1HighThreshold,AWD1ITMode,AWD1LowThreshold,AWD1FilteringConfig
ADC1.NbrOfConversionFlag=1
ADC1.OffsetNumber-2\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.OversamplingMode=ENABLE
ADC1.Rank-2\#ChannelRegularConversion=1
ADC1.SamplingTime-2\#ChannelRegularConversion=ADC_SAMPLETIME_47CYCLES_5
ADC1.WatchdogChannel=ADC_CHANNEL_VOPAMP1
ADC1.master=1
ARM.CMSIS.5.7.0.CMSISJjCORE=true
ARM.CMSIS.5.7.0.CMSISJjCORE_Checked=true
ARM.CMSIS.5.7.0.CMSISJjDSP=Source
ARM.CMSIS.5.7.0.CMSISJjDSP_Checked=true
ARM.CMSIS.5.7.0.IPParameters=CMSISJjCORE,CMSISJjDSP
ARM.CMSIS.5.7.0_SwParameter=CMSISJjDSP\:Source;CMSISJjCORE\:true;
DAC1.DAC_Channel-DAC_OUT2=DAC_CHANNEL_2
DAC1.DAC_DMADoubleDataMode-DAC_OUT1=DISABLE
DAC1.DAC_OutputBuffer-DAC_OUT1=DAC_OUTPUTBUFFER_ENABLE
DAC1.DAC_SampleAndHold-DAC_OUT1=DAC_SAMPLEANDHOLD_DISABLE
DAC1.DAC_SignedFormat-DAC_OUT1=ENABLE
DAC1.DAC_Trigger_OUT1-DAC_OUT1=DAC_TRIGGER_T6_TRGO
DAC1.IPParameters=DAC_OutputBuffer-DAC_OUT1,DAC_SampleAndHold-DAC_OUT1,DAC_Trigger_OUT1-DAC_OUT1,DAC_SignedFormat-DAC_OUT1,DAC_DMADoubleDataMode-DAC_OUT1,DAC_Channel-DAC_OUT2
Dma.ADC1.3.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC1.3.EventEnable=DISABLE
Dma.ADC1.3.Instance=DMA1_Channel1
Dma.ADC1.3.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.ADC1.3.MemInc=DMA_MINC_ENABLE
Dma.ADC1.3.Mode=DMA_CIRCULAR
Dma.ADC1.3.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.ADC1.3.PeriphInc=DMA_PINC_DISABLE
Dma.ADC1.3.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.ADC1.3.Priority=DMA_PRIORITY_LOW
Dma.ADC1.3.RequestNumber=1
Dma.ADC1.3.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.ADC1.3.SignalID=NONE
Dma.ADC1.3.SyncEnable=DISABLE
Dma.ADC1.3.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.ADC1.3.SyncRequestNumber=1
Dma.ADC1.3.SyncSignalID=NONE
Dma.DAC1_CH1.0.Direction=DMA_MEMORY_TO_PERIPH
Dma.DAC1_CH1.0.EventEnable=DISABLE
Dma.DAC1_CH1.0.Instance=DMA1_Channel2
Dma.DAC1_CH1.0.MemDataAlignment=DMA_MDATAALIGN_WORD
Dma.DAC1_CH1.0.MemInc=DMA_MINC_ENABLE
Dma.DAC1_CH1.0.Mode=DMA_CIRCULAR
Dma.DAC1_CH1.0.PeriphDataAlignment=DMA_PDATAALIGN_WORD
Dma.DAC1_CH1.0.PeriphInc=DMA_PINC_DISABLE
Dma.DAC1_CH1.0.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.DAC1_CH1.0.Priority=DMA_PRIORITY_LOW
Dma.DAC1_CH1.0.RequestNumber=1
Dma.DAC1_CH1.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.DAC1_CH1.0.SignalID=NONE
Dma.DAC1_CH1.0.SyncEnable=DISABLE
Dma.DAC1_CH1.0.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.DAC1_CH1.0.SyncRequestNumber=1
Dma.DAC1_CH1.0.SyncSignalID=NONE
Dma.DAC1_CH2.1.Direction=DMA_MEMORY_TO_PERIPH
Dma.DAC1_CH2.1.EventEnable=DISABLE
Dma.DAC1_CH2.1.Instance=DMA1_Channel4
Dma.DAC1_CH2.1.MemDataAlignment=DMA_MDATAALIGN_WORD
Dma.DAC1_CH2.1.MemInc=DMA_MINC_ENABLE
Dma.DAC1_CH2.1.Mode=DMA_CIRCULAR
Dma.DAC1_CH2.1.PeriphDataAlignment=DMA_PDATAALIGN_WORD
Dma.DAC1_CH2.1.PeriphInc=DMA_PINC_DISABLE
Dma.DAC1_CH2.1.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.DAC1_CH2.1.Priority=DMA_PRIORITY_LOW
Dma.DAC1_CH2.1.RequestNumber=1
Dma.DAC1_CH2.1.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.DAC1_CH2.1.SignalID=NONE
Dma.DAC1_CH2.1.SyncEnable=DISABLE
Dma.DAC1_CH2.1.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.DAC1_CH2.1.SyncRequestNumber=1
Dma.DAC1_CH2.1.SyncSignalID=NONE
Dma.Request0=DAC1_CH1
Dma.Request1=DAC1_CH2
Dma.Request2=USART1_TX
Dma.Request3=ADC1
Dma.RequestsNb=4
Dma.USART1_TX.2.Direction=DMA_MEMORY_TO_PERIPH
Dma.USART1_TX.2.EventEnable=DISABLE
Dma.USART1_TX.2.Instance=DMA1_Channel5
Dma.USART1_TX.2.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART1_TX.2.MemInc=DMA_MINC_ENABLE
Dma.USART1_TX.2.Mode=DMA_NORMAL
Dma.USART1_TX.2.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART1_TX.2.PeriphInc=DMA_PINC_DISABLE
Dma.USART1_TX.2.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.USART1_TX.2.Priority=DMA_PRIORITY_LOW
Dma.USART1_TX.2.RequestNumber=1
Dma.USART1_TX.2.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.USART1_TX.2.SignalID=NONE
Dma.USART1_TX.2.SyncEnable=DISABLE
Dma.USART1_TX.2.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.USART1_TX.2.SyncRequestNumber=1
Dma.USART1_TX.2.SyncSignalID=NONE
File.Version=6
GPIO.groupedBy=Group By Peripherals
KeepUserPlacement=false
Mcu.Family=STM32G4
Mcu.IP0=ADC1
Mcu.IP1=CORDIC
Mcu.IP10=TIM8
Mcu.IP11=USART1
Mcu.IP2=DAC1
Mcu.IP3=DMA
Mcu.IP4=NVIC
Mcu.IP5=OPAMP1
Mcu.IP6=RCC
Mcu.IP7=SYS
Mcu.IP8=TIM6
Mcu.IP9=TIM7
Mcu.IPNb=12
Mcu.Name=STM32G431K(6-8-B)Tx
Mcu.Package=LQFP32
Mcu.Pin0=PF0-OSC_IN
Mcu.Pin1=PF1-OSC_OUT
Mcu.Pin10=PB3
Mcu.Pin11=PB5
Mcu.Pin12=VP_ADC1_OPAMP_INTERNAL1
Mcu.Pin13=VP_CORDIC_VS_CORDIC
Mcu.Pin14=VP_SYS_VS_Systick
Mcu.Pin15=VP_SYS_VS_DBSignals
Mcu.Pin16=VP_TIM6_VS_ClockSourceINT
Mcu.Pin17=VP_TIM7_VS_ClockSourceINT
Mcu.Pin18=VP_TIM8_VS_ClockSourceINT
Mcu.Pin19=VP_ARM.CMSIS_VS_CMSISJjCORE_5.4.0_5.7.0
Mcu.Pin2=PA1
Mcu.Pin20=VP_ARM.CMSIS_VS_CMSISJjDSP_1.8.0_5.7.0
Mcu.Pin3=PA3
Mcu.Pin4=PA4
Mcu.Pin5=PA5
Mcu.Pin6=PA9
Mcu.Pin7=PA10
Mcu.Pin8=PA13
Mcu.Pin9=PA14
Mcu.PinsNb=21
Mcu.ThirdParty0=ARM.CMSIS.5.7.0
Mcu.ThirdPartyNb=1
Mcu.UserConstants=
Mcu.UserName=STM32G431KBTx
MxCube.Version=6.2.1
MxDb.Version=DB.6.0.21
NVIC.ADC1_2_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.DMA1_Channel1_IRQn=true\:0\:0\:false\:false\:true\:false\:true
NVIC.DMA1_Channel2_IRQn=true\:0\:0\:false\:false\:true\:false\:true
NVIC.DMA1_Channel4_IRQn=true\:0\:0\:false\:false\:true\:false\:true
NVIC.DMA1_Channel5_IRQn=true\:0\:0\:false\:false\:true\:false\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.SysTick_IRQn=true\:0\:0\:false\:false\:true\:false\:true
NVIC.TIM7_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.USART1_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
OPAMP1.IPParameters=PowerMode,PgaGain
OPAMP1.PgaGain=OPAMP_PGA_GAIN_64_OR_MINUS_63
OPAMP1.PowerMode=OPAMP_POWERMODE_HIGHSPEED
PA1.Mode=PGA Internally connected_IO0_BIAS
PA1.Signal=OPAMP1_VINP
PA10.GPIOParameters=GPIO_FM7
PA10.GPIO_FM7=__NULL
PA10.Locked=true
PA10.Mode=Asynchronous
PA10.Signal=USART1_RX
PA13.GPIOParameters=GPIO_Label
PA13.GPIO_Label=T_SWDIO
PA13.Locked=true
PA13.Mode=Serial_Wire
PA13.Signal=SYS_JTMS-SWDIO
PA14.GPIOParameters=GPIO_Label
PA14.GPIO_Label=T_SWCLK
PA14.Locked=true
PA14.Mode=Serial_Wire
PA14.Signal=SYS_JTCK-SWCLK
PA3.Mode=PGA Internally connected_IO0_BIAS
PA3.Signal=OPAMP1_VINM0
PA4.Signal=COMP_DAC11_group
PA5.Signal=COMP_DAC12_group
PA9.GPIOParameters=GPIO_FM6
PA9.GPIO_FM6=__NULL
PA9.Locked=true
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB3.GPIOParameters=GPIO_Label
PB3.GPIO_Label=T_SWO
PB3.Locked=true
PB3.Signal=SYS_JTDO-SWO
PB5.GPIOParameters=GPIO_Label
PB5.GPIO_Label=OUT
PB5.Locked=true
PB5.Signal=GPIO_Output
PF0-OSC_IN.Mode=HSE-External-Oscillator
PF0-OSC_IN.Signal=RCC_OSC_IN
PF1-OSC_OUT.Mode=HSE-External-Oscillator
PF1-OSC_OUT.Signal=RCC_OSC_OUT
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32G431KBTx
ProjectManager.FirmwarePackage=STM32Cube FW_G4 V1.4.0
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=0
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=bassofono.ioc
ProjectManager.ProjectName=bassofono
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=Makefile
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=false
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-HAL-true,2-MX_DMA_Init-DMA-false-HAL-true,3-SystemClock_Config-RCC-false-HAL-false,4-MX_DAC1_Init-DAC1-false-HAL-true,5-MX_ADC1_Init-ADC1-false-HAL-true,6-MX_TIM7_Init-TIM7-false-HAL-true,7-MX_TIM6_Init-TIM6-false-HAL-true,8-MX_CORDIC_Init-CORDIC-false-HAL-true,9-MX_USART1_UART_Init-USART1-false-HAL-true,10-MX_TIM8_Init-TIM8-false-HAL-true,11-MX_OPAMP1_Init-OPAMP1-false-HAL-true
RCC.ADC12Freq_Value=168000000
RCC.AHBFreq_Value=168000000
RCC.APB1Freq_Value=168000000
RCC.APB1TimFreq_Value=168000000
RCC.APB2Freq_Value=168000000
RCC.APB2TimFreq_Value=168000000
RCC.CRSFreq_Value=48000000
RCC.CortexFreq_Value=168000000
RCC.EXTERNAL_CLOCK_VALUE=12288000
RCC.FCLKCortexFreq_Value=168000000
RCC.FDCANFreq_Value=168000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=168000000
RCC.HSE_VALUE=24000000
RCC.HSI48_VALUE=48000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=168000000
RCC.I2C2Freq_Value=168000000
RCC.I2C3Freq_Value=168000000
RCC.I2SFreq_Value=168000000
RCC.IPParameters=ADC12Freq_Value,AHBFreq_Value,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,CRSFreq_Value,CortexFreq_Value,EXTERNAL_CLOCK_VALUE,FCLKCortexFreq_Value,FDCANFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI48_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2SFreq_Value,LPTIM1Freq_Value,LPUART1Freq_Value,LSCOPinFreq_Value,LSE_VALUE,LSI_VALUE,MCO1PinFreq_Value,PLLM,PLLN,PLLPoutputFreq_Value,PLLQoutputFreq_Value,PLLRCLKFreq_Value,PLLSourceVirtual,PWRFreq_Value,RNGFreq_Value,SAI1Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USBFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value
RCC.LPTIM1Freq_Value=168000000
RCC.LPUART1Freq_Value=168000000
RCC.LSCOPinFreq_Value=32000
RCC.LSE_VALUE=32768
RCC.LSI_VALUE=32000
RCC.MCO1PinFreq_Value=16000000
RCC.PLLM=RCC_PLLM_DIV2
RCC.PLLN=28
RCC.PLLPoutputFreq_Value=168000000
RCC.PLLQoutputFreq_Value=168000000
RCC.PLLRCLKFreq_Value=168000000
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.PWRFreq_Value=168000000
RCC.RNGFreq_Value=168000000
RCC.SAI1Freq_Value=168000000
RCC.SYSCLKFreq_VALUE=168000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=168000000
RCC.USART1Freq_Value=168000000
RCC.USART2Freq_Value=168000000
RCC.USART3Freq_Value=168000000
RCC.USBFreq_Value=168000000
RCC.VCOInputFreq_Value=12000000
RCC.VCOOutputFreq_Value=336000000
SH.COMP_DAC11_group.0=DAC1_OUT1,DAC_OUT1
SH.COMP_DAC11_group.ConfNb=1
SH.COMP_DAC12_group.0=DAC1_OUT2,DAC_OUT2
SH.COMP_DAC12_group.ConfNb=1
TIM6.IPParameters=PeriodNoDither,TIM_MasterOutputTrigger
TIM6.PeriodNoDither=7679
TIM6.TIM_MasterOutputTrigger=TIM_TRGO_UPDATE
TIM7.IPParameters=Prescaler,PeriodNoDither
TIM7.PeriodNoDither=999
TIM7.Prescaler=1679
TIM8.IPParameters=PeriodNoDither,TIM_MasterOutputTrigger,TIM_MasterOutputTrigger2
TIM8.PeriodNoDither=239
TIM8.TIM_MasterOutputTrigger=TIM_TRGO_UPDATE
TIM8.TIM_MasterOutputTrigger2=TIM_TRGO2_RESET
USART1.IPParameters=VirtualMode-Asynchronous
USART1.VirtualMode-Asynchronous=VM_ASYNC
VP_ADC1_OPAMP_INTERNAL1.Mode=IN-OPAMP1
VP_ADC1_OPAMP_INTERNAL1.Signal=ADC1_OPAMP_INTERNAL1
VP_ARM.CMSIS_VS_CMSISJjCORE_5.4.0_5.7.0.Mode=CMSISJjCORE
VP_ARM.CMSIS_VS_CMSISJjCORE_5.4.0_5.7.0.Signal=ARM.CMSIS_VS_CMSISJjCORE_5.4.0_5.7.0
VP_ARM.CMSIS_VS_CMSISJjDSP_1.8.0_5.7.0.Mode=CMSISJjDSP
VP_ARM.CMSIS_VS_CMSISJjDSP_1.8.0_5.7.0.Signal=ARM.CMSIS_VS_CMSISJjDSP_1.8.0_5.7.0
VP_CORDIC_VS_CORDIC.Mode=CORDIC_Activate
VP_CORDIC_VS_CORDIC.Signal=CORDIC_VS_CORDIC
VP_SYS_VS_DBSignals.Mode=DisableDeadBatterySignals
VP_SYS_VS_DBSignals.Signal=SYS_VS_DBSignals
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
VP_TIM6_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM6_VS_ClockSourceINT.Signal=TIM6_VS_ClockSourceINT
VP_TIM7_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM7_VS_ClockSourceINT.Signal=TIM7_VS_ClockSourceINT
VP_TIM8_VS_ClockSourceINT.Mode=Internal
VP_TIM8_VS_ClockSourceINT.Signal=TIM8_VS_ClockSourceINT
board=NUCLEO-G431KB
boardIOC=true
