ARM GAS  /tmp/ccJPteqL.s 			page 1


   1              		.cpu cortex-m4
   2              		.arch armv7e-m
   3              		.fpu fpv4-sp-d16
   4              		.eabi_attribute 27, 1
   5              		.eabi_attribute 28, 1
   6              		.eabi_attribute 20, 1
   7              		.eabi_attribute 21, 1
   8              		.eabi_attribute 23, 3
   9              		.eabi_attribute 24, 1
  10              		.eabi_attribute 25, 1
  11              		.eabi_attribute 26, 1
  12              		.eabi_attribute 30, 1
  13              		.eabi_attribute 34, 1
  14              		.eabi_attribute 18, 4
  15              		.file	"stm32g4xx_hal_pcd.c"
  16              		.text
  17              	.Ltext0:
  18              		.cfi_sections	.debug_frame
  19              		.file 1 "Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c"
  20              		.section	.text.HAL_PCD_EP_DB_Receive,"ax",%progbits
  21              		.align	1
  22              		.syntax unified
  23              		.thumb
  24              		.thumb_func
  26              	HAL_PCD_EP_DB_Receive:
  27              	.LVL0:
  28              	.LFB362:
   1:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
   2:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ******************************************************************************
   3:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @file    stm32g4xx_hal_pcd.c
   4:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @author  MCD Application Team
   5:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief   PCD HAL module driver.
   6:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          This file provides firmware functions to manage the following
   7:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          functionalities of the USB Peripheral Controller:
   8:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *           + Initialization and de-initialization functions
   9:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *           + IO operation functions
  10:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *           + Peripheral Control functions
  11:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *           + Peripheral State functions
  12:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *
  13:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ******************************************************************************
  14:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @attention
  15:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *
  16:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * Copyright (c) 2019 STMicroelectronics.
  17:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * All rights reserved.
  18:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *
  19:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * This software is licensed under terms that can be found in the LICENSE file
  20:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * in the root directory of this software component.
  21:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  22:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *
  23:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ******************************************************************************
  24:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   @verbatim
  25:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ==============================================================================
  26:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                     ##### How to use this driver #####
  27:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ==============================================================================
  28:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     [..]
  29:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       The PCD HAL driver can be used as follows:
  30:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 2


  31:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****      (#) Declare a PCD_HandleTypeDef handle structure, for example:
  32:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****          PCD_HandleTypeDef  hpcd;
  33:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  34:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****      (#) Fill parameters of Init structure in HCD handle
  35:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  36:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****      (#) Call HAL_PCD_Init() API to initialize the PCD peripheral (Core, Device core, ...)
  37:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  38:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****      (#) Initialize the PCD low level resources through the HAL_PCD_MspInit() API:
  39:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****          (##) Enable the PCD/USB Low Level interface clock using
  40:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               (+++) __HAL_RCC_USB_CLK_ENABLE(); For USB Device only FS peripheral
  41:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  42:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****          (##) Initialize the related GPIO clocks
  43:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****          (##) Configure PCD pin-out
  44:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****          (##) Configure PCD NVIC interrupt
  45:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  46:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****      (#)Associate the Upper USB device stack to the HAL PCD Driver:
  47:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****          (##) hpcd.pData = pdev;
  48:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  49:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****      (#)Enable PCD transmission and reception:
  50:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****          (##) HAL_PCD_Start();
  51:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  52:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   @endverbatim
  53:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ******************************************************************************
  54:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
  55:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  56:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /* Includes ------------------------------------------------------------------*/
  57:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #include "stm32g4xx_hal.h"
  58:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  59:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /** @addtogroup STM32G4xx_HAL_Driver
  60:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @{
  61:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
  62:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  63:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /** @defgroup PCD PCD
  64:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief PCD HAL module driver
  65:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @{
  66:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
  67:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  68:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #ifdef HAL_PCD_MODULE_ENABLED
  69:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  70:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if defined (USB)
  71:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  72:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /* Private types -------------------------------------------------------------*/
  73:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /* Private variables ---------------------------------------------------------*/
  74:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /* Private constants ---------------------------------------------------------*/
  75:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /* Private macros ------------------------------------------------------------*/
  76:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /** @defgroup PCD_Private_Macros PCD Private Macros
  77:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @{
  78:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
  79:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #define PCD_MIN(a, b)  (((a) < (b)) ? (a) : (b))
  80:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #define PCD_MAX(a, b)  (((a) > (b)) ? (a) : (b))
  81:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
  82:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @}
  83:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
  84:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  85:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /* Private functions prototypes ----------------------------------------------*/
  86:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /** @defgroup PCD_Private_Functions PCD Private Functions
  87:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @{
ARM GAS  /tmp/ccJPteqL.s 			page 3


  88:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
  89:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  90:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** static HAL_StatusTypeDef PCD_EP_ISR_Handler(PCD_HandleTypeDef *hpcd);
  91:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_USB_DOUBLE_BUFFER == 1U)
  92:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** static HAL_StatusTypeDef HAL_PCD_EP_DB_Transmit(PCD_HandleTypeDef *hpcd, PCD_EPTypeDef *ep, uint16_
  93:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** static uint16_t HAL_PCD_EP_DB_Receive(PCD_HandleTypeDef *hpcd, PCD_EPTypeDef *ep, uint16_t wEPVal);
  94:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* (USE_USB_DOUBLE_BUFFER == 1U) */
  95:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
  96:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
  97:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @}
  98:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
  99:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 100:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /* Exported functions --------------------------------------------------------*/
 101:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /** @defgroup PCD_Exported_Functions PCD Exported Functions
 102:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @{
 103:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 104:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 105:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /** @defgroup PCD_Exported_Functions_Group1 Initialization and de-initialization functions
 106:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *  @brief    Initialization and Configuration functions
 107:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *
 108:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** @verbatim
 109:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****  ===============================================================================
 110:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             ##### Initialization and de-initialization functions #####
 111:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****  ===============================================================================
 112:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     [..]  This section provides functions allowing to:
 113:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 114:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** @endverbatim
 115:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @{
 116:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 117:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 118:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 119:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Initializes the PCD according to the specified
 120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         parameters in the PCD_InitTypeDef and initialize the associated handle.
 121:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 122:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 123:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 124:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_Init(PCD_HandleTypeDef *hpcd)
 125:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 126:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint8_t i;
 127:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 128:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Check the PCD handle allocation */
 129:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd == NULL)
 130:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 131:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
 132:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 133:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 134:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Check the parameters */
 135:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   assert_param(IS_PCD_ALL_INSTANCE(hpcd->Instance));
 136:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 137:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_RESET)
 138:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 139:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Allocate lock resource and initialize it */
 140:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->Lock = HAL_UNLOCKED;
 141:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 142:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
 143:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->SOFCallback = HAL_PCD_SOFCallback;
 144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->SetupStageCallback = HAL_PCD_SetupStageCallback;
ARM GAS  /tmp/ccJPteqL.s 			page 4


 145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ResetCallback = HAL_PCD_ResetCallback;
 146:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->SuspendCallback = HAL_PCD_SuspendCallback;
 147:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ResumeCallback = HAL_PCD_ResumeCallback;
 148:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ConnectCallback = HAL_PCD_ConnectCallback;
 149:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->DisconnectCallback = HAL_PCD_DisconnectCallback;
 150:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->DataOutStageCallback = HAL_PCD_DataOutStageCallback;
 151:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->DataInStageCallback = HAL_PCD_DataInStageCallback;
 152:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ISOOUTIncompleteCallback = HAL_PCD_ISOOUTIncompleteCallback;
 153:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ISOINIncompleteCallback = HAL_PCD_ISOINIncompleteCallback;
 154:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->LPMCallback = HAL_PCDEx_LPM_Callback;
 155:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->BCDCallback = HAL_PCDEx_BCD_Callback;
 156:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (hpcd->MspInitCallback == NULL)
 158:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 159:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->MspInitCallback = HAL_PCD_MspInit;
 160:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 161:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 162:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Init the low level hardware */
 163:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->MspInitCallback(hpcd);
 164:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
 165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Init the low level hardware : GPIO, CLOCK, NVIC... */
 166:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     HAL_PCD_MspInit(hpcd);
 167:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* (USE_HAL_PCD_REGISTER_CALLBACKS) */
 168:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 169:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 170:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->State = HAL_PCD_STATE_BUSY;
 171:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 172:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Disable the Interrupts */
 173:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_DISABLE(hpcd);
 174:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 175:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Init endpoints structures */
 176:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   for (i = 0U; i < hpcd->Init.dev_endpoints; i++)
 177:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 178:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Init ep structure */
 179:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].is_in = 1U;
 180:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].num = i;
 181:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].tx_fifo_num = i;
 182:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Control until ep is activated */
 183:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].type = EP_TYPE_CTRL;
 184:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].maxpacket = 0U;
 185:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].xfer_buff = 0U;
 186:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].xfer_len = 0U;
 187:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 188:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   for (i = 0U; i < hpcd->Init.dev_endpoints; i++)
 190:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 191:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].is_in = 0U;
 192:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].num = i;
 193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Control until ep is activated */
 194:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].type = EP_TYPE_CTRL;
 195:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].maxpacket = 0U;
 196:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].xfer_buff = 0U;
 197:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].xfer_len = 0U;
 198:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 199:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 200:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Init Device */
 201:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevInit(hpcd->Instance, hpcd->Init);
ARM GAS  /tmp/ccJPteqL.s 			page 5


 202:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 203:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->USB_Address = 0U;
 204:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->State = HAL_PCD_STATE_READY;
 205:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 206:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Activate LPM */
 207:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->Init.lpm_enable == 1U)
 208:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 209:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     (void)HAL_PCDEx_ActivateLPM(hpcd);
 210:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 211:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 212:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
 213:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 214:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 215:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 216:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  DeInitializes the PCD peripheral.
 217:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 218:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 219:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 220:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_DeInit(PCD_HandleTypeDef *hpcd)
 221:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 222:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Check the PCD handle allocation */
 223:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd == NULL)
 224:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 225:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
 226:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 227:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 228:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->State = HAL_PCD_STATE_BUSY;
 229:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 230:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Stop Device */
 231:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (USB_StopDevice(hpcd->Instance) != HAL_OK)
 232:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 233:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
 234:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 235:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 236:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
 237:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->MspDeInitCallback == NULL)
 238:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 239:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->MspDeInitCallback = HAL_PCD_MspDeInit; /* Legacy weak MspDeInit  */
 240:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 241:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 242:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* DeInit the low level hardware */
 243:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->MspDeInitCallback(hpcd);
 244:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
 245:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* DeInit the low level hardware: CLOCK, NVIC.*/
 246:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_PCD_MspDeInit(hpcd);
 247:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 248:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 249:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->State = HAL_PCD_STATE_RESET;
 250:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 251:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
 252:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 253:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 254:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 255:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Initializes the PCD MSP.
 256:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 257:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
 258:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
ARM GAS  /tmp/ccJPteqL.s 			page 6


 259:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_MspInit(PCD_HandleTypeDef *hpcd)
 260:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 261:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 262:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
 263:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 264:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
 265:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_MspInit could be implemented in the user file
 266:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
 267:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 268:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 269:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 270:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  DeInitializes PCD MSP.
 271:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 272:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
 273:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 274:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_MspDeInit(PCD_HandleTypeDef *hpcd)
 275:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 276:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 277:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
 278:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 279:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
 280:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_MspDeInit could be implemented in the user file
 281:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
 282:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 283:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 284:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
 285:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 286:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Register a User USB PCD Callback
 287:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         To be used instead of the weak predefined callback
 288:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd USB PCD handle
 289:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  CallbackID ID of the callback to be registered
 290:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         This parameter can be one of the following values:
 291:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_SOF_CB_ID USB PCD SOF callback ID
 292:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_SETUPSTAGE_CB_ID USB PCD Setup callback ID
 293:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_RESET_CB_ID USB PCD Reset callback ID
 294:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_SUSPEND_CB_ID USB PCD Suspend callback ID
 295:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_RESUME_CB_ID USB PCD Resume callback ID
 296:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_CONNECT_CB_ID USB PCD Connect callback ID
 297:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_DISCONNECT_CB_ID OTG PCD Disconnect callback ID
 298:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_MSPINIT_CB_ID MspDeInit callback ID
 299:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_MSPDEINIT_CB_ID MspDeInit callback ID
 300:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  pCallback pointer to the Callback function
 301:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 302:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 303:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_RegisterCallback(PCD_HandleTypeDef *hpcd,
 304:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                                            HAL_PCD_CallbackIDTypeDef CallbackID,
 305:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                                            pPCD_CallbackTypeDef pCallback)
 306:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 307:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 308:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 309:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (pCallback == NULL)
 310:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 311:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 312:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 313:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
 314:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 315:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
ARM GAS  /tmp/ccJPteqL.s 			page 7


 316:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 317:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 318:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 319:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 320:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     switch (CallbackID)
 321:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 322:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_SOF_CB_ID :
 323:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->SOFCallback = pCallback;
 324:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 325:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 326:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_SETUPSTAGE_CB_ID :
 327:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->SetupStageCallback = pCallback;
 328:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 329:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 330:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_RESET_CB_ID :
 331:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->ResetCallback = pCallback;
 332:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 333:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 334:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_SUSPEND_CB_ID :
 335:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->SuspendCallback = pCallback;
 336:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 337:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 338:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_RESUME_CB_ID :
 339:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->ResumeCallback = pCallback;
 340:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 341:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 342:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_CONNECT_CB_ID :
 343:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->ConnectCallback = pCallback;
 344:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 345:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 346:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_DISCONNECT_CB_ID :
 347:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->DisconnectCallback = pCallback;
 348:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 349:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 350:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_MSPINIT_CB_ID :
 351:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->MspInitCallback = pCallback;
 352:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 353:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 354:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_MSPDEINIT_CB_ID :
 355:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->MspDeInitCallback = pCallback;
 356:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 357:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 358:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       default :
 359:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Update the error code */
 360:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 361:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Return error status */
 362:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         status =  HAL_ERROR;
 363:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 364:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 365:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 366:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else if (hpcd->State == HAL_PCD_STATE_RESET)
 367:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 368:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     switch (CallbackID)
 369:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 370:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_MSPINIT_CB_ID :
 371:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->MspInitCallback = pCallback;
 372:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
ARM GAS  /tmp/ccJPteqL.s 			page 8


 373:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 374:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_MSPDEINIT_CB_ID :
 375:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->MspDeInitCallback = pCallback;
 376:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 377:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 378:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       default :
 379:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Update the error code */
 380:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 381:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Return error status */
 382:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         status =  HAL_ERROR;
 383:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 384:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 385:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 386:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 387:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 388:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 389:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 390:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 391:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 392:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 393:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 394:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 395:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 396:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 397:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 398:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 399:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 400:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Unregister an USB PCD Callback
 401:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         USB PCD callabck is redirected to the weak predefined callback
 402:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd USB PCD handle
 403:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  CallbackID ID of the callback to be unregistered
 404:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         This parameter can be one of the following values:
 405:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_SOF_CB_ID USB PCD SOF callback ID
 406:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_SETUPSTAGE_CB_ID USB PCD Setup callback ID
 407:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_RESET_CB_ID USB PCD Reset callback ID
 408:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_SUSPEND_CB_ID USB PCD Suspend callback ID
 409:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_RESUME_CB_ID USB PCD Resume callback ID
 410:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_CONNECT_CB_ID USB PCD Connect callback ID
 411:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_DISCONNECT_CB_ID OTG PCD Disconnect callback ID
 412:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_MSPINIT_CB_ID MspDeInit callback ID
 413:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *          @arg @ref HAL_PCD_MSPDEINIT_CB_ID MspDeInit callback ID
 414:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 415:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 416:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_UnRegisterCallback(PCD_HandleTypeDef *hpcd, HAL_PCD_CallbackIDTypeDef Cal
 417:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 418:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 419:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 420:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 421:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 422:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 423:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Setup Legacy weak Callbacks  */
 424:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 425:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 426:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     switch (CallbackID)
 427:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 428:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_SOF_CB_ID :
 429:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->SOFCallback = HAL_PCD_SOFCallback;
ARM GAS  /tmp/ccJPteqL.s 			page 9


 430:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 431:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 432:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_SETUPSTAGE_CB_ID :
 433:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->SetupStageCallback = HAL_PCD_SetupStageCallback;
 434:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 435:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 436:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_RESET_CB_ID :
 437:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->ResetCallback = HAL_PCD_ResetCallback;
 438:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 439:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 440:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_SUSPEND_CB_ID :
 441:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->SuspendCallback = HAL_PCD_SuspendCallback;
 442:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 443:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 444:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_RESUME_CB_ID :
 445:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->ResumeCallback = HAL_PCD_ResumeCallback;
 446:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 447:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 448:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_CONNECT_CB_ID :
 449:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->ConnectCallback = HAL_PCD_ConnectCallback;
 450:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 451:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 452:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_DISCONNECT_CB_ID :
 453:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->DisconnectCallback = HAL_PCD_DisconnectCallback;
 454:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 455:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 456:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_MSPINIT_CB_ID :
 457:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->MspInitCallback = HAL_PCD_MspInit;
 458:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 459:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 460:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_MSPDEINIT_CB_ID :
 461:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->MspDeInitCallback = HAL_PCD_MspDeInit;
 462:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 463:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 464:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       default :
 465:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Update the error code */
 466:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 467:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 468:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Return error status */
 469:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         status =  HAL_ERROR;
 470:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 471:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 472:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 473:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else if (hpcd->State == HAL_PCD_STATE_RESET)
 474:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 475:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     switch (CallbackID)
 476:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 477:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_MSPINIT_CB_ID :
 478:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->MspInitCallback = HAL_PCD_MspInit;
 479:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 480:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 481:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       case HAL_PCD_MSPDEINIT_CB_ID :
 482:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->MspDeInitCallback = HAL_PCD_MspDeInit;
 483:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 484:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 485:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       default :
 486:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Update the error code */
ARM GAS  /tmp/ccJPteqL.s 			page 10


 487:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 488:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 489:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Return error status */
 490:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         status =  HAL_ERROR;
 491:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         break;
 492:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 493:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 494:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 495:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 496:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 497:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 498:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 499:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 500:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 501:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 502:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 503:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 504:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 505:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 506:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 507:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 508:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 509:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Register USB PCD Data OUT Stage Callback
 510:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         To be used instead of the weak HAL_PCD_DataOutStageCallback() predefined callback
 511:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 512:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  pCallback pointer to the USB PCD Data OUT Stage Callback function
 513:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 514:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 515:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_RegisterDataOutStageCallback(PCD_HandleTypeDef *hpcd,
 516:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                                                        pPCD_DataOutStageCallbackTypeDef pCallback)
 517:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 518:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 519:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 520:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (pCallback == NULL)
 521:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 522:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 523:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 524:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 525:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
 526:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 527:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 528:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 529:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 530:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 531:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 532:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 533:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->DataOutStageCallback = pCallback;
 534:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 535:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 536:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 537:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 538:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 539:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 540:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 541:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 542:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 543:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 11


 544:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 545:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 546:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 547:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 548:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 549:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 550:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 551:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Unregister the USB PCD Data OUT Stage Callback
 552:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         USB PCD Data OUT Stage Callback is redirected to the weak HAL_PCD_DataOutStageCallback(
 553:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 554:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 555:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 556:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_UnRegisterDataOutStageCallback(PCD_HandleTypeDef *hpcd)
 557:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 558:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 559:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 560:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 561:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 562:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 563:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 564:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 565:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->DataOutStageCallback = HAL_PCD_DataOutStageCallback; /* Legacy weak DataOutStageCallback 
 566:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 567:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 568:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 569:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 570:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 571:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 572:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 573:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 574:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 575:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 576:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 577:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 578:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 579:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 580:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 581:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 582:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 583:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Register USB PCD Data IN Stage Callback
 584:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         To be used instead of the weak HAL_PCD_DataInStageCallback() predefined callback
 585:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 586:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  pCallback pointer to the USB PCD Data IN Stage Callback function
 587:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 588:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 589:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_RegisterDataInStageCallback(PCD_HandleTypeDef *hpcd,
 590:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                                                       pPCD_DataInStageCallbackTypeDef pCallback)
 591:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 592:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 593:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 594:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (pCallback == NULL)
 595:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 596:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 597:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 598:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 599:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
 600:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
ARM GAS  /tmp/ccJPteqL.s 			page 12


 601:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 602:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 603:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 604:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 605:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 606:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 607:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->DataInStageCallback = pCallback;
 608:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 609:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 610:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 611:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 612:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 613:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 614:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 615:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 616:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 617:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 618:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 619:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 620:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 621:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 622:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 623:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 624:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 625:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Unregister the USB PCD Data IN Stage Callback
 626:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         USB PCD Data OUT Stage Callback is redirected to the weak HAL_PCD_DataInStageCallback()
 627:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 628:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 629:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 630:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_UnRegisterDataInStageCallback(PCD_HandleTypeDef *hpcd)
 631:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 632:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 633:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 634:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 635:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 636:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 637:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 638:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 639:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->DataInStageCallback = HAL_PCD_DataInStageCallback; /* Legacy weak DataInStageCallback  */
 640:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 641:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 642:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 643:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 644:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 645:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 646:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 647:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 648:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 649:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 650:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 651:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 652:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 653:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 654:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 655:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 656:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 657:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Register USB PCD Iso OUT incomplete Callback
ARM GAS  /tmp/ccJPteqL.s 			page 13


 658:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         To be used instead of the weak HAL_PCD_ISOOUTIncompleteCallback() predefined callback
 659:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 660:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  pCallback pointer to the USB PCD Iso OUT incomplete Callback function
 661:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 662:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 663:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_RegisterIsoOutIncpltCallback(PCD_HandleTypeDef *hpcd,
 664:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                                                        pPCD_IsoOutIncpltCallbackTypeDef pCallback)
 665:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 666:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 667:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 668:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (pCallback == NULL)
 669:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 670:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 671:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 672:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 673:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
 674:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 675:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 676:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 677:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 678:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 679:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 680:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 681:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ISOOUTIncompleteCallback = pCallback;
 682:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 683:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 684:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 685:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 686:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 687:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 688:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 689:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 690:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 691:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 692:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 693:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 694:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 695:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 696:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 697:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 698:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 699:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Unregister the USB PCD Iso OUT incomplete Callback
 700:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         USB PCD Iso OUT incomplete Callback is redirected
 701:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         to the weak HAL_PCD_ISOOUTIncompleteCallback() predefined callback
 702:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 703:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 704:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 705:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_UnRegisterIsoOutIncpltCallback(PCD_HandleTypeDef *hpcd)
 706:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 707:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 708:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 709:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 710:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 711:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 712:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 713:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 714:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ISOOUTIncompleteCallback = HAL_PCD_ISOOUTIncompleteCallback; /* Legacy weak ISOOUTIncompl
ARM GAS  /tmp/ccJPteqL.s 			page 14


 715:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 716:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 717:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 718:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 719:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 720:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 721:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 722:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 723:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 724:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 725:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 726:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 727:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 728:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 729:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 730:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 731:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 732:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Register USB PCD Iso IN incomplete Callback
 733:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         To be used instead of the weak HAL_PCD_ISOINIncompleteCallback() predefined callback
 734:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 735:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  pCallback pointer to the USB PCD Iso IN incomplete Callback function
 736:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 737:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 738:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_RegisterIsoInIncpltCallback(PCD_HandleTypeDef *hpcd,
 739:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                                                       pPCD_IsoInIncpltCallbackTypeDef pCallback)
 740:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 741:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 742:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 743:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (pCallback == NULL)
 744:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 745:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 746:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 747:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 748:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
 749:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 750:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 751:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 752:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 753:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 754:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 755:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 756:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ISOINIncompleteCallback = pCallback;
 757:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 758:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 759:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 760:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 761:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 762:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 763:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 764:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 765:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 766:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 767:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 768:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 769:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 770:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 771:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
ARM GAS  /tmp/ccJPteqL.s 			page 15


 772:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 773:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 774:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Unregister the USB PCD Iso IN incomplete Callback
 775:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         USB PCD Iso IN incomplete Callback is redirected
 776:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         to the weak HAL_PCD_ISOINIncompleteCallback() predefined callback
 777:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 778:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 779:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 780:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_UnRegisterIsoInIncpltCallback(PCD_HandleTypeDef *hpcd)
 781:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 782:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 783:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 784:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 785:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 786:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 787:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 788:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 789:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ISOINIncompleteCallback = HAL_PCD_ISOINIncompleteCallback; /* Legacy weak ISOINIncomplete
 790:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 793:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 794:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 795:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 796:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 797:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 798:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 799:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 800:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 801:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 802:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 803:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 804:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 805:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 806:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 807:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Register USB PCD BCD Callback
 808:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         To be used instead of the weak HAL_PCDEx_BCD_Callback() predefined callback
 809:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 810:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  pCallback pointer to the USB PCD BCD Callback function
 811:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 812:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 813:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_RegisterBcdCallback(PCD_HandleTypeDef *hpcd, pPCD_BcdCallbackTypeDef pCal
 814:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 815:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 816:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 817:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (pCallback == NULL)
 818:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 819:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 820:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 821:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 822:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
 823:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 824:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 825:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 826:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 827:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 828:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
ARM GAS  /tmp/ccJPteqL.s 			page 16


 829:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->BCDCallback = pCallback;
 831:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 832:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 833:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 834:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 835:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 836:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 837:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 838:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 839:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 840:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 841:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 842:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 843:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 844:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 845:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 846:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 847:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 848:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Unregister the USB PCD BCD Callback
 849:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         USB BCD Callback is redirected to the weak HAL_PCDEx_BCD_Callback() predefined callback
 850:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 851:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 852:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 853:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_UnRegisterBcdCallback(PCD_HandleTypeDef *hpcd)
 854:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 855:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 856:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 857:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 858:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 859:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 860:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 861:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 862:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->BCDCallback = HAL_PCDEx_BCD_Callback; /* Legacy weak HAL_PCDEx_BCD_Callback  */
 863:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 864:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 865:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 866:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 867:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 868:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 869:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 870:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 871:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 872:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 873:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 874:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 875:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 876:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 877:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 878:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 879:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 880:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Register USB PCD LPM Callback
 881:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         To be used instead of the weak HAL_PCDEx_LPM_Callback() predefined callback
 882:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 883:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  pCallback pointer to the USB PCD LPM Callback function
 884:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 885:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
ARM GAS  /tmp/ccJPteqL.s 			page 17


 886:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_RegisterLpmCallback(PCD_HandleTypeDef *hpcd, pPCD_LpmCallbackTypeDef pCal
 887:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 888:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 889:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 890:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (pCallback == NULL)
 891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 892:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 893:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 894:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
 896:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 897:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 898:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 899:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 900:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 901:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 902:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 903:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->LPMCallback = pCallback;
 904:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 905:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 906:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 907:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 908:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 909:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 910:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
 911:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 912:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 913:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 914:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 915:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 916:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 917:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 918:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 919:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 920:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 921:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Unregister the USB PCD LPM Callback
 922:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *         USB LPM Callback is redirected to the weak HAL_PCDEx_LPM_Callback() predefined callback
 923:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 924:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 925:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 926:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_UnRegisterLpmCallback(PCD_HandleTypeDef *hpcd)
 927:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 928:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef status = HAL_OK;
 929:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 930:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Process locked */
 931:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 932:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 933:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (hpcd->State == HAL_PCD_STATE_READY)
 934:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 935:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->LPMCallback = HAL_PCDEx_LPM_Callback; /* Legacy weak HAL_PCDEx_LPM_Callback  */
 936:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 937:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
 938:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 939:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Update the error code */
 940:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ErrorCode |= HAL_PCD_ERROR_INVALID_CALLBACK;
 941:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 942:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Return error status */
ARM GAS  /tmp/ccJPteqL.s 			page 18


 943:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     status =  HAL_ERROR;
 944:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 945:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 946:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Release Lock */
 947:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 948:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 949:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return status;
 950:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 951:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 952:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 953:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 954:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @}
 955:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 956:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 957:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /** @defgroup PCD_Exported_Functions_Group2 Input and Output operation functions
 958:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *  @brief   Data transfers functions
 959:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *
 960:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** @verbatim
 961:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****  ===============================================================================
 962:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                       ##### IO operation functions #####
 963:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****  ===============================================================================
 964:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     [..]
 965:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     This subsection provides a set of functions allowing to manage the PCD data
 966:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     transfers.
 967:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 968:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** @endverbatim
 969:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @{
 970:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 971:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 972:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 973:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Start the USB device
 974:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 975:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 976:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 977:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_Start(PCD_HandleTypeDef *hpcd)
 978:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 979:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 980:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_ENABLE(hpcd);
 981:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevConnect(hpcd->Instance);
 982:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 983:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 984:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
 985:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 986:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 987:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 988:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Stop the USB device.
 989:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
 990:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
 991:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
 992:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_Stop(PCD_HandleTypeDef *hpcd)
 993:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 994:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 995:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_DISABLE(hpcd);
 996:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevDisconnect(hpcd->Instance);
 997:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 998:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 999:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
ARM GAS  /tmp/ccJPteqL.s 			page 19


1000:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1001:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1002:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1003:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1004:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  This function handles PCD interrupt request.
1005:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1006:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1007:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1008:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** void HAL_PCD_IRQHandler(PCD_HandleTypeDef *hpcd)
1009:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1010:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint32_t wIstr = USB_ReadInterrupts(hpcd->Instance);
1011:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1012:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wIstr & USB_ISTR_CTR) == USB_ISTR_CTR)
1013:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1014:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* servicing of the endpoint correct transfer interrupt */
1015:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* clear of the CTR flag into the sub */
1016:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     (void)PCD_EP_ISR_Handler(hpcd);
1017:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1018:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return;
1019:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1020:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wIstr & USB_ISTR_RESET) == USB_ISTR_RESET)
1022:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1023:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     __HAL_PCD_CLEAR_FLAG(hpcd, USB_ISTR_RESET);
1024:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1025:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1026:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ResetCallback(hpcd);
1027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1028:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     HAL_PCD_ResetCallback(hpcd);
1029:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1030:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1031:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     (void)HAL_PCD_SetAddress(hpcd, 0U);
1032:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1033:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return;
1034:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1035:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1036:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wIstr & USB_ISTR_PMAOVR) == USB_ISTR_PMAOVR)
1037:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1038:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     __HAL_PCD_CLEAR_FLAG(hpcd, USB_ISTR_PMAOVR);
1039:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1040:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return;
1041:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1042:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1043:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wIstr & USB_ISTR_ERR) == USB_ISTR_ERR)
1044:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1045:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     __HAL_PCD_CLEAR_FLAG(hpcd, USB_ISTR_ERR);
1046:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1047:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return;
1048:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1049:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1050:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wIstr & USB_ISTR_WKUP) == USB_ISTR_WKUP)
1051:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1052:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->Instance->CNTR &= (uint16_t) ~(USB_CNTR_LPMODE);
1053:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->Instance->CNTR &= (uint16_t) ~(USB_CNTR_FSUSP);
1054:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1055:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (hpcd->LPM_State == LPM_L1)
1056:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
ARM GAS  /tmp/ccJPteqL.s 			page 20


1057:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->LPM_State = LPM_L0;
1058:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1059:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->LPMCallback(hpcd, PCD_LPM_L0_ACTIVE);
1060:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1061:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       HAL_PCDEx_LPM_Callback(hpcd, PCD_LPM_L0_ACTIVE);
1062:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1063:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
1064:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1065:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1066:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->ResumeCallback(hpcd);
1067:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1068:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     HAL_PCD_ResumeCallback(hpcd);
1069:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1070:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     __HAL_PCD_CLEAR_FLAG(hpcd, USB_ISTR_WKUP);
1072:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1073:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return;
1074:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1075:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1076:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wIstr & USB_ISTR_SUSP) == USB_ISTR_SUSP)
1077:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1078:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Force low-power mode in the macrocell */
1079:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->Instance->CNTR |= (uint16_t)USB_CNTR_FSUSP;
1080:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1081:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* clear of the ISTR bit must be done after setting of CNTR_FSUSP */
1082:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     __HAL_PCD_CLEAR_FLAG(hpcd, USB_ISTR_SUSP);
1083:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1084:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->Instance->CNTR |= (uint16_t)USB_CNTR_LPMODE;
1085:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1086:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1087:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->SuspendCallback(hpcd);
1088:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1089:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     HAL_PCD_SuspendCallback(hpcd);
1090:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1091:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1092:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return;
1093:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1094:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1095:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Handle LPM Interrupt */
1096:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wIstr & USB_ISTR_L1REQ) == USB_ISTR_L1REQ)
1097:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1098:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     __HAL_PCD_CLEAR_FLAG(hpcd, USB_ISTR_L1REQ);
1099:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (hpcd->LPM_State == LPM_L0)
1100:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
1101:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* Force suspend and low-power mode before going to L1 state*/
1102:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->Instance->CNTR |= (uint16_t)USB_CNTR_LPMODE;
1103:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->Instance->CNTR |= (uint16_t)USB_CNTR_FSUSP;
1104:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1105:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->LPM_State = LPM_L1;
1106:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->BESL = ((uint32_t)hpcd->Instance->LPMCSR & USB_LPMCSR_BESL) >> 2;
1107:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1108:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->LPMCallback(hpcd, PCD_LPM_L1_ACTIVE);
1109:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1110:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       HAL_PCDEx_LPM_Callback(hpcd, PCD_LPM_L1_ACTIVE);
1111:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1112:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
1113:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     else
ARM GAS  /tmp/ccJPteqL.s 			page 21


1114:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
1115:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1116:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->SuspendCallback(hpcd);
1117:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1118:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       HAL_PCD_SuspendCallback(hpcd);
1119:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
1121:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1122:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return;
1123:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1124:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1125:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wIstr & USB_ISTR_SOF) == USB_ISTR_SOF)
1126:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1127:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     __HAL_PCD_CLEAR_FLAG(hpcd, USB_ISTR_SOF);
1128:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1129:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1130:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->SOFCallback(hpcd);
1131:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1132:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     HAL_PCD_SOFCallback(hpcd);
1133:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1134:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1135:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return;
1136:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1137:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1138:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wIstr & USB_ISTR_ESOF) == USB_ISTR_ESOF)
1139:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1140:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* clear ESOF flag in ISTR */
1141:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     __HAL_PCD_CLEAR_FLAG(hpcd, USB_ISTR_ESOF);
1142:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1143:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return;
1144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1146:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1147:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1148:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1149:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Data OUT stage callback.
1150:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1151:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  epnum endpoint number
1152:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1153:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1154:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_DataOutStageCallback(PCD_HandleTypeDef *hpcd, uint8_t epnum)
1155:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1156:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1158:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(epnum);
1159:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1160:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1161:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_DataOutStageCallback could be implemented in the user file
1162:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1163:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1164:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1166:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Data IN stage callback
1167:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1168:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  epnum endpoint number
1169:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1170:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
ARM GAS  /tmp/ccJPteqL.s 			page 22


1171:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_DataInStageCallback(PCD_HandleTypeDef *hpcd, uint8_t epnum)
1172:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1173:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1174:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1175:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(epnum);
1176:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1177:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1178:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_DataInStageCallback could be implemented in the user file
1179:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1180:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1181:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1182:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Setup stage callback
1183:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1184:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1185:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1186:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_SetupStageCallback(PCD_HandleTypeDef *hpcd)
1187:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1188:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1190:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1191:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1192:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_SetupStageCallback could be implemented in the user file
1193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1194:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1195:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1196:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1197:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  USB Start Of Frame callback.
1198:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1199:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1200:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1201:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_SOFCallback(PCD_HandleTypeDef *hpcd)
1202:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1203:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1204:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1205:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1206:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1207:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_SOFCallback could be implemented in the user file
1208:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1209:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1210:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1211:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1212:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  USB Reset callback.
1213:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1214:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1215:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1216:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_ResetCallback(PCD_HandleTypeDef *hpcd)
1217:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1218:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1219:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1220:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1221:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1222:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_ResetCallback could be implemented in the user file
1223:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1224:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1225:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1226:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1227:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Suspend event callback.
ARM GAS  /tmp/ccJPteqL.s 			page 23


1228:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1229:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1230:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1231:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_SuspendCallback(PCD_HandleTypeDef *hpcd)
1232:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1233:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1234:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1235:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1236:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1237:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_SuspendCallback could be implemented in the user file
1238:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1239:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1240:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1241:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1242:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Resume event callback.
1243:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1244:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1245:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1246:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_ResumeCallback(PCD_HandleTypeDef *hpcd)
1247:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1248:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1249:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1250:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1251:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1252:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_ResumeCallback could be implemented in the user file
1253:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1254:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1255:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1256:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1257:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Incomplete ISO OUT callback.
1258:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1259:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  epnum endpoint number
1260:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1261:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1262:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_ISOOUTIncompleteCallback(PCD_HandleTypeDef *hpcd, uint8_t epnum)
1263:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1264:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1265:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1266:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(epnum);
1267:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1268:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1269:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_ISOOUTIncompleteCallback could be implemented in the user file
1270:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1271:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1272:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1273:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1274:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Incomplete ISO IN callback.
1275:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1276:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  epnum endpoint number
1277:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1278:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1279:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_ISOINIncompleteCallback(PCD_HandleTypeDef *hpcd, uint8_t epnum)
1280:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1281:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1282:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1283:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(epnum);
1284:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 24


1285:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1286:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_ISOINIncompleteCallback could be implemented in the user file
1287:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1288:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1289:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1290:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1291:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Connection event callback.
1292:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1293:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1294:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1295:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_ConnectCallback(PCD_HandleTypeDef *hpcd)
1296:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1297:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1298:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1299:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1300:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1301:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_ConnectCallback could be implemented in the user file
1302:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1303:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1304:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1305:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1306:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Disconnection event callback.
1307:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1308:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval None
1309:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1310:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** __weak void HAL_PCD_DisconnectCallback(PCD_HandleTypeDef *hpcd)
1311:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1312:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1313:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1314:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1315:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* NOTE : This function should not be modified, when the callback is needed,
1316:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             the HAL_PCD_DisconnectCallback could be implemented in the user file
1317:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****    */
1318:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1319:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1320:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1321:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @}
1322:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1323:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1324:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /** @defgroup PCD_Exported_Functions_Group3 Peripheral Control functions
1325:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *  @brief   management functions
1326:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *
1327:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** @verbatim
1328:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****  ===============================================================================
1329:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                       ##### Peripheral Control functions #####
1330:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****  ===============================================================================
1331:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     [..]
1332:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     This subsection provides a set of functions allowing to control the PCD data
1333:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     transfers.
1334:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1335:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** @endverbatim
1336:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @{
1337:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1338:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1339:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1340:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Connect the USB device
1341:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
ARM GAS  /tmp/ccJPteqL.s 			page 25


1342:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1343:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1344:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_DevConnect(PCD_HandleTypeDef *hpcd)
1345:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1346:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
1347:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevConnect(hpcd->Instance);
1348:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
1349:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1350:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
1351:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1352:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1353:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1354:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Disconnect the USB device.
1355:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1356:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1357:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1358:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_DevDisconnect(PCD_HandleTypeDef *hpcd)
1359:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1360:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
1361:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevDisconnect(hpcd->Instance);
1362:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
1363:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1364:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
1365:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1366:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1367:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1368:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Set the USB Device address.
1369:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1370:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  address new device address
1371:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1372:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1373:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_SetAddress(PCD_HandleTypeDef *hpcd, uint8_t address)
1374:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1375:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
1376:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->USB_Address = address;
1377:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_SetDevAddress(hpcd->Instance, address);
1378:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
1379:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1380:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
1381:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1382:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1383:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Open and configure an endpoint.
1384:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1385:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep_addr endpoint address
1386:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep_mps endpoint max packet size
1387:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep_type endpoint type
1388:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1389:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1390:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_EP_Open(PCD_HandleTypeDef *hpcd, uint8_t ep_addr,
1391:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                                   uint16_t ep_mps, uint8_t ep_type)
1392:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1393:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef  ret = HAL_OK;
1394:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
1395:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1396:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((ep_addr & 0x80U) == 0x80U)
1397:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1398:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep = &hpcd->IN_ep[ep_addr & EP_ADDR_MSK];
ARM GAS  /tmp/ccJPteqL.s 			page 26


1399:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
1400:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1401:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
1402:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1403:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep = &hpcd->OUT_ep[ep_addr & EP_ADDR_MSK];
1404:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
1405:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1406:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1407:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
1408:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->maxpacket = ep_mps;
1409:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->type = ep_type;
1410:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1411:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (ep->is_in != 0U)
1412:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1413:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Assign a Tx FIFO */
1414:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->tx_fifo_num = ep->num;
1415:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1416:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Set initial data PID. */
1417:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (ep_type == EP_TYPE_BULK)
1418:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1419:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->data_pid_start = 0U;
1420:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1421:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1422:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
1423:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_ActivateEndpoint(hpcd->Instance, ep);
1424:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
1425:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1426:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return ret;
1427:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1428:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1429:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1430:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Deactivate an endpoint.
1431:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1432:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep_addr endpoint address
1433:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1434:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1435:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_EP_Close(PCD_HandleTypeDef *hpcd, uint8_t ep_addr)
1436:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1437:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
1438:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1439:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((ep_addr & 0x80U) == 0x80U)
1440:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1441:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep = &hpcd->IN_ep[ep_addr & EP_ADDR_MSK];
1442:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
1443:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1444:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
1445:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1446:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep = &hpcd->OUT_ep[ep_addr & EP_ADDR_MSK];
1447:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
1448:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1449:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num   = ep_addr & EP_ADDR_MSK;
1450:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1451:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
1452:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DeactivateEndpoint(hpcd->Instance, ep);
1453:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
1454:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
1455:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
ARM GAS  /tmp/ccJPteqL.s 			page 27


1456:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1457:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1458:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1459:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Receive an amount of data.
1460:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1461:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep_addr endpoint address
1462:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  pBuf pointer to the reception buffer
1463:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  len amount of data to be received
1464:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1465:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1466:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_EP_Receive(PCD_HandleTypeDef *hpcd, uint8_t ep_addr, uint8_t *pBuf, uint3
1467:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1468:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
1469:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1470:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep = &hpcd->OUT_ep[ep_addr & EP_ADDR_MSK];
1471:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1472:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /*setup and start the Xfer */
1473:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_buff = pBuf;
1474:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_len = len;
1475:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_count = 0U;
1476:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->is_in = 0U;
1477:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
1478:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1479:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((ep_addr & EP_ADDR_MSK) == 0U)
1480:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1481:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     (void)USB_EP0StartXfer(hpcd->Instance, ep);
1482:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1483:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
1484:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1485:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     (void)USB_EPStartXfer(hpcd->Instance, ep);
1486:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1487:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1488:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
1489:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1490:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1491:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1492:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Get Received Data Size
1493:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1494:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep_addr endpoint address
1495:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval Data Size
1496:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1497:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** uint32_t HAL_PCD_EP_GetRxCount(PCD_HandleTypeDef *hpcd, uint8_t ep_addr)
1498:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1499:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return hpcd->OUT_ep[ep_addr & EP_ADDR_MSK].xfer_count;
1500:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1501:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1502:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Send an amount of data
1503:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1504:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep_addr endpoint address
1505:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  pBuf pointer to the transmission buffer
1506:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  len amount of data to be sent
1507:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1508:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1509:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_EP_Transmit(PCD_HandleTypeDef *hpcd, uint8_t ep_addr, uint8_t *pBuf, uint
1510:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1511:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
1512:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 28


1513:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep = &hpcd->IN_ep[ep_addr & EP_ADDR_MSK];
1514:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1515:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /*setup and start the Xfer */
1516:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_buff = pBuf;
1517:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_len = len;
1518:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_fill_db = 1U;
1519:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_len_db = len;
1520:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_count = 0U;
1521:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->is_in = 1U;
1522:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
1523:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1524:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((ep_addr & EP_ADDR_MSK) == 0U)
1525:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1526:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     (void)USB_EP0StartXfer(hpcd->Instance, ep);
1527:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1528:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
1529:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1530:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     (void)USB_EPStartXfer(hpcd->Instance, ep);
1531:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1532:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1533:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
1534:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1535:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1536:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1537:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Set a STALL condition over an endpoint
1538:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1539:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep_addr endpoint address
1540:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1541:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1542:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_EP_SetStall(PCD_HandleTypeDef *hpcd, uint8_t ep_addr)
1543:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1544:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
1545:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1546:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (((uint32_t)ep_addr & EP_ADDR_MSK) > hpcd->Init.dev_endpoints)
1547:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1548:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
1549:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1550:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1551:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((0x80U & ep_addr) == 0x80U)
1552:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1553:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep = &hpcd->IN_ep[ep_addr & EP_ADDR_MSK];
1554:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
1555:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1556:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
1557:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1558:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep = &hpcd->OUT_ep[ep_addr];
1559:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
1560:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1561:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1562:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->is_stall = 1U;
1563:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
1564:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1565:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
1566:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1567:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_EPSetStall(hpcd->Instance, ep);
1568:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1569:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
ARM GAS  /tmp/ccJPteqL.s 			page 29


1570:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1571:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
1572:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1573:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1574:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1575:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Clear a STALL condition over in an endpoint
1576:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1577:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep_addr endpoint address
1578:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1579:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1580:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_EP_ClrStall(PCD_HandleTypeDef *hpcd, uint8_t ep_addr)
1581:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1582:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
1583:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1584:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if (((uint32_t)ep_addr & 0x0FU) > hpcd->Init.dev_endpoints)
1585:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1586:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     return HAL_ERROR;
1587:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1588:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1589:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((0x80U & ep_addr) == 0x80U)
1590:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1591:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep = &hpcd->IN_ep[ep_addr & EP_ADDR_MSK];
1592:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
1593:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1594:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
1595:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1596:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep = &hpcd->OUT_ep[ep_addr & EP_ADDR_MSK];
1597:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
1598:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1599:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1600:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->is_stall = 0U;
1601:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
1602:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1603:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
1604:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_EPClearStall(hpcd->Instance, ep);
1605:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
1606:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1607:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
1608:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1609:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1610:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1611:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Flush an endpoint
1612:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1613:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep_addr endpoint address
1614:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1615:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1616:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_EP_Flush(PCD_HandleTypeDef *hpcd, uint8_t ep_addr)
1617:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1618:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
1619:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(hpcd);
1620:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(ep_addr);
1621:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1622:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
1623:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1624:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1625:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1626:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Activate remote wakeup signalling
ARM GAS  /tmp/ccJPteqL.s 			page 30


1627:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1628:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1629:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1630:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_ActivateRemoteWakeup(PCD_HandleTypeDef *hpcd)
1631:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1632:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return (USB_ActivateRemoteWakeup(hpcd->Instance));
1633:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1634:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1635:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1636:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  De-activate remote wakeup signalling.
1637:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1638:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1639:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1640:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** HAL_StatusTypeDef HAL_PCD_DeActivateRemoteWakeup(PCD_HandleTypeDef *hpcd)
1641:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1642:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return (USB_DeActivateRemoteWakeup(hpcd->Instance));
1643:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1644:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1645:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1646:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @}
1647:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1648:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1649:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /** @defgroup PCD_Exported_Functions_Group4 Peripheral State functions
1650:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *  @brief   Peripheral State functions
1651:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   *
1652:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** @verbatim
1653:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****  ===============================================================================
1654:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                       ##### Peripheral State functions #####
1655:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****  ===============================================================================
1656:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     [..]
1657:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     This subsection permits to get in run-time the status of the peripheral
1658:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     and the data flow.
1659:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1660:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** @endverbatim
1661:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @{
1662:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1663:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1664:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1665:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Return the PCD handle state.
1666:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1667:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL state
1668:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1669:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** PCD_StateTypeDef HAL_PCD_GetState(PCD_HandleTypeDef *hpcd)
1670:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1671:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return hpcd->State;
1672:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1673:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1674:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1675:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @}
1676:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1677:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1678:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1679:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @}
1680:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1681:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1682:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /* Private functions ---------------------------------------------------------*/
1683:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /** @addtogroup PCD_Private_Functions
ARM GAS  /tmp/ccJPteqL.s 			page 31


1684:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @{
1685:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1686:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1687:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1688:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1689:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  This function handles PCD Endpoint interrupt request.
1690:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1691:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1692:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1693:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** static HAL_StatusTypeDef PCD_EP_ISR_Handler(PCD_HandleTypeDef *hpcd)
1694:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
1695:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
1696:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint16_t count;
1697:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint16_t wIstr;
1698:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint16_t wEPVal;
1699:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint16_t TxPctSize;
1700:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint8_t epindex;
1701:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1702:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* stay in loop while pending interrupts */
1703:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   while ((hpcd->Instance->ISTR & USB_ISTR_CTR) != 0U)
1704:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1705:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     wIstr = hpcd->Instance->ISTR;
1706:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1707:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* extract highest priority endpoint number */
1708:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     epindex = (uint8_t)(wIstr & USB_ISTR_EP_ID);
1709:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1710:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (epindex == 0U)
1711:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
1712:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* Decode and service control endpoint interrupt */
1713:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1714:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* DIR bit = origin of the interrupt */
1715:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       if ((wIstr & USB_ISTR_DIR) == 0U)
1716:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
1717:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* DIR = 0 */
1718:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1719:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* DIR = 0 => IN  int */
1720:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* DIR = 0 implies that (EP_CTR_TX = 1) always */
1721:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         PCD_CLEAR_TX_EP_CTR(hpcd->Instance, PCD_ENDP0);
1722:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->IN_ep[0];
1723:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1724:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_count = PCD_GET_EP_TX_CNT(hpcd->Instance, ep->num);
1725:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_buff += ep->xfer_count;
1726:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1727:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* TX COMPLETE */
1728:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1729:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         hpcd->DataInStageCallback(hpcd, 0U);
1730:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1731:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         HAL_PCD_DataInStageCallback(hpcd, 0U);
1732:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1733:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1734:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         if ((hpcd->USB_Address > 0U) && (ep->xfer_len == 0U))
1735:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
1736:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           hpcd->Instance->DADDR = ((uint16_t)hpcd->USB_Address | USB_DADDR_EF);
1737:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           hpcd->USB_Address = 0U;
1738:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
1739:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
1740:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       else
ARM GAS  /tmp/ccJPteqL.s 			page 32


1741:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
1742:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* DIR = 1 */
1743:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1744:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* DIR = 1 & CTR_RX => SETUP or OUT int */
1745:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* DIR = 1 & (CTR_TX | CTR_RX) => 2 int pending */
1746:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->OUT_ep[0];
1747:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         wEPVal = PCD_GET_ENDPOINT(hpcd->Instance, PCD_ENDP0);
1748:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1749:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         if ((wEPVal & USB_EP_SETUP) != 0U)
1750:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
1751:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           /* Get SETUP Packet */
1752:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_count = PCD_GET_EP_RX_CNT(hpcd->Instance, ep->num);
1753:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1754:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           USB_ReadPMA(hpcd->Instance, (uint8_t *)hpcd->Setup,
1755:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                       ep->pmaadress, (uint16_t)ep->xfer_count);
1756:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1757:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           /* SETUP bit kept frozen while CTR_RX = 1 */
1758:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           PCD_CLEAR_RX_EP_CTR(hpcd->Instance, PCD_ENDP0);
1759:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1760:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           /* Process SETUP Packet*/
1761:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1762:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           hpcd->SetupStageCallback(hpcd);
1763:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1764:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           HAL_PCD_SetupStageCallback(hpcd);
1765:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1766:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
1767:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         else if ((wEPVal & USB_EP_CTR_RX) != 0U)
1768:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
1769:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           PCD_CLEAR_RX_EP_CTR(hpcd->Instance, PCD_ENDP0);
1770:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1771:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           /* Get Control Data OUT Packet */
1772:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_count = PCD_GET_EP_RX_CNT(hpcd->Instance, ep->num);
1773:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1774:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           if ((ep->xfer_count != 0U) && (ep->xfer_buff != 0U))
1775:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
1776:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             USB_ReadPMA(hpcd->Instance, ep->xfer_buff,
1777:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                         ep->pmaadress, (uint16_t)ep->xfer_count);
1778:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1779:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             ep->xfer_buff += ep->xfer_count;
1780:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1781:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             /* Process Control Data OUT Packet */
1782:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1783:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             hpcd->DataOutStageCallback(hpcd, 0U);
1784:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1785:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             HAL_PCD_DataOutStageCallback(hpcd, 0U);
1786:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1787:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
1788:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1789:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           if ((PCD_GET_ENDPOINT(hpcd->Instance, PCD_ENDP0) & USB_EP_SETUP) == 0U)
1790:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_CNT(hpcd->Instance, PCD_ENDP0, ep->maxpacket);
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
1793:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
1794:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
1795:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
1796:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
1797:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     else
ARM GAS  /tmp/ccJPteqL.s 			page 33


1798:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
1799:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* Decode and service non control endpoints interrupt */
1800:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* process related endpoint register */
1801:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       wEPVal = PCD_GET_ENDPOINT(hpcd->Instance, epindex);
1802:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1803:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       if ((wEPVal & USB_EP_CTR_RX) != 0U)
1804:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
1805:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* clear int flag */
1806:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         PCD_CLEAR_RX_EP_CTR(hpcd->Instance, epindex);
1807:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->OUT_ep[epindex];
1808:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1809:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* OUT Single Buffering */
1810:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         if (ep->doublebuffer == 0U)
1811:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
1812:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           count = (uint16_t)PCD_GET_EP_RX_CNT(hpcd->Instance, ep->num);
1813:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1814:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           if (count != 0U)
1815:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
1816:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             USB_ReadPMA(hpcd->Instance, ep->xfer_buff, ep->pmaadress, count);
1817:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
1818:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
1819:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_USB_DOUBLE_BUFFER == 1U)
1820:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         else
1821:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
1822:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           /* manage double buffer bulk out */
1823:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           if (ep->type == EP_TYPE_BULK)
1824:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
1825:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             count = HAL_PCD_EP_DB_Receive(hpcd, ep, wEPVal);
1826:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
1827:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           else /* manage double buffer iso out */
1828:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
1829:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             /* free EP OUT Buffer */
1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_FREE_USER_BUFFER(hpcd->Instance, ep->num, 0U);
1831:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1832:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             if ((PCD_GET_ENDPOINT(hpcd->Instance, ep->num) & USB_EP_DTOG_RX) != 0U)
1833:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
1834:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               /* read from endpoint BUF0Addr buffer */
1835:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               count = (uint16_t)PCD_GET_EP_DBUF0_CNT(hpcd->Instance, ep->num);
1836:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1837:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               if (count != 0U)
1838:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               {
1839:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                 USB_ReadPMA(hpcd->Instance, ep->xfer_buff, ep->pmaaddr0, count);
1840:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               }
1841:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
1842:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             else
1843:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
1844:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               /* read from endpoint BUF1Addr buffer */
1845:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               count = (uint16_t)PCD_GET_EP_DBUF1_CNT(hpcd->Instance, ep->num);
1846:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1847:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               if (count != 0U)
1848:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               {
1849:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                 USB_ReadPMA(hpcd->Instance, ep->xfer_buff, ep->pmaaddr1, count);
1850:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               }
1851:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
1852:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
1853:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
1854:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* (USE_USB_DOUBLE_BUFFER == 1U) */
ARM GAS  /tmp/ccJPteqL.s 			page 34


1855:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1856:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* multi-packet on the NON control OUT endpoint */
1857:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_count += count;
1858:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_buff += count;
1859:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1860:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         if ((ep->xfer_len == 0U) || (count < ep->maxpacket))
1861:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
1862:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           /* RX COMPLETE */
1863:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1864:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           hpcd->DataOutStageCallback(hpcd, ep->num);
1865:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1866:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           HAL_PCD_DataOutStageCallback(hpcd, ep->num);
1867:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1868:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
1869:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         else
1870:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
1871:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           (void) USB_EPStartXfer(hpcd->Instance, ep);
1872:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
1873:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
1874:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1875:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       if ((wEPVal & USB_EP_CTR_TX) != 0U)
1876:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
1877:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->IN_ep[epindex];
1878:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1879:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* clear int flag */
1880:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         PCD_CLEAR_TX_EP_CTR(hpcd->Instance, epindex);
1881:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1882:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         if (ep->type != EP_TYPE_BULK)
1883:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
1884:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len = 0U;
1885:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1886:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_USB_DOUBLE_BUFFER == 1U)
1887:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           if (ep->doublebuffer != 0U)
1888:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
1889:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             if ((wEPVal & USB_EP_DTOG_TX) != 0U)
1890:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               PCD_SET_EP_DBUF0_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
1892:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
1893:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             else
1894:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
1896:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
1897:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
1898:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* (USE_USB_DOUBLE_BUFFER == 1U) */
1899:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1900:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           /* TX COMPLETE */
1901:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1902:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           hpcd->DataInStageCallback(hpcd, ep->num);
1903:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1904:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           HAL_PCD_DataInStageCallback(hpcd, ep->num);
1905:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1906:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
1907:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         else
1908:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
1909:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           /* Manage Bulk Single Buffer Transaction */
1910:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           if ((wEPVal & USB_EP_KIND) == 0U)
1911:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
ARM GAS  /tmp/ccJPteqL.s 			page 35


1912:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             /* multi-packet on the NON control IN endpoint */
1913:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             TxPctSize = (uint16_t)PCD_GET_EP_TX_CNT(hpcd->Instance, ep->num);
1914:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1915:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             if (ep->xfer_len > TxPctSize)
1916:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
1917:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               ep->xfer_len -= TxPctSize;
1918:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
1919:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             else
1920:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
1921:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               ep->xfer_len = 0U;
1922:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
1923:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1924:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             /* Zero Length Packet? */
1925:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             if (ep->xfer_len == 0U)
1926:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
1927:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               /* TX COMPLETE */
1928:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
1929:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               hpcd->DataInStageCallback(hpcd, ep->num);
1930:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
1931:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               HAL_PCD_DataInStageCallback(hpcd, ep->num);
1932:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
1933:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
1934:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             else
1935:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
1936:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               /* Transfer is not yet Done */
1937:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               ep->xfer_buff += TxPctSize;
1938:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               ep->xfer_count += TxPctSize;
1939:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               (void)USB_EPStartXfer(hpcd->Instance, ep);
1940:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
1941:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
1942:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_USB_DOUBLE_BUFFER == 1U)
1943:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           /* Double Buffer bulk IN (bulk transfer Len > Ep_Mps) */
1944:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           else
1945:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
1946:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             (void)HAL_PCD_EP_DB_Transmit(hpcd, ep, wEPVal);
1947:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
1948:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* (USE_USB_DOUBLE_BUFFER == 1U) */
1949:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
1950:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
1951:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
1952:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
1953:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1954:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
1955:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
1956:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1957:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1958:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_USB_DOUBLE_BUFFER == 1U)
1959:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
1960:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Manage double buffer bulk out transaction from ISR
1961:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
1962:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep current endpoint handle
1963:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  wEPVal Last snapshot of EPRx register value taken in ISR
1964:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
1965:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
1966:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** static uint16_t HAL_PCD_EP_DB_Receive(PCD_HandleTypeDef *hpcd,
1967:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                                       PCD_EPTypeDef *ep, uint16_t wEPVal)
1968:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
ARM GAS  /tmp/ccJPteqL.s 			page 36


  29              		.loc 1 1968 1 view -0
  30              		.cfi_startproc
  31              		@ args = 0, pretend = 0, frame = 0
  32              		@ frame_needed = 0, uses_anonymous_args = 0
  33              		.loc 1 1968 1 is_stmt 0 view .LVU1
  34 0000 38B5     		push	{r3, r4, r5, lr}
  35              	.LCFI0:
  36              		.cfi_def_cfa_offset 16
  37              		.cfi_offset 3, -16
  38              		.cfi_offset 4, -12
  39              		.cfi_offset 5, -8
  40              		.cfi_offset 14, -4
1969:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint16_t count;
  41              		.loc 1 1969 3 is_stmt 1 view .LVU2
1970:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1971:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Manage Buffer0 OUT */
1972:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wEPVal & USB_EP_DTOG_RX) != 0U)
  42              		.loc 1 1972 3 view .LVU3
  43              		.loc 1 1972 6 is_stmt 0 view .LVU4
  44 0002 12F4804F 		tst	r2, #16384
  45 0006 43D0     		beq	.L2
1973:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
1974:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Get count of received Data on buffer0 */
1975:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     count = (uint16_t)PCD_GET_EP_DBUF0_CNT(hpcd->Instance, ep->num);
  46              		.loc 1 1975 5 is_stmt 1 view .LVU5
  47              		.loc 1 1975 23 is_stmt 0 view .LVU6
  48 0008 0468     		ldr	r4, [r0]
  49 000a B4F85030 		ldrh	r3, [r4, #80]
  50 000e 91F800C0 		ldrb	ip, [r1]	@ zero_extendqisi2
  51 0012 4FEACC0E 		lsl	lr, ip, #3
  52 0016 1EFA83F3 		uxtah	r3, lr, r3
  53 001a 2344     		add	r3, r3, r4
  54 001c B3F80244 		ldrh	r4, [r3, #1026]
  55              		.loc 1 1975 11 view .LVU7
  56 0020 C4F30904 		ubfx	r4, r4, #0, #10
  57              	.LVL1:
1976:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1977:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (ep->xfer_len >= count)
  58              		.loc 1 1977 5 is_stmt 1 view .LVU8
  59              		.loc 1 1977 11 is_stmt 0 view .LVU9
  60 0024 8B69     		ldr	r3, [r1, #24]
  61              		.loc 1 1977 8 view .LVU10
  62 0026 A342     		cmp	r3, r4
  63 0028 28D3     		bcc	.L3
1978:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
1979:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       ep->xfer_len -= count;
  64              		.loc 1 1979 7 is_stmt 1 view .LVU11
  65              		.loc 1 1979 20 is_stmt 0 view .LVU12
  66 002a 1B1B     		subs	r3, r3, r4
  67 002c 8B61     		str	r3, [r1, #24]
  68              	.L4:
1980:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
1981:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     else
1982:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
1983:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       ep->xfer_len = 0U;
1984:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
1985:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 37


1986:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (ep->xfer_len == 0U)
  69              		.loc 1 1986 5 is_stmt 1 view .LVU13
  70              		.loc 1 1986 11 is_stmt 0 view .LVU14
  71 002e 8B69     		ldr	r3, [r1, #24]
  72              		.loc 1 1986 8 view .LVU15
  73 0030 7BB9     		cbnz	r3, .L5
1987:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
1988:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* set NAK to OUT endpoint since double buffer is enabled */
1989:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_RX_STATUS(hpcd->Instance, ep->num, USB_EP_RX_NAK);
  74              		.loc 1 1989 7 is_stmt 1 view .LVU16
  75              	.LBB2:
  76              		.loc 1 1989 7 view .LVU17
  77              		.loc 1 1989 7 view .LVU18
  78 0032 0568     		ldr	r5, [r0]
  79 0034 35F82C30 		ldrh	r3, [r5, ip, lsl #2]
  80 0038 9BB2     		uxth	r3, r3
  81 003a 23F48043 		bic	r3, r3, #16384
  82 003e 23F07003 		bic	r3, r3, #112
  83              	.LVL2:
  84              		.loc 1 1989 7 view .LVU19
  85              		.loc 1 1989 7 view .LVU20
  86              		.loc 1 1989 7 view .LVU21
  87 0042 83F40053 		eor	r3, r3, #8192
  88              	.LVL3:
  89              		.loc 1 1989 7 view .LVU22
  90 0046 43F40043 		orr	r3, r3, #32768
  91              	.LVL4:
  92              		.loc 1 1989 7 is_stmt 0 view .LVU23
  93 004a 43F08003 		orr	r3, r3, #128
  94 004e 25F82C30 		strh	r3, [r5, ip, lsl #2]	@ movhi
  95              	.LVL5:
  96              	.L5:
  97              		.loc 1 1989 7 view .LVU24
  98              	.LBE2:
  99              		.loc 1 1989 7 is_stmt 1 discriminator 7 view .LVU25
1990:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
1991:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1992:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Check if Buffer1 is in blocked state which requires to toggle */
1993:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if ((wEPVal & USB_EP_DTOG_TX) != 0U)
 100              		.loc 1 1993 5 discriminator 7 view .LVU26
 101              		.loc 1 1993 8 is_stmt 0 discriminator 7 view .LVU27
 102 0052 12F0400F 		tst	r2, #64
 103 0056 0ED0     		beq	.L6
1994:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
1995:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_FREE_USER_BUFFER(hpcd->Instance, ep->num, 0U);
 104              		.loc 1 1995 7 is_stmt 1 discriminator 1 view .LVU28
 105              		.loc 1 1995 7 discriminator 1 view .LVU29
 106              		.loc 1 1995 7 discriminator 1 view .LVU30
 107              	.LBB3:
 108              		.loc 1 1995 7 discriminator 1 view .LVU31
 109              		.loc 1 1995 7 discriminator 1 view .LVU32
 110 0058 0268     		ldr	r2, [r0]
 111              	.LVL6:
 112              		.loc 1 1995 7 is_stmt 0 discriminator 1 view .LVU33
 113 005a 0D78     		ldrb	r5, [r1]	@ zero_extendqisi2
 114 005c 32F82530 		ldrh	r3, [r2, r5, lsl #2]
 115 0060 9BB2     		uxth	r3, r3
ARM GAS  /tmp/ccJPteqL.s 			page 38


 116 0062 23F4E043 		bic	r3, r3, #28672
 117 0066 23F07003 		bic	r3, r3, #112
 118              	.LVL7:
 119              		.loc 1 1995 7 is_stmt 1 discriminator 1 view .LVU34
 120 006a 43F40043 		orr	r3, r3, #32768
 121              	.LVL8:
 122              		.loc 1 1995 7 is_stmt 0 discriminator 1 view .LVU35
 123 006e 43F0C003 		orr	r3, r3, #192
 124 0072 22F82530 		strh	r3, [r2, r5, lsl #2]	@ movhi
 125              	.LBE3:
 126              		.loc 1 1995 7 is_stmt 1 discriminator 1 view .LVU36
 127              	.LVL9:
 128              	.L6:
 129              		.loc 1 1995 7 discriminator 6 view .LVU37
 130              		.loc 1 1995 7 discriminator 6 view .LVU38
1996:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
1997:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
1998:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (count != 0U)
 131              		.loc 1 1998 5 discriminator 6 view .LVU39
 132              		.loc 1 1998 8 is_stmt 0 discriminator 6 view .LVU40
 133 0076 24B9     		cbnz	r4, .L13
 134              	.LVL10:
 135              	.L7:
1999:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2000:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       USB_ReadPMA(hpcd->Instance, ep->xfer_buff, ep->pmaaddr0, count);
2001:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2002:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
2003:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Manage Buffer 1 DTOG_RX=0 */
2004:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else
2005:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
2006:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Get count of received data */
2007:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     count = (uint16_t)PCD_GET_EP_DBUF1_CNT(hpcd->Instance, ep->num);
2008:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2009:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (ep->xfer_len >= count)
2010:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2011:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       ep->xfer_len -= count;
2012:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2013:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     else
2014:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2015:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       ep->xfer_len = 0U;
2016:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2017:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2018:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (ep->xfer_len == 0U)
2019:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2020:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* set NAK on the current endpoint */
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_RX_STATUS(hpcd->Instance, ep->num, USB_EP_RX_NAK);
2022:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2023:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2024:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /*Need to FreeUser Buffer*/
2025:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if ((wEPVal & USB_EP_DTOG_TX) == 0U)
2026:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_FREE_USER_BUFFER(hpcd->Instance, ep->num, 0U);
2028:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2029:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2030:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (count != 0U)
2031:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2032:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       USB_ReadPMA(hpcd->Instance, ep->xfer_buff, ep->pmaaddr1, count);
ARM GAS  /tmp/ccJPteqL.s 			page 39


2033:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2034:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
2035:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2036:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return count;
 136              		.loc 1 2036 3 is_stmt 1 view .LVU41
2037:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 137              		.loc 1 2037 1 is_stmt 0 view .LVU42
 138 0078 2046     		mov	r0, r4
 139 007a 38BD     		pop	{r3, r4, r5, pc}
 140              	.LVL11:
 141              	.L3:
1983:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 142              		.loc 1 1983 7 is_stmt 1 view .LVU43
1983:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 143              		.loc 1 1983 20 is_stmt 0 view .LVU44
 144 007c 0023     		movs	r3, #0
 145 007e 8B61     		str	r3, [r1, #24]
 146 0080 D5E7     		b	.L4
 147              	.LVL12:
 148              	.L13:
2000:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 149              		.loc 1 2000 7 is_stmt 1 view .LVU45
 150 0082 2346     		mov	r3, r4
 151 0084 0A89     		ldrh	r2, [r1, #8]
 152 0086 4969     		ldr	r1, [r1, #20]
 153              	.LVL13:
2000:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 154              		.loc 1 2000 7 is_stmt 0 view .LVU46
 155 0088 0068     		ldr	r0, [r0]
 156              	.LVL14:
2000:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 157              		.loc 1 2000 7 view .LVU47
 158 008a FFF7FEFF 		bl	USB_ReadPMA
 159              	.LVL15:
 160 008e F3E7     		b	.L7
 161              	.LVL16:
 162              	.L2:
2007:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 163              		.loc 1 2007 5 is_stmt 1 view .LVU48
2007:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 164              		.loc 1 2007 23 is_stmt 0 view .LVU49
 165 0090 0468     		ldr	r4, [r0]
 166 0092 B4F85030 		ldrh	r3, [r4, #80]
 167 0096 91F800C0 		ldrb	ip, [r1]	@ zero_extendqisi2
 168 009a 4FEACC0E 		lsl	lr, ip, #3
 169 009e 1EFA83F3 		uxtah	r3, lr, r3
 170 00a2 2344     		add	r3, r3, r4
 171 00a4 B3F80644 		ldrh	r4, [r3, #1030]
2007:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 172              		.loc 1 2007 11 view .LVU50
 173 00a8 C4F30904 		ubfx	r4, r4, #0, #10
 174              	.LVL17:
2009:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 175              		.loc 1 2009 5 is_stmt 1 view .LVU51
2009:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 176              		.loc 1 2009 11 is_stmt 0 view .LVU52
 177 00ac 8B69     		ldr	r3, [r1, #24]
ARM GAS  /tmp/ccJPteqL.s 			page 40


2009:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 178              		.loc 1 2009 8 view .LVU53
 179 00ae A342     		cmp	r3, r4
 180 00b0 2FD3     		bcc	.L8
2011:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 181              		.loc 1 2011 7 is_stmt 1 view .LVU54
2011:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 182              		.loc 1 2011 20 is_stmt 0 view .LVU55
 183 00b2 1B1B     		subs	r3, r3, r4
 184 00b4 8B61     		str	r3, [r1, #24]
 185              	.L9:
2018:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 186              		.loc 1 2018 5 is_stmt 1 view .LVU56
2018:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 187              		.loc 1 2018 11 is_stmt 0 view .LVU57
 188 00b6 8B69     		ldr	r3, [r1, #24]
2018:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 189              		.loc 1 2018 8 view .LVU58
 190 00b8 7BB9     		cbnz	r3, .L10
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 191              		.loc 1 2021 7 is_stmt 1 view .LVU59
 192              	.LBB4:
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 193              		.loc 1 2021 7 view .LVU60
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 194              		.loc 1 2021 7 view .LVU61
 195 00ba 0568     		ldr	r5, [r0]
 196 00bc 35F82C30 		ldrh	r3, [r5, ip, lsl #2]
 197 00c0 9BB2     		uxth	r3, r3
 198 00c2 23F48043 		bic	r3, r3, #16384
 199 00c6 23F07003 		bic	r3, r3, #112
 200              	.LVL18:
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 201              		.loc 1 2021 7 view .LVU62
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 202              		.loc 1 2021 7 view .LVU63
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 203              		.loc 1 2021 7 view .LVU64
 204 00ca 83F40053 		eor	r3, r3, #8192
 205              	.LVL19:
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 206              		.loc 1 2021 7 view .LVU65
 207 00ce 43F40043 		orr	r3, r3, #32768
 208              	.LVL20:
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 209              		.loc 1 2021 7 is_stmt 0 view .LVU66
 210 00d2 43F08003 		orr	r3, r3, #128
 211 00d6 25F82C30 		strh	r3, [r5, ip, lsl #2]	@ movhi
 212              	.LVL21:
 213              	.L10:
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 214              		.loc 1 2021 7 view .LVU67
 215              	.LBE4:
2021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 216              		.loc 1 2021 7 is_stmt 1 discriminator 7 view .LVU68
2025:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 217              		.loc 1 2025 5 discriminator 7 view .LVU69
ARM GAS  /tmp/ccJPteqL.s 			page 41


2025:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 218              		.loc 1 2025 8 is_stmt 0 discriminator 7 view .LVU70
 219 00da 12F0400F 		tst	r2, #64
 220 00de 0FD1     		bne	.L11
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 221              		.loc 1 2027 7 is_stmt 1 discriminator 1 view .LVU71
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 222              		.loc 1 2027 7 discriminator 1 view .LVU72
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 223              		.loc 1 2027 7 discriminator 1 view .LVU73
 224              	.LBB5:
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 225              		.loc 1 2027 7 discriminator 1 view .LVU74
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 226              		.loc 1 2027 7 discriminator 1 view .LVU75
 227 00e0 0268     		ldr	r2, [r0]
 228              	.LVL22:
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 229              		.loc 1 2027 7 is_stmt 0 discriminator 1 view .LVU76
 230 00e2 91F800C0 		ldrb	ip, [r1]	@ zero_extendqisi2
 231 00e6 32F82C30 		ldrh	r3, [r2, ip, lsl #2]
 232 00ea 9BB2     		uxth	r3, r3
 233 00ec 23F4E043 		bic	r3, r3, #28672
 234 00f0 23F07003 		bic	r3, r3, #112
 235              	.LVL23:
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 236              		.loc 1 2027 7 is_stmt 1 discriminator 1 view .LVU77
 237 00f4 43F40043 		orr	r3, r3, #32768
 238              	.LVL24:
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 239              		.loc 1 2027 7 is_stmt 0 discriminator 1 view .LVU78
 240 00f8 43F0C003 		orr	r3, r3, #192
 241 00fc 22F82C30 		strh	r3, [r2, ip, lsl #2]	@ movhi
 242              	.LBE5:
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 243              		.loc 1 2027 7 is_stmt 1 discriminator 1 view .LVU79
 244              	.LVL25:
 245              	.L11:
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 246              		.loc 1 2027 7 discriminator 6 view .LVU80
2027:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 247              		.loc 1 2027 7 discriminator 6 view .LVU81
2030:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 248              		.loc 1 2030 5 discriminator 6 view .LVU82
2030:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 249              		.loc 1 2030 8 is_stmt 0 discriminator 6 view .LVU83
 250 0100 002C     		cmp	r4, #0
 251 0102 B9D0     		beq	.L7
2032:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 252              		.loc 1 2032 7 is_stmt 1 view .LVU84
 253 0104 2346     		mov	r3, r4
 254 0106 4A89     		ldrh	r2, [r1, #10]
 255 0108 4969     		ldr	r1, [r1, #20]
 256              	.LVL26:
2032:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 257              		.loc 1 2032 7 is_stmt 0 view .LVU85
 258 010a 0068     		ldr	r0, [r0]
ARM GAS  /tmp/ccJPteqL.s 			page 42


 259              	.LVL27:
2032:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 260              		.loc 1 2032 7 view .LVU86
 261 010c FFF7FEFF 		bl	USB_ReadPMA
 262              	.LVL28:
 263 0110 B2E7     		b	.L7
 264              	.LVL29:
 265              	.L8:
2015:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 266              		.loc 1 2015 7 is_stmt 1 view .LVU87
2015:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 267              		.loc 1 2015 20 is_stmt 0 view .LVU88
 268 0112 0023     		movs	r3, #0
 269 0114 8B61     		str	r3, [r1, #24]
 270 0116 CEE7     		b	.L9
 271              		.cfi_endproc
 272              	.LFE362:
 274              		.section	.text.HAL_PCD_MspInit,"ax",%progbits
 275              		.align	1
 276              		.weak	HAL_PCD_MspInit
 277              		.syntax unified
 278              		.thumb
 279              		.thumb_func
 281              	HAL_PCD_MspInit:
 282              	.LVL30:
 283              	.LFB331:
 260:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 284              		.loc 1 260 1 is_stmt 1 view -0
 285              		.cfi_startproc
 286              		@ args = 0, pretend = 0, frame = 0
 287              		@ frame_needed = 0, uses_anonymous_args = 0
 288              		@ link register save eliminated.
 262:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 289              		.loc 1 262 3 view .LVU90
 267:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 290              		.loc 1 267 1 is_stmt 0 view .LVU91
 291 0000 7047     		bx	lr
 292              		.cfi_endproc
 293              	.LFE331:
 295              		.section	.text.HAL_PCD_Init,"ax",%progbits
 296              		.align	1
 297              		.global	HAL_PCD_Init
 298              		.syntax unified
 299              		.thumb
 300              		.thumb_func
 302              	HAL_PCD_Init:
 303              	.LVL31:
 304              	.LFB329:
 125:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint8_t i;
 305              		.loc 1 125 1 is_stmt 1 view -0
 306              		.cfi_startproc
 307              		@ args = 0, pretend = 0, frame = 0
 308              		@ frame_needed = 0, uses_anonymous_args = 0
 126:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 309              		.loc 1 126 3 view .LVU93
 129:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 310              		.loc 1 129 3 view .LVU94
ARM GAS  /tmp/ccJPteqL.s 			page 43


 129:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 311              		.loc 1 129 6 is_stmt 0 view .LVU95
 312 0000 0028     		cmp	r0, #0
 313 0002 6DD0     		beq	.L22
 125:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint8_t i;
 314              		.loc 1 125 1 view .LVU96
 315 0004 30B5     		push	{r4, r5, lr}
 316              	.LCFI1:
 317              		.cfi_def_cfa_offset 12
 318              		.cfi_offset 4, -12
 319              		.cfi_offset 5, -8
 320              		.cfi_offset 14, -4
 321 0006 87B0     		sub	sp, sp, #28
 322              	.LCFI2:
 323              		.cfi_def_cfa_offset 40
 324 0008 0446     		mov	r4, r0
 135:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 325              		.loc 1 135 3 is_stmt 1 view .LVU97
 137:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 326              		.loc 1 137 3 view .LVU98
 137:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 327              		.loc 1 137 11 is_stmt 0 view .LVU99
 328 000a 90F8A932 		ldrb	r3, [r0, #681]	@ zero_extendqisi2
 137:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 329              		.loc 1 137 6 view .LVU100
 330 000e 3BB1     		cbz	r3, .L28
 331              	.LVL32:
 332              	.L17:
 170:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 333              		.loc 1 170 3 is_stmt 1 view .LVU101
 170:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 334              		.loc 1 170 15 is_stmt 0 view .LVU102
 335 0010 0323     		movs	r3, #3
 336 0012 84F8A932 		strb	r3, [r4, #681]
 173:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 337              		.loc 1 173 3 is_stmt 1 view .LVU103
 338 0016 2068     		ldr	r0, [r4]
 339 0018 FFF7FEFF 		bl	USB_DisableGlobalInt
 340              	.LVL33:
 176:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 341              		.loc 1 176 3 view .LVU104
 176:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 342              		.loc 1 176 10 is_stmt 0 view .LVU105
 343 001c 0023     		movs	r3, #0
 176:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 344              		.loc 1 176 3 view .LVU106
 345 001e 1FE0     		b	.L18
 346              	.LVL34:
 347              	.L28:
 140:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 348              		.loc 1 140 5 is_stmt 1 view .LVU107
 140:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 349              		.loc 1 140 16 is_stmt 0 view .LVU108
 350 0020 80F8A832 		strb	r3, [r0, #680]
 166:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* (USE_HAL_PCD_REGISTER_CALLBACKS) */
 351              		.loc 1 166 5 is_stmt 1 view .LVU109
 352 0024 FFF7FEFF 		bl	HAL_PCD_MspInit
ARM GAS  /tmp/ccJPteqL.s 			page 44


 353              	.LVL35:
 166:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* (USE_HAL_PCD_REGISTER_CALLBACKS) */
 354              		.loc 1 166 5 is_stmt 0 view .LVU110
 355 0028 F2E7     		b	.L17
 356              	.LVL36:
 357              	.L19:
 179:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].num = i;
 358              		.loc 1 179 5 is_stmt 1 discriminator 3 view .LVU111
 179:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].num = i;
 359              		.loc 1 179 26 is_stmt 0 discriminator 3 view .LVU112
 360 002a 5A1C     		adds	r2, r3, #1
 361 002c 02EB8201 		add	r1, r2, r2, lsl #2
 362 0030 04EBC101 		add	r1, r4, r1, lsl #3
 363 0034 0120     		movs	r0, #1
 364 0036 4870     		strb	r0, [r1, #1]
 180:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].tx_fifo_num = i;
 365              		.loc 1 180 5 is_stmt 1 discriminator 3 view .LVU113
 180:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].tx_fifo_num = i;
 366              		.loc 1 180 24 is_stmt 0 discriminator 3 view .LVU114
 367 0038 02EB8201 		add	r1, r2, r2, lsl #2
 368 003c 04F83130 		strb	r3, [r4, r1, lsl #3]
 181:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Control until ep is activated */
 369              		.loc 1 181 5 is_stmt 1 discriminator 3 view .LVU115
 181:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Control until ep is activated */
 370              		.loc 1 181 32 is_stmt 0 discriminator 3 view .LVU116
 371 0040 03EB8301 		add	r1, r3, r3, lsl #2
 372 0044 04EBC101 		add	r1, r4, r1, lsl #3
 373 0048 CB86     		strh	r3, [r1, #54]	@ movhi
 183:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].maxpacket = 0U;
 374              		.loc 1 183 5 is_stmt 1 discriminator 3 view .LVU117
 183:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].maxpacket = 0U;
 375              		.loc 1 183 25 is_stmt 0 discriminator 3 view .LVU118
 376 004a 02EB820C 		add	ip, r2, r2, lsl #2
 377 004e 04EBCC0C 		add	ip, r4, ip, lsl #3
 378 0052 0020     		movs	r0, #0
 379 0054 8CF80300 		strb	r0, [ip, #3]
 184:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].xfer_buff = 0U;
 380              		.loc 1 184 5 is_stmt 1 discriminator 3 view .LVU119
 184:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].xfer_buff = 0U;
 381              		.loc 1 184 30 is_stmt 0 discriminator 3 view .LVU120
 382 0058 8863     		str	r0, [r1, #56]
 185:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].xfer_len = 0U;
 383              		.loc 1 185 5 is_stmt 1 discriminator 3 view .LVU121
 185:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->IN_ep[i].xfer_len = 0U;
 384              		.loc 1 185 30 is_stmt 0 discriminator 3 view .LVU122
 385 005a C863     		str	r0, [r1, #60]
 186:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 386              		.loc 1 186 5 is_stmt 1 discriminator 3 view .LVU123
 186:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 387              		.loc 1 186 29 is_stmt 0 discriminator 3 view .LVU124
 388 005c 0864     		str	r0, [r1, #64]
 176:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 389              		.loc 1 176 47 is_stmt 1 discriminator 3 view .LVU125
 390 005e D3B2     		uxtb	r3, r2
 391              	.LVL37:
 392              	.L18:
 176:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
ARM GAS  /tmp/ccJPteqL.s 			page 45


 393              		.loc 1 176 18 discriminator 1 view .LVU126
 176:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 394              		.loc 1 176 30 is_stmt 0 discriminator 1 view .LVU127
 395 0060 6068     		ldr	r0, [r4, #4]
 176:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 396              		.loc 1 176 18 discriminator 1 view .LVU128
 397 0062 8342     		cmp	r3, r0
 398 0064 E1D3     		bcc	.L19
 189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 399              		.loc 1 189 10 view .LVU129
 400 0066 0023     		movs	r3, #0
 401              	.LVL38:
 189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 402              		.loc 1 189 10 view .LVU130
 403 0068 16E0     		b	.L20
 404              	.LVL39:
 405              	.L21:
 191:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].num = i;
 406              		.loc 1 191 5 is_stmt 1 discriminator 3 view .LVU131
 191:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].num = i;
 407              		.loc 1 191 27 is_stmt 0 discriminator 3 view .LVU132
 408 006a 03EB8302 		add	r2, r3, r3, lsl #2
 409 006e 04EBC202 		add	r2, r4, r2, lsl #3
 410 0072 0021     		movs	r1, #0
 411 0074 82F86911 		strb	r1, [r2, #361]
 192:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Control until ep is activated */
 412              		.loc 1 192 5 is_stmt 1 discriminator 3 view .LVU133
 192:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Control until ep is activated */
 413              		.loc 1 192 25 is_stmt 0 discriminator 3 view .LVU134
 414 0078 82F86831 		strb	r3, [r2, #360]
 194:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].maxpacket = 0U;
 415              		.loc 1 194 5 is_stmt 1 discriminator 3 view .LVU135
 194:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].maxpacket = 0U;
 416              		.loc 1 194 26 is_stmt 0 discriminator 3 view .LVU136
 417 007c 82F86B11 		strb	r1, [r2, #363]
 195:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].xfer_buff = 0U;
 418              		.loc 1 195 5 is_stmt 1 discriminator 3 view .LVU137
 195:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].xfer_buff = 0U;
 419              		.loc 1 195 31 is_stmt 0 discriminator 3 view .LVU138
 420 0080 C2F87811 		str	r1, [r2, #376]
 196:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].xfer_len = 0U;
 421              		.loc 1 196 5 is_stmt 1 discriminator 3 view .LVU139
 196:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->OUT_ep[i].xfer_len = 0U;
 422              		.loc 1 196 31 is_stmt 0 discriminator 3 view .LVU140
 423 0084 C2F87C11 		str	r1, [r2, #380]
 197:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 424              		.loc 1 197 5 is_stmt 1 discriminator 3 view .LVU141
 197:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 425              		.loc 1 197 30 is_stmt 0 discriminator 3 view .LVU142
 426 0088 03EB8302 		add	r2, r3, r3, lsl #2
 427 008c 04EBC202 		add	r2, r4, r2, lsl #3
 428 0090 C2F88011 		str	r1, [r2, #384]
 189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 429              		.loc 1 189 47 is_stmt 1 discriminator 3 view .LVU143
 430 0094 0133     		adds	r3, r3, #1
 431              	.LVL40:
 189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
ARM GAS  /tmp/ccJPteqL.s 			page 46


 432              		.loc 1 189 47 is_stmt 0 discriminator 3 view .LVU144
 433 0096 DBB2     		uxtb	r3, r3
 434              	.LVL41:
 435              	.L20:
 189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 436              		.loc 1 189 18 is_stmt 1 discriminator 1 view .LVU145
 437 0098 9842     		cmp	r0, r3
 438 009a E6D8     		bhi	.L21
 201:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 439              		.loc 1 201 3 view .LVU146
 201:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 440              		.loc 1 201 25 is_stmt 0 view .LVU147
 441 009c A446     		mov	ip, r4
 442 009e 5CF8105B 		ldr	r5, [ip], #16
 201:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 443              		.loc 1 201 9 view .LVU148
 444 00a2 EE46     		mov	lr, sp
 445 00a4 BCE80F00 		ldmia	ip!, {r0, r1, r2, r3}
 446              	.LVL42:
 201:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 447              		.loc 1 201 9 view .LVU149
 448 00a8 AEE80F00 		stmia	lr!, {r0, r1, r2, r3}
 449 00ac DCF80030 		ldr	r3, [ip]
 450 00b0 CEF80030 		str	r3, [lr]
 451 00b4 231D     		adds	r3, r4, #4
 452 00b6 0ECB     		ldm	r3, {r1, r2, r3}
 453 00b8 2846     		mov	r0, r5
 454 00ba FFF7FEFF 		bl	USB_DevInit
 455              	.LVL43:
 203:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->State = HAL_PCD_STATE_READY;
 456              		.loc 1 203 3 is_stmt 1 view .LVU150
 203:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->State = HAL_PCD_STATE_READY;
 457              		.loc 1 203 21 is_stmt 0 view .LVU151
 458 00be 0023     		movs	r3, #0
 459 00c0 84F82430 		strb	r3, [r4, #36]
 204:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 460              		.loc 1 204 3 is_stmt 1 view .LVU152
 204:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 461              		.loc 1 204 15 is_stmt 0 view .LVU153
 462 00c4 0123     		movs	r3, #1
 463 00c6 84F8A932 		strb	r3, [r4, #681]
 207:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 464              		.loc 1 207 3 is_stmt 1 view .LVU154
 207:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 465              		.loc 1 207 17 is_stmt 0 view .LVU155
 466 00ca E369     		ldr	r3, [r4, #28]
 207:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 467              		.loc 1 207 6 view .LVU156
 468 00cc 012B     		cmp	r3, #1
 469 00ce 02D0     		beq	.L29
 212:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 470              		.loc 1 212 10 view .LVU157
 471 00d0 0020     		movs	r0, #0
 472              	.L16:
 213:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 473              		.loc 1 213 1 view .LVU158
 474 00d2 07B0     		add	sp, sp, #28
ARM GAS  /tmp/ccJPteqL.s 			page 47


 475              	.LCFI3:
 476              		.cfi_remember_state
 477              		.cfi_def_cfa_offset 12
 478              		@ sp needed
 479 00d4 30BD     		pop	{r4, r5, pc}
 480              	.LVL44:
 481              	.L29:
 482              	.LCFI4:
 483              		.cfi_restore_state
 209:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 484              		.loc 1 209 5 is_stmt 1 view .LVU159
 209:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 485              		.loc 1 209 11 is_stmt 0 view .LVU160
 486 00d6 2046     		mov	r0, r4
 487 00d8 FFF7FEFF 		bl	HAL_PCDEx_ActivateLPM
 488              	.LVL45:
 212:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 489              		.loc 1 212 10 view .LVU161
 490 00dc 0020     		movs	r0, #0
 491 00de F8E7     		b	.L16
 492              	.LVL46:
 493              	.L22:
 494              	.LCFI5:
 495              		.cfi_def_cfa_offset 0
 496              		.cfi_restore 4
 497              		.cfi_restore 5
 498              		.cfi_restore 14
 131:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 499              		.loc 1 131 12 view .LVU162
 500 00e0 0120     		movs	r0, #1
 501              	.LVL47:
 213:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 502              		.loc 1 213 1 view .LVU163
 503 00e2 7047     		bx	lr
 504              		.cfi_endproc
 505              	.LFE329:
 507              		.section	.text.HAL_PCD_MspDeInit,"ax",%progbits
 508              		.align	1
 509              		.weak	HAL_PCD_MspDeInit
 510              		.syntax unified
 511              		.thumb
 512              		.thumb_func
 514              	HAL_PCD_MspDeInit:
 515              	.LVL48:
 516              	.LFB332:
 275:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 517              		.loc 1 275 1 is_stmt 1 view -0
 518              		.cfi_startproc
 519              		@ args = 0, pretend = 0, frame = 0
 520              		@ frame_needed = 0, uses_anonymous_args = 0
 521              		@ link register save eliminated.
 277:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 522              		.loc 1 277 3 view .LVU165
 282:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 523              		.loc 1 282 1 is_stmt 0 view .LVU166
 524 0000 7047     		bx	lr
 525              		.cfi_endproc
ARM GAS  /tmp/ccJPteqL.s 			page 48


 526              	.LFE332:
 528              		.section	.text.HAL_PCD_DeInit,"ax",%progbits
 529              		.align	1
 530              		.global	HAL_PCD_DeInit
 531              		.syntax unified
 532              		.thumb
 533              		.thumb_func
 535              	HAL_PCD_DeInit:
 536              	.LVL49:
 537              	.LFB330:
 221:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Check the PCD handle allocation */
 538              		.loc 1 221 1 is_stmt 1 view -0
 539              		.cfi_startproc
 540              		@ args = 0, pretend = 0, frame = 0
 541              		@ frame_needed = 0, uses_anonymous_args = 0
 221:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Check the PCD handle allocation */
 542              		.loc 1 221 1 is_stmt 0 view .LVU168
 543 0000 38B5     		push	{r3, r4, r5, lr}
 544              	.LCFI6:
 545              		.cfi_def_cfa_offset 16
 546              		.cfi_offset 3, -16
 547              		.cfi_offset 4, -12
 548              		.cfi_offset 5, -8
 549              		.cfi_offset 14, -4
 223:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 550              		.loc 1 223 3 is_stmt 1 view .LVU169
 223:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 551              		.loc 1 223 6 is_stmt 0 view .LVU170
 552 0002 90B1     		cbz	r0, .L33
 553 0004 0446     		mov	r4, r0
 228:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 554              		.loc 1 228 3 is_stmt 1 view .LVU171
 228:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 555              		.loc 1 228 15 is_stmt 0 view .LVU172
 556 0006 0323     		movs	r3, #3
 557 0008 80F8A932 		strb	r3, [r0, #681]
 231:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 558              		.loc 1 231 3 is_stmt 1 view .LVU173
 231:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 559              		.loc 1 231 7 is_stmt 0 view .LVU174
 560 000c 0068     		ldr	r0, [r0]
 561              	.LVL50:
 231:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 562              		.loc 1 231 7 view .LVU175
 563 000e FFF7FEFF 		bl	USB_StopDevice
 564              	.LVL51:
 231:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 565              		.loc 1 231 6 view .LVU176
 566 0012 0546     		mov	r5, r0
 567 0014 10B1     		cbz	r0, .L36
 233:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 568              		.loc 1 233 12 view .LVU177
 569 0016 0125     		movs	r5, #1
 570              	.LVL52:
 571              	.L32:
 252:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 572              		.loc 1 252 1 view .LVU178
ARM GAS  /tmp/ccJPteqL.s 			page 49


 573 0018 2846     		mov	r0, r5
 574 001a 38BD     		pop	{r3, r4, r5, pc}
 575              	.LVL53:
 576              	.L36:
 246:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 577              		.loc 1 246 3 is_stmt 1 view .LVU179
 578 001c 2046     		mov	r0, r4
 579 001e FFF7FEFF 		bl	HAL_PCD_MspDeInit
 580              	.LVL54:
 249:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 581              		.loc 1 249 3 view .LVU180
 249:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 582              		.loc 1 249 15 is_stmt 0 view .LVU181
 583 0022 0023     		movs	r3, #0
 584 0024 84F8A932 		strb	r3, [r4, #681]
 251:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 585              		.loc 1 251 3 is_stmt 1 view .LVU182
 251:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 586              		.loc 1 251 10 is_stmt 0 view .LVU183
 587 0028 F6E7     		b	.L32
 588              	.LVL55:
 589              	.L33:
 225:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 590              		.loc 1 225 12 view .LVU184
 591 002a 0125     		movs	r5, #1
 592 002c F4E7     		b	.L32
 593              		.cfi_endproc
 594              	.LFE330:
 596              		.section	.text.HAL_PCD_Start,"ax",%progbits
 597              		.align	1
 598              		.global	HAL_PCD_Start
 599              		.syntax unified
 600              		.thumb
 601              		.thumb_func
 603              	HAL_PCD_Start:
 604              	.LVL56:
 605              	.LFB333:
 978:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 606              		.loc 1 978 1 is_stmt 1 view -0
 607              		.cfi_startproc
 608              		@ args = 0, pretend = 0, frame = 0
 609              		@ frame_needed = 0, uses_anonymous_args = 0
 979:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_ENABLE(hpcd);
 610              		.loc 1 979 3 view .LVU186
 979:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_ENABLE(hpcd);
 611              		.loc 1 979 3 view .LVU187
 612 0000 90F8A832 		ldrb	r3, [r0, #680]	@ zero_extendqisi2
 613 0004 012B     		cmp	r3, #1
 614 0006 0ED0     		beq	.L39
 978:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 615              		.loc 1 978 1 is_stmt 0 discriminator 2 view .LVU188
 616 0008 10B5     		push	{r4, lr}
 617              	.LCFI7:
 618              		.cfi_def_cfa_offset 8
 619              		.cfi_offset 4, -8
 620              		.cfi_offset 14, -4
 621 000a 0446     		mov	r4, r0
ARM GAS  /tmp/ccJPteqL.s 			page 50


 979:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_ENABLE(hpcd);
 622              		.loc 1 979 3 is_stmt 1 discriminator 2 view .LVU189
 623 000c 0123     		movs	r3, #1
 624 000e 80F8A832 		strb	r3, [r0, #680]
 979:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_ENABLE(hpcd);
 625              		.loc 1 979 3 discriminator 2 view .LVU190
 980:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevConnect(hpcd->Instance);
 626              		.loc 1 980 3 discriminator 2 view .LVU191
 627 0012 0068     		ldr	r0, [r0]
 628              	.LVL57:
 980:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevConnect(hpcd->Instance);
 629              		.loc 1 980 3 is_stmt 0 discriminator 2 view .LVU192
 630 0014 FFF7FEFF 		bl	USB_EnableGlobalInt
 631              	.LVL58:
 981:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 632              		.loc 1 981 3 is_stmt 1 discriminator 2 view .LVU193
 981:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 633              		.loc 1 981 9 is_stmt 0 discriminator 2 view .LVU194
 634 0018 2068     		ldr	r0, [r4]
 635 001a FFF7FEFF 		bl	USB_DevConnect
 636              	.LVL59:
 982:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 637              		.loc 1 982 3 is_stmt 1 discriminator 2 view .LVU195
 982:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 638              		.loc 1 982 3 discriminator 2 view .LVU196
 639 001e 0020     		movs	r0, #0
 640 0020 84F8A802 		strb	r0, [r4, #680]
 982:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 641              		.loc 1 982 3 discriminator 2 view .LVU197
 984:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 642              		.loc 1 984 3 discriminator 2 view .LVU198
 985:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 643              		.loc 1 985 1 is_stmt 0 discriminator 2 view .LVU199
 644 0024 10BD     		pop	{r4, pc}
 645              	.LVL60:
 646              	.L39:
 647              	.LCFI8:
 648              		.cfi_def_cfa_offset 0
 649              		.cfi_restore 4
 650              		.cfi_restore 14
 979:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_ENABLE(hpcd);
 651              		.loc 1 979 3 view .LVU200
 652 0026 0220     		movs	r0, #2
 653              	.LVL61:
 985:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 654              		.loc 1 985 1 view .LVU201
 655 0028 7047     		bx	lr
 656              		.cfi_endproc
 657              	.LFE333:
 659              		.section	.text.HAL_PCD_Stop,"ax",%progbits
 660              		.align	1
 661              		.global	HAL_PCD_Stop
 662              		.syntax unified
 663              		.thumb
 664              		.thumb_func
 666              	HAL_PCD_Stop:
 667              	.LVL62:
ARM GAS  /tmp/ccJPteqL.s 			page 51


 668              	.LFB334:
 993:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 669              		.loc 1 993 1 is_stmt 1 view -0
 670              		.cfi_startproc
 671              		@ args = 0, pretend = 0, frame = 0
 672              		@ frame_needed = 0, uses_anonymous_args = 0
 994:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_DISABLE(hpcd);
 673              		.loc 1 994 3 view .LVU203
 994:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_DISABLE(hpcd);
 674              		.loc 1 994 3 view .LVU204
 675 0000 90F8A832 		ldrb	r3, [r0, #680]	@ zero_extendqisi2
 676 0004 012B     		cmp	r3, #1
 677 0006 0ED0     		beq	.L46
 993:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 678              		.loc 1 993 1 is_stmt 0 discriminator 2 view .LVU205
 679 0008 10B5     		push	{r4, lr}
 680              	.LCFI9:
 681              		.cfi_def_cfa_offset 8
 682              		.cfi_offset 4, -8
 683              		.cfi_offset 14, -4
 684 000a 0446     		mov	r4, r0
 994:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_DISABLE(hpcd);
 685              		.loc 1 994 3 is_stmt 1 discriminator 2 view .LVU206
 686 000c 0123     		movs	r3, #1
 687 000e 80F8A832 		strb	r3, [r0, #680]
 994:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_DISABLE(hpcd);
 688              		.loc 1 994 3 discriminator 2 view .LVU207
 995:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevDisconnect(hpcd->Instance);
 689              		.loc 1 995 3 discriminator 2 view .LVU208
 690 0012 0068     		ldr	r0, [r0]
 691              	.LVL63:
 995:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevDisconnect(hpcd->Instance);
 692              		.loc 1 995 3 is_stmt 0 discriminator 2 view .LVU209
 693 0014 FFF7FEFF 		bl	USB_DisableGlobalInt
 694              	.LVL64:
 996:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 695              		.loc 1 996 3 is_stmt 1 discriminator 2 view .LVU210
 996:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 696              		.loc 1 996 9 is_stmt 0 discriminator 2 view .LVU211
 697 0018 2068     		ldr	r0, [r4]
 698 001a FFF7FEFF 		bl	USB_DevDisconnect
 699              	.LVL65:
 997:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 700              		.loc 1 997 3 is_stmt 1 discriminator 2 view .LVU212
 997:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 701              		.loc 1 997 3 discriminator 2 view .LVU213
 702 001e 0020     		movs	r0, #0
 703 0020 84F8A802 		strb	r0, [r4, #680]
 997:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 704              		.loc 1 997 3 discriminator 2 view .LVU214
 999:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 705              		.loc 1 999 3 discriminator 2 view .LVU215
1000:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 706              		.loc 1 1000 1 is_stmt 0 discriminator 2 view .LVU216
 707 0024 10BD     		pop	{r4, pc}
 708              	.LVL66:
 709              	.L46:
ARM GAS  /tmp/ccJPteqL.s 			page 52


 710              	.LCFI10:
 711              		.cfi_def_cfa_offset 0
 712              		.cfi_restore 4
 713              		.cfi_restore 14
 994:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_PCD_DISABLE(hpcd);
 714              		.loc 1 994 3 view .LVU217
 715 0026 0220     		movs	r0, #2
 716              	.LVL67:
1000:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 717              		.loc 1 1000 1 view .LVU218
 718 0028 7047     		bx	lr
 719              		.cfi_endproc
 720              	.LFE334:
 722              		.section	.text.HAL_PCD_DataOutStageCallback,"ax",%progbits
 723              		.align	1
 724              		.weak	HAL_PCD_DataOutStageCallback
 725              		.syntax unified
 726              		.thumb
 727              		.thumb_func
 729              	HAL_PCD_DataOutStageCallback:
 730              	.LVL68:
 731              	.LFB336:
1155:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 732              		.loc 1 1155 1 is_stmt 1 view -0
 733              		.cfi_startproc
 734              		@ args = 0, pretend = 0, frame = 0
 735              		@ frame_needed = 0, uses_anonymous_args = 0
 736              		@ link register save eliminated.
1157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(epnum);
 737              		.loc 1 1157 3 view .LVU220
1158:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 738              		.loc 1 1158 3 view .LVU221
1163:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 739              		.loc 1 1163 1 is_stmt 0 view .LVU222
 740 0000 7047     		bx	lr
 741              		.cfi_endproc
 742              	.LFE336:
 744              		.section	.text.HAL_PCD_DataInStageCallback,"ax",%progbits
 745              		.align	1
 746              		.weak	HAL_PCD_DataInStageCallback
 747              		.syntax unified
 748              		.thumb
 749              		.thumb_func
 751              	HAL_PCD_DataInStageCallback:
 752              	.LVL69:
 753              	.LFB337:
1172:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 754              		.loc 1 1172 1 is_stmt 1 view -0
 755              		.cfi_startproc
 756              		@ args = 0, pretend = 0, frame = 0
 757              		@ frame_needed = 0, uses_anonymous_args = 0
 758              		@ link register save eliminated.
1174:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(epnum);
 759              		.loc 1 1174 3 view .LVU224
1175:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 760              		.loc 1 1175 3 view .LVU225
1180:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
ARM GAS  /tmp/ccJPteqL.s 			page 53


 761              		.loc 1 1180 1 is_stmt 0 view .LVU226
 762 0000 7047     		bx	lr
 763              		.cfi_endproc
 764              	.LFE337:
 766              		.section	.text.HAL_PCD_EP_DB_Transmit,"ax",%progbits
 767              		.align	1
 768              		.syntax unified
 769              		.thumb
 770              		.thumb_func
 772              	HAL_PCD_EP_DB_Transmit:
 773              	.LVL70:
 774              	.LFB363:
2038:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2039:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2040:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
2041:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @brief  Manage double buffer bulk IN transaction from ISR
2042:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  hpcd PCD handle
2043:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  ep current endpoint handle
2044:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @param  wEPVal Last snapshot of EPRx register value taken in ISR
2045:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   * @retval HAL status
2046:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   */
2047:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** static HAL_StatusTypeDef HAL_PCD_EP_DB_Transmit(PCD_HandleTypeDef *hpcd,
2048:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                                                 PCD_EPTypeDef *ep, uint16_t wEPVal)
2049:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** {
 775              		.loc 1 2049 1 is_stmt 1 view -0
 776              		.cfi_startproc
 777              		@ args = 0, pretend = 0, frame = 0
 778              		@ frame_needed = 0, uses_anonymous_args = 0
 779              		.loc 1 2049 1 is_stmt 0 view .LVU228
 780 0000 70B5     		push	{r4, r5, r6, lr}
 781              	.LCFI11:
 782              		.cfi_def_cfa_offset 16
 783              		.cfi_offset 4, -16
 784              		.cfi_offset 5, -12
 785              		.cfi_offset 6, -8
 786              		.cfi_offset 14, -4
 787 0002 0546     		mov	r5, r0
 788 0004 0C46     		mov	r4, r1
 789 0006 1646     		mov	r6, r2
2050:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint32_t len;
 790              		.loc 1 2050 3 is_stmt 1 view .LVU229
2051:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint16_t TxPctSize;
 791              		.loc 1 2051 3 view .LVU230
2052:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2053:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Data Buffer0 ACK received */
2054:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   if ((wEPVal & USB_EP_DTOG_TX) != 0U)
 792              		.loc 1 2054 3 view .LVU231
 793              		.loc 1 2054 6 is_stmt 0 view .LVU232
 794 0008 12F0400F 		tst	r2, #64
 795 000c 00F00981 		beq	.L54
2055:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
2056:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* multi-packet on the NON control IN endpoint */
2057:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     TxPctSize = (uint16_t)PCD_GET_EP_DBUF0_CNT(hpcd->Instance, ep->num);
 796              		.loc 1 2057 5 is_stmt 1 view .LVU233
 797              		.loc 1 2057 27 is_stmt 0 view .LVU234
 798 0010 0268     		ldr	r2, [r0]
 799              	.LVL71:
ARM GAS  /tmp/ccJPteqL.s 			page 54


 800              		.loc 1 2057 27 view .LVU235
 801 0012 B2F85030 		ldrh	r3, [r2, #80]
 802 0016 0978     		ldrb	r1, [r1]	@ zero_extendqisi2
 803              	.LVL72:
 804              		.loc 1 2057 27 view .LVU236
 805 0018 C800     		lsls	r0, r1, #3
 806              	.LVL73:
 807              		.loc 1 2057 27 view .LVU237
 808 001a 10FA83F3 		uxtah	r3, r0, r3
 809 001e 1344     		add	r3, r3, r2
 810 0020 B3F80224 		ldrh	r2, [r3, #1026]
 811              		.loc 1 2057 15 view .LVU238
 812 0024 C2F30902 		ubfx	r2, r2, #0, #10
 813              	.LVL74:
2058:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2059:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (ep->xfer_len > TxPctSize)
 814              		.loc 1 2059 5 is_stmt 1 view .LVU239
 815              		.loc 1 2059 11 is_stmt 0 view .LVU240
 816 0028 A369     		ldr	r3, [r4, #24]
 817              		.loc 1 2059 8 view .LVU241
 818 002a 9342     		cmp	r3, r2
 819 002c 51D9     		bls	.L55
2060:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2061:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       ep->xfer_len -= TxPctSize;
 820              		.loc 1 2061 7 is_stmt 1 view .LVU242
 821              		.loc 1 2061 20 is_stmt 0 view .LVU243
 822 002e 9B1A     		subs	r3, r3, r2
 823 0030 A361     		str	r3, [r4, #24]
 824              	.L56:
2062:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2063:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     else
2064:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2065:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       ep->xfer_len = 0U;
2066:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2067:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2068:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Transfer is completed */
2069:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (ep->xfer_len == 0U)
 825              		.loc 1 2069 5 is_stmt 1 view .LVU244
 826              		.loc 1 2069 11 is_stmt 0 view .LVU245
 827 0032 A369     		ldr	r3, [r4, #24]
 828              		.loc 1 2069 8 view .LVU246
 829 0034 002B     		cmp	r3, #0
 830 0036 68D1     		bne	.L57
2070:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF0_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 831              		.loc 1 2071 7 is_stmt 1 view .LVU247
 832              		.loc 1 2071 7 view .LVU248
 833 0038 6378     		ldrb	r3, [r4, #1]	@ zero_extendqisi2
 834 003a 002B     		cmp	r3, #0
 835 003c 4CD1     		bne	.L58
 836              		.loc 1 2071 7 discriminator 1 view .LVU249
 837              	.LBB6:
 838              		.loc 1 2071 7 discriminator 1 view .LVU250
 839 003e 2A68     		ldr	r2, [r5]
 840              	.LVL75:
 841              		.loc 1 2071 7 discriminator 1 view .LVU251
 842              		.loc 1 2071 7 discriminator 1 view .LVU252
ARM GAS  /tmp/ccJPteqL.s 			page 55


 843 0040 B2F85030 		ldrh	r3, [r2, #80]
 844 0044 12FA83F3 		uxtah	r3, r2, r3
 845              	.LVL76:
 846              		.loc 1 2071 7 discriminator 1 view .LVU253
 847 0048 0344     		add	r3, r3, r0
 848              	.LVL77:
 849              		.loc 1 2071 7 discriminator 1 view .LVU254
 850              	.LBB7:
 851              		.loc 1 2071 7 discriminator 1 view .LVU255
 852              		.loc 1 2071 7 discriminator 1 view .LVU256
 853              		.loc 1 2071 7 discriminator 1 view .LVU257
 854              		.loc 1 2071 7 discriminator 1 view .LVU258
 855 004a B3F80224 		ldrh	r2, [r3, #1026]
 856 004e 92B2     		uxth	r2, r2
 857 0050 22F4F842 		bic	r2, r2, #31744
 858 0054 92B2     		uxth	r2, r2
 859 0056 A3F80224 		strh	r2, [r3, #1026]	@ movhi
 860              		.loc 1 2071 7 discriminator 1 view .LVU259
 861 005a B3F80224 		ldrh	r2, [r3, #1026]
 862 005e 6FEA4242 		mvn	r2, r2, lsl #17
 863 0062 6FEA5242 		mvn	r2, r2, lsr #17
 864 0066 92B2     		uxth	r2, r2
 865 0068 A3F80224 		strh	r2, [r3, #1026]	@ movhi
 866              	.LVL78:
 867              	.L59:
 868              		.loc 1 2071 7 is_stmt 0 discriminator 1 view .LVU260
 869              	.LBE7:
 870              	.LBE6:
 871              		.loc 1 2071 7 is_stmt 1 discriminator 18 view .LVU261
 872              		.loc 1 2071 7 discriminator 18 view .LVU262
2072:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 873              		.loc 1 2072 7 discriminator 18 view .LVU263
 874              	.LBB8:
 875              		.loc 1 2072 7 discriminator 18 view .LVU264
 876 006c 2A68     		ldr	r2, [r5]
 877              	.LVL79:
 878              		.loc 1 2072 7 discriminator 18 view .LVU265
 879              		.loc 1 2072 7 discriminator 18 view .LVU266
 880 006e 6378     		ldrb	r3, [r4, #1]	@ zero_extendqisi2
 881 0070 002B     		cmp	r3, #0
 882 0072 3DD1     		bne	.L60
 883              		.loc 1 2072 7 discriminator 1 view .LVU267
 884              	.LBB9:
 885              		.loc 1 2072 7 discriminator 1 view .LVU268
 886              	.LVL80:
 887              		.loc 1 2072 7 discriminator 1 view .LVU269
 888              		.loc 1 2072 7 discriminator 1 view .LVU270
 889 0074 B2F85030 		ldrh	r3, [r2, #80]
 890 0078 12FA83F3 		uxtah	r3, r2, r3
 891              	.LVL81:
 892              		.loc 1 2072 7 discriminator 1 view .LVU271
 893 007c 2278     		ldrb	r2, [r4]	@ zero_extendqisi2
 894              	.LVL82:
 895              		.loc 1 2072 7 is_stmt 0 discriminator 1 view .LVU272
 896 007e 03EBC203 		add	r3, r3, r2, lsl #3
 897              	.LVL83:
 898              		.loc 1 2072 7 is_stmt 1 discriminator 1 view .LVU273
ARM GAS  /tmp/ccJPteqL.s 			page 56


 899              	.LBB10:
 900              		.loc 1 2072 7 discriminator 1 view .LVU274
 901              		.loc 1 2072 7 discriminator 1 view .LVU275
 902              		.loc 1 2072 7 discriminator 1 view .LVU276
 903              		.loc 1 2072 7 discriminator 1 view .LVU277
 904 0082 B3F80624 		ldrh	r2, [r3, #1030]
 905 0086 92B2     		uxth	r2, r2
 906 0088 22F4F842 		bic	r2, r2, #31744
 907 008c 92B2     		uxth	r2, r2
 908 008e A3F80624 		strh	r2, [r3, #1030]	@ movhi
 909              	.LVL84:
 910              		.loc 1 2072 7 discriminator 1 view .LVU278
 911 0092 B3F80624 		ldrh	r2, [r3, #1030]
 912 0096 6FEA4242 		mvn	r2, r2, lsl #17
 913 009a 6FEA5242 		mvn	r2, r2, lsr #17
 914 009e 92B2     		uxth	r2, r2
 915 00a0 A3F80624 		strh	r2, [r3, #1030]	@ movhi
 916              	.LVL85:
 917              	.L61:
 918              		.loc 1 2072 7 is_stmt 0 discriminator 1 view .LVU279
 919              	.LBE10:
 920              	.LBE9:
 921              	.LBE8:
 922              		.loc 1 2072 7 is_stmt 1 discriminator 18 view .LVU280
2073:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2074:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* TX COMPLETE */
2075:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
2076:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->DataInStageCallback(hpcd, ep->num);
2077:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
2078:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       HAL_PCD_DataInStageCallback(hpcd, ep->num);
 923              		.loc 1 2078 7 discriminator 18 view .LVU281
 924 00a4 2178     		ldrb	r1, [r4]	@ zero_extendqisi2
 925 00a6 2846     		mov	r0, r5
 926 00a8 FFF7FEFF 		bl	HAL_PCD_DataInStageCallback
 927              	.LVL86:
2079:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
2080:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2081:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       if ((wEPVal & USB_EP_DTOG_RX) != 0U)
 928              		.loc 1 2081 7 discriminator 18 view .LVU282
 929              		.loc 1 2081 10 is_stmt 0 discriminator 18 view .LVU283
 930 00ac 16F4804F 		tst	r6, #16384
 931 00b0 40D0     		beq	.L62
2082:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
2083:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         PCD_FREE_USER_BUFFER(hpcd->Instance, ep->num, 1U);
 932              		.loc 1 2083 9 is_stmt 1 discriminator 4 view .LVU284
 933              		.loc 1 2083 9 discriminator 4 view .LVU285
 934              		.loc 1 2083 9 discriminator 4 view .LVU286
 935              		.loc 1 2083 9 discriminator 4 view .LVU287
 936              	.LBB11:
 937              		.loc 1 2083 9 discriminator 4 view .LVU288
 938              		.loc 1 2083 9 discriminator 4 view .LVU289
 939 00b2 2A68     		ldr	r2, [r5]
 940 00b4 2178     		ldrb	r1, [r4]	@ zero_extendqisi2
 941 00b6 32F82130 		ldrh	r3, [r2, r1, lsl #2]
 942 00ba 9BB2     		uxth	r3, r3
 943 00bc 23F4E043 		bic	r3, r3, #28672
 944 00c0 23F07003 		bic	r3, r3, #112
ARM GAS  /tmp/ccJPteqL.s 			page 57


 945              	.LVL87:
 946              		.loc 1 2083 9 discriminator 4 view .LVU290
 947 00c4 43F44043 		orr	r3, r3, #49152
 948              	.LVL88:
 949              		.loc 1 2083 9 is_stmt 0 discriminator 4 view .LVU291
 950 00c8 43F08003 		orr	r3, r3, #128
 951 00cc 22F82130 		strh	r3, [r2, r1, lsl #2]	@ movhi
 952 00d0 30E0     		b	.L62
 953              	.LVL89:
 954              	.L55:
 955              		.loc 1 2083 9 discriminator 4 view .LVU292
 956              	.LBE11:
2065:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 957              		.loc 1 2065 7 is_stmt 1 view .LVU293
2065:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 958              		.loc 1 2065 20 is_stmt 0 view .LVU294
 959 00d2 0023     		movs	r3, #0
 960 00d4 A361     		str	r3, [r4, #24]
 961 00d6 ACE7     		b	.L56
 962              	.L58:
2071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 963              		.loc 1 2071 7 is_stmt 1 discriminator 2 view .LVU295
 964 00d8 012B     		cmp	r3, #1
 965 00da C7D1     		bne	.L59
2071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 966              		.loc 1 2071 7 discriminator 16 view .LVU296
 967              	.LBB12:
2071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 968              		.loc 1 2071 7 discriminator 16 view .LVU297
 969 00dc 2A68     		ldr	r2, [r5]
 970              	.LVL90:
2071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 971              		.loc 1 2071 7 discriminator 16 view .LVU298
2071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 972              		.loc 1 2071 7 discriminator 16 view .LVU299
 973 00de B2F85030 		ldrh	r3, [r2, #80]
 974 00e2 12FA83F3 		uxtah	r3, r2, r3
 975              	.LVL91:
2071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 976              		.loc 1 2071 7 discriminator 16 view .LVU300
 977 00e6 0344     		add	r3, r3, r0
 978              	.LVL92:
2071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 979              		.loc 1 2071 7 discriminator 16 view .LVU301
 980 00e8 0022     		movs	r2, #0
 981 00ea A3F80224 		strh	r2, [r3, #1026]	@ movhi
 982 00ee BDE7     		b	.L59
 983              	.LVL93:
 984              	.L60:
2071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 985              		.loc 1 2071 7 is_stmt 0 discriminator 16 view .LVU302
 986              	.LBE12:
 987              	.LBB13:
2072:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 988              		.loc 1 2072 7 is_stmt 1 discriminator 2 view .LVU303
 989 00f0 012B     		cmp	r3, #1
 990 00f2 D7D1     		bne	.L61
ARM GAS  /tmp/ccJPteqL.s 			page 58


2072:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 991              		.loc 1 2072 7 discriminator 16 view .LVU304
 992 00f4 B2F85030 		ldrh	r3, [r2, #80]
 993 00f8 12FA83F3 		uxtah	r3, r2, r3
 994              	.LVL94:
2072:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 995              		.loc 1 2072 7 discriminator 16 view .LVU305
 996 00fc 2278     		ldrb	r2, [r4]	@ zero_extendqisi2
 997 00fe 03EBC203 		add	r3, r3, r2, lsl #3
 998              	.LVL95:
2072:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 999              		.loc 1 2072 7 discriminator 16 view .LVU306
 1000 0102 0022     		movs	r2, #0
 1001 0104 A3F80624 		strh	r2, [r3, #1030]	@ movhi
 1002 0108 CCE7     		b	.L61
 1003              	.LVL96:
 1004              	.L57:
2072:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1005              		.loc 1 2072 7 is_stmt 0 discriminator 16 view .LVU307
 1006              	.LBE13:
2084:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
2085:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2086:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     else /* Transfer is not yet Done */
2087:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2088:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* need to Free USB Buff */
2089:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       if ((wEPVal & USB_EP_DTOG_RX) != 0U)
 1007              		.loc 1 2089 7 is_stmt 1 view .LVU308
 1008              		.loc 1 2089 10 is_stmt 0 view .LVU309
 1009 010a 16F4804F 		tst	r6, #16384
 1010 010e 0DD0     		beq	.L63
2090:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
2091:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         PCD_FREE_USER_BUFFER(hpcd->Instance, ep->num, 1U);
 1011              		.loc 1 2091 9 is_stmt 1 discriminator 4 view .LVU310
 1012              		.loc 1 2091 9 discriminator 4 view .LVU311
 1013              		.loc 1 2091 9 discriminator 4 view .LVU312
 1014              		.loc 1 2091 9 discriminator 4 view .LVU313
 1015              	.LBB14:
 1016              		.loc 1 2091 9 discriminator 4 view .LVU314
 1017              		.loc 1 2091 9 discriminator 4 view .LVU315
 1018 0110 2868     		ldr	r0, [r5]
 1019 0112 30F82130 		ldrh	r3, [r0, r1, lsl #2]
 1020 0116 9BB2     		uxth	r3, r3
 1021 0118 23F4E043 		bic	r3, r3, #28672
 1022 011c 23F07003 		bic	r3, r3, #112
 1023              	.LVL97:
 1024              		.loc 1 2091 9 discriminator 4 view .LVU316
 1025 0120 43F44043 		orr	r3, r3, #49152
 1026              	.LVL98:
 1027              		.loc 1 2091 9 is_stmt 0 discriminator 4 view .LVU317
 1028 0124 43F08003 		orr	r3, r3, #128
 1029 0128 20F82130 		strh	r3, [r0, r1, lsl #2]	@ movhi
 1030              	.LVL99:
 1031              	.L63:
 1032              		.loc 1 2091 9 discriminator 4 view .LVU318
 1033              	.LBE14:
 1034              		.loc 1 2091 9 is_stmt 1 discriminator 6 view .LVU319
 1035              		.loc 1 2091 9 discriminator 6 view .LVU320
ARM GAS  /tmp/ccJPteqL.s 			page 59


2092:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
2093:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2094:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* Still there is data to Fill in the next Buffer */
2095:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       if (ep->xfer_fill_db == 1U)
 1036              		.loc 1 2095 7 discriminator 6 view .LVU321
 1037              		.loc 1 2095 13 is_stmt 0 discriminator 6 view .LVU322
 1038 012c 94F82430 		ldrb	r3, [r4, #36]	@ zero_extendqisi2
 1039              		.loc 1 2095 10 discriminator 6 view .LVU323
 1040 0130 012B     		cmp	r3, #1
 1041 0132 12D0     		beq	.L91
 1042              	.LVL100:
 1043              	.L62:
2096:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
2097:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_buff += TxPctSize;
2098:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_count += TxPctSize;
2099:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2100:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Calculate the len of the new buffer to fill */
2101:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         if (ep->xfer_len_db >= ep->maxpacket)
2102:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
2103:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           len = ep->maxpacket;
2104:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len_db -= len;
2105:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
2106:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         else if (ep->xfer_len_db == 0U)
2107:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
2108:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           len = TxPctSize;
2109:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_fill_db = 0U;
2110:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
2111:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         else
2112:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
2113:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_fill_db = 0U;
2114:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           len = ep->xfer_len_db;
2115:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len_db = 0U;
2116:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
2117:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2118:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Write remaining Data to Buffer */
2119:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Set the Double buffer counter for pma buffer1 */
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         PCD_SET_EP_DBUF0_CNT(hpcd->Instance, ep->num, ep->is_in, len);
2121:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2122:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Copy user buffer to USB PMA */
2123:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         USB_WritePMA(hpcd->Instance, ep->xfer_buff,  ep->pmaaddr0, (uint16_t)len);
2124:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
2125:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2126:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
2127:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   else /* Data Buffer1 ACK received */
2128:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
2129:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* multi-packet on the NON control IN endpoint */
2130:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     TxPctSize = (uint16_t)PCD_GET_EP_DBUF1_CNT(hpcd->Instance, ep->num);
2131:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2132:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (ep->xfer_len >= TxPctSize)
2133:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2134:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       ep->xfer_len -= TxPctSize;
2135:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2136:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     else
2137:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2138:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       ep->xfer_len = 0U;
2139:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2140:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 60


2141:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     /* Transfer is completed */
2142:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (ep->xfer_len == 0U)
2143:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF0_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
2146:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2147:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* TX COMPLETE */
2148:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
2149:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->DataInStageCallback(hpcd, ep->num);
2150:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #else
2151:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       HAL_PCD_DataInStageCallback(hpcd, ep->num);
2152:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
2153:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2154:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* need to Free USB Buff */
2155:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       if ((wEPVal & USB_EP_DTOG_RX) == 0U)
2156:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
2157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         PCD_FREE_USER_BUFFER(hpcd->Instance, ep->num, 1U);
2158:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
2159:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2160:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     else /* Transfer is not yet Done */
2161:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
2162:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* need to Free USB Buff */
2163:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       if ((wEPVal & USB_EP_DTOG_RX) == 0U)
2164:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         PCD_FREE_USER_BUFFER(hpcd->Instance, ep->num, 1U);
2166:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
2167:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2168:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       /* Still there is data to Fill in the next Buffer */
2169:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       if (ep->xfer_fill_db == 1U)
2170:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
2171:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_buff += TxPctSize;
2172:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_count += TxPctSize;
2173:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2174:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Calculate the len of the new buffer to fill */
2175:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         if (ep->xfer_len_db >= ep->maxpacket)
2176:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
2177:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           len = ep->maxpacket;
2178:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len_db -= len;
2179:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
2180:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         else if (ep->xfer_len_db == 0U)
2181:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
2182:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           len = TxPctSize;
2183:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_fill_db = 0U;
2184:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
2185:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         else
2186:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
2187:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           len = ep->xfer_len_db;
2188:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len_db = 0U;
2189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_fill_db = 0;
2190:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
2191:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2192:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Set the Double buffer counter for pmabuffer1 */
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, len);
2194:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2195:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         /* Copy the user buffer to USB PMA */
2196:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         USB_WritePMA(hpcd->Instance, ep->xfer_buff,  ep->pmaaddr1, (uint16_t)len);
2197:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
ARM GAS  /tmp/ccJPteqL.s 			page 61


2198:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
2199:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
2200:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2201:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /*enable endpoint IN*/
2202:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_SET_EP_TX_STATUS(hpcd->Instance, ep->num, USB_EP_TX_VALID);
 1044              		.loc 1 2202 3 is_stmt 1 view .LVU324
 1045              	.LBB15:
 1046              		.loc 1 2202 3 view .LVU325
 1047              		.loc 1 2202 3 view .LVU326
 1048 0134 2A68     		ldr	r2, [r5]
 1049 0136 2178     		ldrb	r1, [r4]	@ zero_extendqisi2
 1050 0138 32F82130 		ldrh	r3, [r2, r1, lsl #2]
 1051 013c 9BB2     		uxth	r3, r3
 1052 013e 23F4E043 		bic	r3, r3, #28672
 1053 0142 23F04003 		bic	r3, r3, #64
 1054              	.LVL101:
 1055              		.loc 1 2202 3 view .LVU327
 1056              		.loc 1 2202 3 view .LVU328
 1057              		.loc 1 2202 3 view .LVU329
 1058              		.loc 1 2202 3 view .LVU330
 1059 0146 83F03003 		eor	r3, r3, #48
 1060              	.LVL102:
 1061              		.loc 1 2202 3 view .LVU331
 1062 014a 43F40043 		orr	r3, r3, #32768
 1063              	.LVL103:
 1064              		.loc 1 2202 3 is_stmt 0 view .LVU332
 1065 014e 43F08003 		orr	r3, r3, #128
 1066 0152 22F82130 		strh	r3, [r2, r1, lsl #2]	@ movhi
 1067              	.LBE15:
 1068              		.loc 1 2202 3 is_stmt 1 view .LVU333
2203:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
2204:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
 1069              		.loc 1 2204 3 view .LVU334
2205:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 1070              		.loc 1 2205 1 is_stmt 0 view .LVU335
 1071 0156 0020     		movs	r0, #0
 1072 0158 70BD     		pop	{r4, r5, r6, pc}
 1073              	.LVL104:
 1074              	.L91:
2097:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_count += TxPctSize;
 1075              		.loc 1 2097 9 is_stmt 1 view .LVU336
2097:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_count += TxPctSize;
 1076              		.loc 1 2097 11 is_stmt 0 view .LVU337
 1077 015a 6369     		ldr	r3, [r4, #20]
2097:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_count += TxPctSize;
 1078              		.loc 1 2097 23 view .LVU338
 1079 015c 1344     		add	r3, r3, r2
 1080 015e 6361     		str	r3, [r4, #20]
2098:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1081              		.loc 1 2098 9 is_stmt 1 view .LVU339
2098:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1082              		.loc 1 2098 11 is_stmt 0 view .LVU340
 1083 0160 E369     		ldr	r3, [r4, #28]
2098:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1084              		.loc 1 2098 24 view .LVU341
 1085 0162 1344     		add	r3, r3, r2
 1086 0164 E361     		str	r3, [r4, #28]
ARM GAS  /tmp/ccJPteqL.s 			page 62


2101:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1087              		.loc 1 2101 9 is_stmt 1 view .LVU342
2101:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1088              		.loc 1 2101 15 is_stmt 0 view .LVU343
 1089 0166 216A     		ldr	r1, [r4, #32]
2101:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1090              		.loc 1 2101 34 view .LVU344
 1091 0168 2369     		ldr	r3, [r4, #16]
2101:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1092              		.loc 1 2101 12 view .LVU345
 1093 016a 9942     		cmp	r1, r3
 1094 016c 1BD3     		bcc	.L64
2103:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len_db -= len;
 1095              		.loc 1 2103 11 is_stmt 1 view .LVU346
 1096              	.LVL105:
2104:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1097              		.loc 1 2104 11 view .LVU347
2104:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1098              		.loc 1 2104 27 is_stmt 0 view .LVU348
 1099 016e C91A     		subs	r1, r1, r3
 1100 0170 2162     		str	r1, [r4, #32]
 1101              	.L65:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1102              		.loc 1 2120 9 is_stmt 1 view .LVU349
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1103              		.loc 1 2120 9 view .LVU350
 1104 0172 6278     		ldrb	r2, [r4, #1]	@ zero_extendqisi2
 1105              	.LVL106:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1106              		.loc 1 2120 9 is_stmt 0 view .LVU351
 1107 0174 002A     		cmp	r2, #0
 1108 0176 3FD1     		bne	.L67
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1109              		.loc 1 2120 9 is_stmt 1 discriminator 1 view .LVU352
 1110              	.LBB16:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1111              		.loc 1 2120 9 discriminator 1 view .LVU353
 1112 0178 2968     		ldr	r1, [r5]
 1113              	.LVL107:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1114              		.loc 1 2120 9 discriminator 1 view .LVU354
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1115              		.loc 1 2120 9 discriminator 1 view .LVU355
 1116 017a B1F85020 		ldrh	r2, [r1, #80]
 1117 017e 11FA82F2 		uxtah	r2, r1, r2
 1118              	.LVL108:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1119              		.loc 1 2120 9 discriminator 1 view .LVU356
 1120 0182 2178     		ldrb	r1, [r4]	@ zero_extendqisi2
 1121 0184 02EBC102 		add	r2, r2, r1, lsl #3
 1122              	.LVL109:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1123              		.loc 1 2120 9 discriminator 1 view .LVU357
 1124              	.LBB17:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1125              		.loc 1 2120 9 discriminator 1 view .LVU358
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 63


 1126              		.loc 1 2120 9 discriminator 1 view .LVU359
 1127 0188 3E2B     		cmp	r3, #62
 1128 018a 18D9     		bls	.L68
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1129              		.loc 1 2120 9 discriminator 3 view .LVU360
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1130              		.loc 1 2120 9 discriminator 3 view .LVU361
 1131 018c 5909     		lsrs	r1, r3, #5
 1132              	.LVL110:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1133              		.loc 1 2120 9 discriminator 3 view .LVU362
 1134 018e 13F01F0F 		tst	r3, #31
 1135 0192 00D1     		bne	.L69
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1136              		.loc 1 2120 9 discriminator 5 view .LVU363
 1137 0194 0139     		subs	r1, r1, #1
 1138              	.LVL111:
 1139              	.L69:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1140              		.loc 1 2120 9 discriminator 7 view .LVU364
 1141 0196 6FEAC161 		mvn	r1, r1, lsl #27
 1142              	.LVL112:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1143              		.loc 1 2120 9 is_stmt 0 discriminator 7 view .LVU365
 1144 019a 6FEA5141 		mvn	r1, r1, lsr #17
 1145 019e 89B2     		uxth	r1, r1
 1146 01a0 A2F80214 		strh	r1, [r2, #1026]	@ movhi
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1147              		.loc 1 2120 9 is_stmt 1 discriminator 7 view .LVU366
 1148 01a4 2AE0     		b	.L70
 1149              	.LVL113:
 1150              	.L64:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1151              		.loc 1 2120 9 is_stmt 0 discriminator 7 view .LVU367
 1152              	.LBE17:
 1153              	.LBE16:
2106:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1154              		.loc 1 2106 14 is_stmt 1 view .LVU368
2106:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1155              		.loc 1 2106 17 is_stmt 0 view .LVU369
 1156 01a6 21B9     		cbnz	r1, .L66
2108:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_fill_db = 0U;
 1157              		.loc 1 2108 11 is_stmt 1 view .LVU370
 1158              	.LVL114:
2109:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1159              		.loc 1 2109 11 view .LVU371
2109:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1160              		.loc 1 2109 28 is_stmt 0 view .LVU372
 1161 01a8 0023     		movs	r3, #0
 1162 01aa 84F82430 		strb	r3, [r4, #36]
2108:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_fill_db = 0U;
 1163              		.loc 1 2108 15 view .LVU373
 1164 01ae 1346     		mov	r3, r2
 1165 01b0 DFE7     		b	.L65
 1166              	.LVL115:
 1167              	.L66:
2113:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           len = ep->xfer_len_db;
ARM GAS  /tmp/ccJPteqL.s 			page 64


 1168              		.loc 1 2113 11 is_stmt 1 view .LVU374
2113:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           len = ep->xfer_len_db;
 1169              		.loc 1 2113 28 is_stmt 0 view .LVU375
 1170 01b2 0023     		movs	r3, #0
 1171 01b4 84F82430 		strb	r3, [r4, #36]
2114:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len_db = 0U;
 1172              		.loc 1 2114 11 is_stmt 1 view .LVU376
 1173              	.LVL116:
2115:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1174              		.loc 1 2115 11 view .LVU377
2115:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1175              		.loc 1 2115 27 is_stmt 0 view .LVU378
 1176 01b8 2362     		str	r3, [r4, #32]
2114:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len_db = 0U;
 1177              		.loc 1 2114 15 view .LVU379
 1178 01ba 0B46     		mov	r3, r1
 1179 01bc D9E7     		b	.L65
 1180              	.LVL117:
 1181              	.L68:
 1182              	.LBB19:
 1183              	.LBB18:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1184              		.loc 1 2120 9 is_stmt 1 discriminator 4 view .LVU380
 1185 01be 8BB9     		cbnz	r3, .L71
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1186              		.loc 1 2120 9 discriminator 9 view .LVU381
 1187 01c0 B2F80214 		ldrh	r1, [r2, #1026]
 1188 01c4 89B2     		uxth	r1, r1
 1189 01c6 21F4F841 		bic	r1, r1, #31744
 1190 01ca 89B2     		uxth	r1, r1
 1191 01cc A2F80214 		strh	r1, [r2, #1026]	@ movhi
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1192              		.loc 1 2120 9 discriminator 9 view .LVU382
 1193 01d0 B2F80214 		ldrh	r1, [r2, #1026]
 1194 01d4 6FEA4141 		mvn	r1, r1, lsl #17
 1195 01d8 6FEA5141 		mvn	r1, r1, lsr #17
 1196 01dc 89B2     		uxth	r1, r1
 1197 01de A2F80214 		strh	r1, [r2, #1026]	@ movhi
 1198 01e2 0BE0     		b	.L70
 1199              	.L71:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1200              		.loc 1 2120 9 discriminator 10 view .LVU383
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1201              		.loc 1 2120 9 discriminator 10 view .LVU384
 1202 01e4 5908     		lsrs	r1, r3, #1
 1203              	.LVL118:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1204              		.loc 1 2120 9 discriminator 10 view .LVU385
 1205 01e6 13F0010F 		tst	r3, #1
 1206 01ea 00D0     		beq	.L72
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1207              		.loc 1 2120 9 discriminator 12 view .LVU386
 1208 01ec 0131     		adds	r1, r1, #1
 1209              	.LVL119:
 1210              	.L72:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1211              		.loc 1 2120 9 discriminator 14 view .LVU387
ARM GAS  /tmp/ccJPteqL.s 			page 65


 1212 01ee 8902     		lsls	r1, r1, #10
 1213              	.LVL120:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1214              		.loc 1 2120 9 is_stmt 0 discriminator 14 view .LVU388
 1215 01f0 89B2     		uxth	r1, r1
 1216 01f2 A2F80214 		strh	r1, [r2, #1026]	@ movhi
 1217 01f6 01E0     		b	.L70
 1218              	.LVL121:
 1219              	.L67:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1220              		.loc 1 2120 9 discriminator 14 view .LVU389
 1221              	.LBE18:
 1222              	.LBE19:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1223              		.loc 1 2120 9 is_stmt 1 discriminator 2 view .LVU390
 1224 01f8 012A     		cmp	r2, #1
 1225 01fa 06D0     		beq	.L92
 1226              	.L70:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1227              		.loc 1 2120 9 discriminator 18 view .LVU391
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1228              		.loc 1 2120 9 discriminator 18 view .LVU392
2123:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1229              		.loc 1 2123 9 discriminator 18 view .LVU393
 1230 01fc 9BB2     		uxth	r3, r3
 1231              	.LVL122:
2123:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1232              		.loc 1 2123 9 is_stmt 0 discriminator 18 view .LVU394
 1233 01fe 2289     		ldrh	r2, [r4, #8]
 1234 0200 6169     		ldr	r1, [r4, #20]
 1235 0202 2868     		ldr	r0, [r5]
 1236 0204 FFF7FEFF 		bl	USB_WritePMA
 1237              	.LVL123:
 1238 0208 94E7     		b	.L62
 1239              	.LVL124:
 1240              	.L92:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1241              		.loc 1 2120 9 is_stmt 1 discriminator 16 view .LVU395
 1242              	.LBB20:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1243              		.loc 1 2120 9 discriminator 16 view .LVU396
 1244 020a 2968     		ldr	r1, [r5]
 1245              	.LVL125:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1246              		.loc 1 2120 9 discriminator 16 view .LVU397
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1247              		.loc 1 2120 9 discriminator 16 view .LVU398
 1248 020c B1F85020 		ldrh	r2, [r1, #80]
 1249 0210 11FA82F2 		uxtah	r2, r1, r2
 1250              	.LVL126:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1251              		.loc 1 2120 9 discriminator 16 view .LVU399
 1252 0214 2178     		ldrb	r1, [r4]	@ zero_extendqisi2
 1253 0216 02EBC102 		add	r2, r2, r1, lsl #3
 1254              	.LVL127:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1255              		.loc 1 2120 9 discriminator 16 view .LVU400
ARM GAS  /tmp/ccJPteqL.s 			page 66


 1256 021a 99B2     		uxth	r1, r3
 1257 021c A2F80214 		strh	r1, [r2, #1026]	@ movhi
 1258 0220 ECE7     		b	.L70
 1259              	.LVL128:
 1260              	.L54:
2120:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1261              		.loc 1 2120 9 is_stmt 0 discriminator 16 view .LVU401
 1262              	.LBE20:
2130:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1263              		.loc 1 2130 5 is_stmt 1 view .LVU402
2130:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1264              		.loc 1 2130 27 is_stmt 0 view .LVU403
 1265 0222 0268     		ldr	r2, [r0]
 1266              	.LVL129:
2130:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1267              		.loc 1 2130 27 view .LVU404
 1268 0224 B2F85030 		ldrh	r3, [r2, #80]
 1269 0228 0978     		ldrb	r1, [r1]	@ zero_extendqisi2
 1270              	.LVL130:
2130:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1271              		.loc 1 2130 27 view .LVU405
 1272 022a C800     		lsls	r0, r1, #3
 1273              	.LVL131:
2130:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1274              		.loc 1 2130 27 view .LVU406
 1275 022c 10FA83F3 		uxtah	r3, r0, r3
 1276 0230 1344     		add	r3, r3, r2
 1277 0232 B3F80624 		ldrh	r2, [r3, #1030]
2130:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1278              		.loc 1 2130 15 view .LVU407
 1279 0236 C2F30902 		ubfx	r2, r2, #0, #10
 1280              	.LVL132:
2132:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 1281              		.loc 1 2132 5 is_stmt 1 view .LVU408
2132:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 1282              		.loc 1 2132 11 is_stmt 0 view .LVU409
 1283 023a A369     		ldr	r3, [r4, #24]
2132:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 1284              		.loc 1 2132 8 view .LVU410
 1285 023c 9342     		cmp	r3, r2
 1286 023e 52D3     		bcc	.L73
2134:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 1287              		.loc 1 2134 7 is_stmt 1 view .LVU411
2134:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 1288              		.loc 1 2134 20 is_stmt 0 view .LVU412
 1289 0240 9B1A     		subs	r3, r3, r2
 1290 0242 A361     		str	r3, [r4, #24]
 1291              	.L74:
2142:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 1292              		.loc 1 2142 5 is_stmt 1 view .LVU413
2142:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 1293              		.loc 1 2142 11 is_stmt 0 view .LVU414
 1294 0244 A369     		ldr	r3, [r4, #24]
2142:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 1295              		.loc 1 2142 8 view .LVU415
 1296 0246 002B     		cmp	r3, #0
 1297 0248 69D1     		bne	.L75
ARM GAS  /tmp/ccJPteqL.s 			page 67


2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1298              		.loc 1 2144 7 is_stmt 1 view .LVU416
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1299              		.loc 1 2144 7 view .LVU417
 1300 024a 6378     		ldrb	r3, [r4, #1]	@ zero_extendqisi2
 1301 024c 002B     		cmp	r3, #0
 1302 024e 4DD1     		bne	.L76
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1303              		.loc 1 2144 7 discriminator 1 view .LVU418
 1304              	.LBB21:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1305              		.loc 1 2144 7 discriminator 1 view .LVU419
 1306 0250 2A68     		ldr	r2, [r5]
 1307              	.LVL133:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1308              		.loc 1 2144 7 discriminator 1 view .LVU420
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1309              		.loc 1 2144 7 discriminator 1 view .LVU421
 1310 0252 B2F85030 		ldrh	r3, [r2, #80]
 1311 0256 12FA83F3 		uxtah	r3, r2, r3
 1312              	.LVL134:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1313              		.loc 1 2144 7 discriminator 1 view .LVU422
 1314 025a 0344     		add	r3, r3, r0
 1315              	.LVL135:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1316              		.loc 1 2144 7 discriminator 1 view .LVU423
 1317              	.LBB22:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1318              		.loc 1 2144 7 discriminator 1 view .LVU424
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1319              		.loc 1 2144 7 discriminator 1 view .LVU425
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1320              		.loc 1 2144 7 discriminator 1 view .LVU426
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1321              		.loc 1 2144 7 discriminator 1 view .LVU427
 1322 025c B3F80224 		ldrh	r2, [r3, #1026]
 1323 0260 92B2     		uxth	r2, r2
 1324 0262 22F4F842 		bic	r2, r2, #31744
 1325 0266 92B2     		uxth	r2, r2
 1326 0268 A3F80224 		strh	r2, [r3, #1026]	@ movhi
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1327              		.loc 1 2144 7 discriminator 1 view .LVU428
 1328 026c B3F80224 		ldrh	r2, [r3, #1026]
 1329 0270 6FEA4242 		mvn	r2, r2, lsl #17
 1330 0274 6FEA5242 		mvn	r2, r2, lsr #17
 1331 0278 92B2     		uxth	r2, r2
 1332 027a A3F80224 		strh	r2, [r3, #1026]	@ movhi
 1333              	.LVL136:
 1334              	.L77:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1335              		.loc 1 2144 7 is_stmt 0 discriminator 1 view .LVU429
 1336              	.LBE22:
 1337              	.LBE21:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1338              		.loc 1 2144 7 is_stmt 1 discriminator 18 view .LVU430
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
ARM GAS  /tmp/ccJPteqL.s 			page 68


 1339              		.loc 1 2144 7 discriminator 18 view .LVU431
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1340              		.loc 1 2145 7 discriminator 18 view .LVU432
 1341              	.LBB23:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1342              		.loc 1 2145 7 discriminator 18 view .LVU433
 1343 027e 2A68     		ldr	r2, [r5]
 1344              	.LVL137:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1345              		.loc 1 2145 7 discriminator 18 view .LVU434
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1346              		.loc 1 2145 7 discriminator 18 view .LVU435
 1347 0280 6378     		ldrb	r3, [r4, #1]	@ zero_extendqisi2
 1348 0282 002B     		cmp	r3, #0
 1349 0284 3ED1     		bne	.L78
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1350              		.loc 1 2145 7 discriminator 1 view .LVU436
 1351              	.LBB24:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1352              		.loc 1 2145 7 discriminator 1 view .LVU437
 1353              	.LVL138:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1354              		.loc 1 2145 7 discriminator 1 view .LVU438
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1355              		.loc 1 2145 7 discriminator 1 view .LVU439
 1356 0286 B2F85030 		ldrh	r3, [r2, #80]
 1357 028a 12FA83F3 		uxtah	r3, r2, r3
 1358              	.LVL139:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1359              		.loc 1 2145 7 discriminator 1 view .LVU440
 1360 028e 2278     		ldrb	r2, [r4]	@ zero_extendqisi2
 1361              	.LVL140:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1362              		.loc 1 2145 7 is_stmt 0 discriminator 1 view .LVU441
 1363 0290 03EBC203 		add	r3, r3, r2, lsl #3
 1364              	.LVL141:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1365              		.loc 1 2145 7 is_stmt 1 discriminator 1 view .LVU442
 1366              	.LBB25:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1367              		.loc 1 2145 7 discriminator 1 view .LVU443
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1368              		.loc 1 2145 7 discriminator 1 view .LVU444
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1369              		.loc 1 2145 7 discriminator 1 view .LVU445
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1370              		.loc 1 2145 7 discriminator 1 view .LVU446
 1371 0294 B3F80624 		ldrh	r2, [r3, #1030]
 1372 0298 92B2     		uxth	r2, r2
 1373 029a 22F4F842 		bic	r2, r2, #31744
 1374 029e 92B2     		uxth	r2, r2
 1375 02a0 A3F80624 		strh	r2, [r3, #1030]	@ movhi
 1376              	.LVL142:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1377              		.loc 1 2145 7 discriminator 1 view .LVU447
 1378 02a4 B3F80624 		ldrh	r2, [r3, #1030]
 1379 02a8 6FEA4242 		mvn	r2, r2, lsl #17
ARM GAS  /tmp/ccJPteqL.s 			page 69


 1380 02ac 6FEA5242 		mvn	r2, r2, lsr #17
 1381 02b0 92B2     		uxth	r2, r2
 1382 02b2 A3F80624 		strh	r2, [r3, #1030]	@ movhi
 1383              	.LVL143:
 1384              	.L79:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1385              		.loc 1 2145 7 is_stmt 0 discriminator 1 view .LVU448
 1386              	.LBE25:
 1387              	.LBE24:
 1388              	.LBE23:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1389              		.loc 1 2145 7 is_stmt 1 discriminator 18 view .LVU449
2151:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 1390              		.loc 1 2151 7 discriminator 18 view .LVU450
 1391 02b6 2178     		ldrb	r1, [r4]	@ zero_extendqisi2
 1392 02b8 2846     		mov	r0, r5
 1393 02ba FFF7FEFF 		bl	HAL_PCD_DataInStageCallback
 1394              	.LVL144:
2155:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 1395              		.loc 1 2155 7 discriminator 18 view .LVU451
2155:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 1396              		.loc 1 2155 10 is_stmt 0 discriminator 18 view .LVU452
 1397 02be 16F4804F 		tst	r6, #16384
 1398 02c2 7FF437AF 		bne	.L62
2157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1399              		.loc 1 2157 9 is_stmt 1 discriminator 4 view .LVU453
2157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1400              		.loc 1 2157 9 discriminator 4 view .LVU454
2157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1401              		.loc 1 2157 9 discriminator 4 view .LVU455
2157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1402              		.loc 1 2157 9 discriminator 4 view .LVU456
 1403              	.LBB26:
2157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1404              		.loc 1 2157 9 discriminator 4 view .LVU457
2157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1405              		.loc 1 2157 9 discriminator 4 view .LVU458
 1406 02c6 2A68     		ldr	r2, [r5]
 1407 02c8 2178     		ldrb	r1, [r4]	@ zero_extendqisi2
 1408 02ca 32F82130 		ldrh	r3, [r2, r1, lsl #2]
 1409 02ce 9BB2     		uxth	r3, r3
 1410 02d0 23F4E043 		bic	r3, r3, #28672
 1411 02d4 23F07003 		bic	r3, r3, #112
 1412              	.LVL145:
2157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1413              		.loc 1 2157 9 discriminator 4 view .LVU459
 1414 02d8 43F44043 		orr	r3, r3, #49152
 1415              	.LVL146:
2157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1416              		.loc 1 2157 9 is_stmt 0 discriminator 4 view .LVU460
 1417 02dc 43F08003 		orr	r3, r3, #128
 1418 02e0 22F82130 		strh	r3, [r2, r1, lsl #2]	@ movhi
 1419 02e4 26E7     		b	.L62
 1420              	.LVL147:
 1421              	.L73:
2157:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1422              		.loc 1 2157 9 discriminator 4 view .LVU461
ARM GAS  /tmp/ccJPteqL.s 			page 70


 1423              	.LBE26:
2138:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 1424              		.loc 1 2138 7 is_stmt 1 view .LVU462
2138:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     }
 1425              		.loc 1 2138 20 is_stmt 0 view .LVU463
 1426 02e6 0023     		movs	r3, #0
 1427 02e8 A361     		str	r3, [r4, #24]
 1428 02ea ABE7     		b	.L74
 1429              	.L76:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1430              		.loc 1 2144 7 is_stmt 1 discriminator 2 view .LVU464
 1431 02ec 012B     		cmp	r3, #1
 1432 02ee C6D1     		bne	.L77
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1433              		.loc 1 2144 7 discriminator 16 view .LVU465
 1434              	.LBB27:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1435              		.loc 1 2144 7 discriminator 16 view .LVU466
 1436 02f0 2A68     		ldr	r2, [r5]
 1437              	.LVL148:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1438              		.loc 1 2144 7 discriminator 16 view .LVU467
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1439              		.loc 1 2144 7 discriminator 16 view .LVU468
 1440 02f2 B2F85030 		ldrh	r3, [r2, #80]
 1441 02f6 12FA83F3 		uxtah	r3, r2, r3
 1442              	.LVL149:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1443              		.loc 1 2144 7 discriminator 16 view .LVU469
 1444 02fa 0344     		add	r3, r3, r0
 1445              	.LVL150:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1446              		.loc 1 2144 7 discriminator 16 view .LVU470
 1447 02fc 0022     		movs	r2, #0
 1448 02fe A3F80224 		strh	r2, [r3, #1026]	@ movhi
 1449 0302 BCE7     		b	.L77
 1450              	.LVL151:
 1451              	.L78:
2144:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       PCD_SET_EP_DBUF1_CNT(hpcd->Instance, ep->num, ep->is_in, 0U);
 1452              		.loc 1 2144 7 is_stmt 0 discriminator 16 view .LVU471
 1453              	.LBE27:
 1454              	.LBB28:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1455              		.loc 1 2145 7 is_stmt 1 discriminator 2 view .LVU472
 1456 0304 012B     		cmp	r3, #1
 1457 0306 D6D1     		bne	.L79
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1458              		.loc 1 2145 7 discriminator 16 view .LVU473
 1459 0308 B2F85030 		ldrh	r3, [r2, #80]
 1460 030c 12FA83F3 		uxtah	r3, r2, r3
 1461              	.LVL152:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1462              		.loc 1 2145 7 discriminator 16 view .LVU474
 1463 0310 2278     		ldrb	r2, [r4]	@ zero_extendqisi2
 1464 0312 03EBC203 		add	r3, r3, r2, lsl #3
 1465              	.LVL153:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 71


 1466              		.loc 1 2145 7 discriminator 16 view .LVU475
 1467 0316 0022     		movs	r2, #0
 1468 0318 A3F80624 		strh	r2, [r3, #1030]	@ movhi
 1469 031c CBE7     		b	.L79
 1470              	.LVL154:
 1471              	.L75:
2145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1472              		.loc 1 2145 7 is_stmt 0 discriminator 16 view .LVU476
 1473              	.LBE28:
2163:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 1474              		.loc 1 2163 7 is_stmt 1 view .LVU477
2163:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 1475              		.loc 1 2163 10 is_stmt 0 view .LVU478
 1476 031e 16F4804F 		tst	r6, #16384
 1477 0322 0DD1     		bne	.L80
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1478              		.loc 1 2165 9 is_stmt 1 discriminator 4 view .LVU479
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1479              		.loc 1 2165 9 discriminator 4 view .LVU480
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1480              		.loc 1 2165 9 discriminator 4 view .LVU481
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1481              		.loc 1 2165 9 discriminator 4 view .LVU482
 1482              	.LBB29:
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1483              		.loc 1 2165 9 discriminator 4 view .LVU483
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1484              		.loc 1 2165 9 discriminator 4 view .LVU484
 1485 0324 2868     		ldr	r0, [r5]
 1486 0326 30F82130 		ldrh	r3, [r0, r1, lsl #2]
 1487 032a 9BB2     		uxth	r3, r3
 1488 032c 23F4E043 		bic	r3, r3, #28672
 1489 0330 23F07003 		bic	r3, r3, #112
 1490              	.LVL155:
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1491              		.loc 1 2165 9 discriminator 4 view .LVU485
 1492 0334 43F44043 		orr	r3, r3, #49152
 1493              	.LVL156:
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1494              		.loc 1 2165 9 is_stmt 0 discriminator 4 view .LVU486
 1495 0338 43F08003 		orr	r3, r3, #128
 1496 033c 20F82130 		strh	r3, [r0, r1, lsl #2]	@ movhi
 1497              	.LVL157:
 1498              	.L80:
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1499              		.loc 1 2165 9 discriminator 4 view .LVU487
 1500              	.LBE29:
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1501              		.loc 1 2165 9 is_stmt 1 discriminator 6 view .LVU488
2165:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1502              		.loc 1 2165 9 discriminator 6 view .LVU489
2169:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 1503              		.loc 1 2169 7 discriminator 6 view .LVU490
2169:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 1504              		.loc 1 2169 13 is_stmt 0 discriminator 6 view .LVU491
 1505 0340 94F82430 		ldrb	r3, [r4, #36]	@ zero_extendqisi2
2169:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
ARM GAS  /tmp/ccJPteqL.s 			page 72


 1506              		.loc 1 2169 10 discriminator 6 view .LVU492
 1507 0344 012B     		cmp	r3, #1
 1508 0346 7FF4F5AE 		bne	.L62
2171:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_count += TxPctSize;
 1509              		.loc 1 2171 9 is_stmt 1 view .LVU493
2171:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_count += TxPctSize;
 1510              		.loc 1 2171 11 is_stmt 0 view .LVU494
 1511 034a 6369     		ldr	r3, [r4, #20]
2171:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_count += TxPctSize;
 1512              		.loc 1 2171 23 view .LVU495
 1513 034c 1344     		add	r3, r3, r2
 1514 034e 6361     		str	r3, [r4, #20]
2172:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1515              		.loc 1 2172 9 is_stmt 1 view .LVU496
2172:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1516              		.loc 1 2172 11 is_stmt 0 view .LVU497
 1517 0350 E369     		ldr	r3, [r4, #28]
2172:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1518              		.loc 1 2172 24 view .LVU498
 1519 0352 1344     		add	r3, r3, r2
 1520 0354 E361     		str	r3, [r4, #28]
2175:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1521              		.loc 1 2175 9 is_stmt 1 view .LVU499
2175:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1522              		.loc 1 2175 15 is_stmt 0 view .LVU500
 1523 0356 216A     		ldr	r1, [r4, #32]
2175:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1524              		.loc 1 2175 34 view .LVU501
 1525 0358 2369     		ldr	r3, [r4, #16]
2175:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1526              		.loc 1 2175 12 view .LVU502
 1527 035a 9942     		cmp	r1, r3
 1528 035c 1BD3     		bcc	.L81
2177:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len_db -= len;
 1529              		.loc 1 2177 11 is_stmt 1 view .LVU503
 1530              	.LVL158:
2178:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1531              		.loc 1 2178 11 view .LVU504
2178:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1532              		.loc 1 2178 27 is_stmt 0 view .LVU505
 1533 035e C91A     		subs	r1, r1, r3
 1534 0360 2162     		str	r1, [r4, #32]
 1535              	.L82:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1536              		.loc 1 2193 9 is_stmt 1 view .LVU506
 1537              	.LBB30:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1538              		.loc 1 2193 9 view .LVU507
 1539 0362 2968     		ldr	r1, [r5]
 1540              	.LVL159:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1541              		.loc 1 2193 9 view .LVU508
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1542              		.loc 1 2193 9 view .LVU509
 1543 0364 6278     		ldrb	r2, [r4, #1]	@ zero_extendqisi2
 1544              	.LVL160:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 73


 1545              		.loc 1 2193 9 is_stmt 0 view .LVU510
 1546 0366 002A     		cmp	r2, #0
 1547 0368 3ED1     		bne	.L84
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1548              		.loc 1 2193 9 is_stmt 1 discriminator 1 view .LVU511
 1549              	.LBB31:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1550              		.loc 1 2193 9 discriminator 1 view .LVU512
 1551              	.LVL161:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1552              		.loc 1 2193 9 discriminator 1 view .LVU513
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1553              		.loc 1 2193 9 discriminator 1 view .LVU514
 1554 036a B1F85020 		ldrh	r2, [r1, #80]
 1555 036e 11FA82F2 		uxtah	r2, r1, r2
 1556              	.LVL162:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1557              		.loc 1 2193 9 discriminator 1 view .LVU515
 1558 0372 2178     		ldrb	r1, [r4]	@ zero_extendqisi2
 1559              	.LVL163:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1560              		.loc 1 2193 9 is_stmt 0 discriminator 1 view .LVU516
 1561 0374 02EBC102 		add	r2, r2, r1, lsl #3
 1562              	.LVL164:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1563              		.loc 1 2193 9 is_stmt 1 discriminator 1 view .LVU517
 1564              	.LBB32:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1565              		.loc 1 2193 9 discriminator 1 view .LVU518
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1566              		.loc 1 2193 9 discriminator 1 view .LVU519
 1567 0378 3E2B     		cmp	r3, #62
 1568 037a 18D9     		bls	.L85
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1569              		.loc 1 2193 9 discriminator 3 view .LVU520
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1570              		.loc 1 2193 9 discriminator 3 view .LVU521
 1571 037c 5909     		lsrs	r1, r3, #5
 1572              	.LVL165:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1573              		.loc 1 2193 9 discriminator 3 view .LVU522
 1574 037e 13F01F0F 		tst	r3, #31
 1575 0382 00D1     		bne	.L86
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1576              		.loc 1 2193 9 discriminator 5 view .LVU523
 1577 0384 0139     		subs	r1, r1, #1
 1578              	.LVL166:
 1579              	.L86:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1580              		.loc 1 2193 9 discriminator 7 view .LVU524
 1581 0386 6FEAC161 		mvn	r1, r1, lsl #27
 1582              	.LVL167:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1583              		.loc 1 2193 9 is_stmt 0 discriminator 7 view .LVU525
 1584 038a 6FEA5141 		mvn	r1, r1, lsr #17
 1585 038e 89B2     		uxth	r1, r1
 1586 0390 A2F80614 		strh	r1, [r2, #1030]	@ movhi
ARM GAS  /tmp/ccJPteqL.s 			page 74


 1587              	.LVL168:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1588              		.loc 1 2193 9 is_stmt 1 discriminator 7 view .LVU526
 1589 0394 2AE0     		b	.L87
 1590              	.LVL169:
 1591              	.L81:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1592              		.loc 1 2193 9 is_stmt 0 discriminator 7 view .LVU527
 1593              	.LBE32:
 1594              	.LBE31:
 1595              	.LBE30:
2180:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1596              		.loc 1 2180 14 is_stmt 1 view .LVU528
2180:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1597              		.loc 1 2180 17 is_stmt 0 view .LVU529
 1598 0396 21B9     		cbnz	r1, .L83
2182:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_fill_db = 0U;
 1599              		.loc 1 2182 11 is_stmt 1 view .LVU530
 1600              	.LVL170:
2183:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1601              		.loc 1 2183 11 view .LVU531
2183:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1602              		.loc 1 2183 28 is_stmt 0 view .LVU532
 1603 0398 0023     		movs	r3, #0
 1604 039a 84F82430 		strb	r3, [r4, #36]
2182:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_fill_db = 0U;
 1605              		.loc 1 2182 15 view .LVU533
 1606 039e 1346     		mov	r3, r2
 1607 03a0 DFE7     		b	.L82
 1608              	.LVL171:
 1609              	.L83:
2187:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len_db = 0U;
 1610              		.loc 1 2187 11 is_stmt 1 view .LVU534
2188:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_fill_db = 0;
 1611              		.loc 1 2188 11 view .LVU535
2188:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_fill_db = 0;
 1612              		.loc 1 2188 27 is_stmt 0 view .LVU536
 1613 03a2 0023     		movs	r3, #0
 1614 03a4 2362     		str	r3, [r4, #32]
2189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1615              		.loc 1 2189 11 is_stmt 1 view .LVU537
2189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1616              		.loc 1 2189 28 is_stmt 0 view .LVU538
 1617 03a6 84F82430 		strb	r3, [r4, #36]
2187:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           ep->xfer_len_db = 0U;
 1618              		.loc 1 2187 15 view .LVU539
 1619 03aa 0B46     		mov	r3, r1
 1620 03ac D9E7     		b	.L82
 1621              	.LVL172:
 1622              	.L85:
 1623              	.LBB35:
 1624              	.LBB34:
 1625              	.LBB33:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1626              		.loc 1 2193 9 is_stmt 1 discriminator 4 view .LVU540
 1627 03ae 8BB9     		cbnz	r3, .L88
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 75


 1628              		.loc 1 2193 9 discriminator 9 view .LVU541
 1629 03b0 B2F80614 		ldrh	r1, [r2, #1030]
 1630 03b4 89B2     		uxth	r1, r1
 1631 03b6 21F4F841 		bic	r1, r1, #31744
 1632 03ba 89B2     		uxth	r1, r1
 1633 03bc A2F80614 		strh	r1, [r2, #1030]	@ movhi
 1634              	.LVL173:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1635              		.loc 1 2193 9 discriminator 9 view .LVU542
 1636 03c0 B2F80614 		ldrh	r1, [r2, #1030]
 1637 03c4 6FEA4141 		mvn	r1, r1, lsl #17
 1638 03c8 6FEA5141 		mvn	r1, r1, lsr #17
 1639 03cc 89B2     		uxth	r1, r1
 1640 03ce A2F80614 		strh	r1, [r2, #1030]	@ movhi
 1641 03d2 0BE0     		b	.L87
 1642              	.LVL174:
 1643              	.L88:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1644              		.loc 1 2193 9 discriminator 10 view .LVU543
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1645              		.loc 1 2193 9 discriminator 10 view .LVU544
 1646 03d4 5908     		lsrs	r1, r3, #1
 1647              	.LVL175:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1648              		.loc 1 2193 9 discriminator 10 view .LVU545
 1649 03d6 13F0010F 		tst	r3, #1
 1650 03da 00D0     		beq	.L89
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1651              		.loc 1 2193 9 discriminator 12 view .LVU546
 1652 03dc 0131     		adds	r1, r1, #1
 1653              	.LVL176:
 1654              	.L89:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1655              		.loc 1 2193 9 discriminator 14 view .LVU547
 1656 03de 8902     		lsls	r1, r1, #10
 1657              	.LVL177:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1658              		.loc 1 2193 9 is_stmt 0 discriminator 14 view .LVU548
 1659 03e0 89B2     		uxth	r1, r1
 1660 03e2 A2F80614 		strh	r1, [r2, #1030]	@ movhi
 1661              	.LVL178:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1662              		.loc 1 2193 9 discriminator 14 view .LVU549
 1663 03e6 01E0     		b	.L87
 1664              	.LVL179:
 1665              	.L84:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1666              		.loc 1 2193 9 discriminator 14 view .LVU550
 1667              	.LBE33:
 1668              	.LBE34:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1669              		.loc 1 2193 9 is_stmt 1 discriminator 2 view .LVU551
 1670 03e8 012A     		cmp	r2, #1
 1671 03ea 06D0     		beq	.L93
 1672              	.LVL180:
 1673              	.L87:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 76


 1674              		.loc 1 2193 9 is_stmt 0 discriminator 2 view .LVU552
 1675              	.LBE35:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1676              		.loc 1 2193 9 is_stmt 1 discriminator 18 view .LVU553
2196:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1677              		.loc 1 2196 9 discriminator 18 view .LVU554
 1678 03ec 9BB2     		uxth	r3, r3
 1679              	.LVL181:
2196:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       }
 1680              		.loc 1 2196 9 is_stmt 0 discriminator 18 view .LVU555
 1681 03ee 6289     		ldrh	r2, [r4, #10]
 1682 03f0 6169     		ldr	r1, [r4, #20]
 1683 03f2 2868     		ldr	r0, [r5]
 1684 03f4 FFF7FEFF 		bl	USB_WritePMA
 1685              	.LVL182:
 1686 03f8 9CE6     		b	.L62
 1687              	.LVL183:
 1688              	.L93:
 1689              	.LBB36:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1690              		.loc 1 2193 9 is_stmt 1 discriminator 16 view .LVU556
 1691 03fa B1F85020 		ldrh	r2, [r1, #80]
 1692 03fe 11FA82F2 		uxtah	r2, r1, r2
 1693              	.LVL184:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1694              		.loc 1 2193 9 discriminator 16 view .LVU557
 1695 0402 2178     		ldrb	r1, [r4]	@ zero_extendqisi2
 1696 0404 02EBC102 		add	r2, r2, r1, lsl #3
 1697              	.LVL185:
2193:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1698              		.loc 1 2193 9 discriminator 16 view .LVU558
 1699 0408 99B2     		uxth	r1, r3
 1700 040a A2F80614 		strh	r1, [r2, #1030]	@ movhi
 1701 040e EDE7     		b	.L87
 1702              	.LBE36:
 1703              		.cfi_endproc
 1704              	.LFE363:
 1706              		.section	.text.HAL_PCD_SetupStageCallback,"ax",%progbits
 1707              		.align	1
 1708              		.weak	HAL_PCD_SetupStageCallback
 1709              		.syntax unified
 1710              		.thumb
 1711              		.thumb_func
 1713              	HAL_PCD_SetupStageCallback:
 1714              	.LVL186:
 1715              	.LFB338:
1187:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 1716              		.loc 1 1187 1 view -0
 1717              		.cfi_startproc
 1718              		@ args = 0, pretend = 0, frame = 0
 1719              		@ frame_needed = 0, uses_anonymous_args = 0
 1720              		@ link register save eliminated.
1189:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1721              		.loc 1 1189 3 view .LVU560
1194:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1722              		.loc 1 1194 1 is_stmt 0 view .LVU561
 1723 0000 7047     		bx	lr
ARM GAS  /tmp/ccJPteqL.s 			page 77


 1724              		.cfi_endproc
 1725              	.LFE338:
 1727              		.section	.text.PCD_EP_ISR_Handler,"ax",%progbits
 1728              		.align	1
 1729              		.syntax unified
 1730              		.thumb
 1731              		.thumb_func
 1733              	PCD_EP_ISR_Handler:
 1734              	.LVL187:
 1735              	.LFB361:
1694:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 1736              		.loc 1 1694 1 is_stmt 1 view -0
 1737              		.cfi_startproc
 1738              		@ args = 0, pretend = 0, frame = 0
 1739              		@ frame_needed = 0, uses_anonymous_args = 0
1694:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 1740              		.loc 1 1694 1 is_stmt 0 view .LVU563
 1741 0000 2DE9F041 		push	{r4, r5, r6, r7, r8, lr}
 1742              	.LCFI12:
 1743              		.cfi_def_cfa_offset 24
 1744              		.cfi_offset 4, -24
 1745              		.cfi_offset 5, -20
 1746              		.cfi_offset 6, -16
 1747              		.cfi_offset 7, -12
 1748              		.cfi_offset 8, -8
 1749              		.cfi_offset 14, -4
 1750 0004 0546     		mov	r5, r0
1695:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint16_t count;
 1751              		.loc 1 1695 3 is_stmt 1 view .LVU564
1696:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint16_t wIstr;
 1752              		.loc 1 1696 3 view .LVU565
1697:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint16_t wEPVal;
 1753              		.loc 1 1697 3 view .LVU566
1698:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint16_t TxPctSize;
 1754              		.loc 1 1698 3 view .LVU567
1699:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint8_t epindex;
 1755              		.loc 1 1699 3 view .LVU568
1700:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1756              		.loc 1 1700 3 view .LVU569
1703:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 1757              		.loc 1 1703 3 view .LVU570
1703:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 1758              		.loc 1 1703 9 is_stmt 0 view .LVU571
 1759 0006 CAE0     		b	.L96
 1760              	.LVL188:
 1761              	.L127:
1721:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->IN_ep[0];
 1762              		.loc 1 1721 9 is_stmt 1 view .LVU572
 1763              	.LBB37:
1721:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->IN_ep[0];
 1764              		.loc 1 1721 9 view .LVU573
1721:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->IN_ep[0];
 1765              		.loc 1 1721 9 view .LVU574
 1766 0008 0388     		ldrh	r3, [r0]
 1767              	.LVL189:
1721:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->IN_ep[0];
 1768              		.loc 1 1721 9 is_stmt 0 view .LVU575
ARM GAS  /tmp/ccJPteqL.s 			page 78


 1769 000a 9BB2     		uxth	r3, r3
 1770 000c 23F4E143 		bic	r3, r3, #28800
 1771 0010 23F07003 		bic	r3, r3, #112
 1772              	.LVL190:
1721:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->IN_ep[0];
 1773              		.loc 1 1721 9 is_stmt 1 view .LVU576
 1774 0014 6FEA4343 		mvn	r3, r3, lsl #17
 1775              	.LVL191:
1721:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->IN_ep[0];
 1776              		.loc 1 1721 9 is_stmt 0 view .LVU577
 1777 0018 6FEA5343 		mvn	r3, r3, lsr #17
 1778 001c 9BB2     		uxth	r3, r3
 1779 001e 0380     		strh	r3, [r0]	@ movhi
 1780              	.LBE37:
1721:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->IN_ep[0];
 1781              		.loc 1 1721 9 is_stmt 1 view .LVU578
1722:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1782              		.loc 1 1722 9 view .LVU579
 1783              	.LVL192:
1724:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_buff += ep->xfer_count;
 1784              		.loc 1 1724 9 view .LVU580
1724:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_buff += ep->xfer_count;
 1785              		.loc 1 1724 26 is_stmt 0 view .LVU581
 1786 0020 2968     		ldr	r1, [r5]
 1787 0022 B1F85030 		ldrh	r3, [r1, #80]
 1788 0026 95F82820 		ldrb	r2, [r5, #40]	@ zero_extendqisi2
 1789 002a D200     		lsls	r2, r2, #3
 1790 002c 12FA83F3 		uxtah	r3, r2, r3
 1791 0030 0B44     		add	r3, r3, r1
 1792 0032 B3F80234 		ldrh	r3, [r3, #1026]
 1793 0036 C3F30903 		ubfx	r3, r3, #0, #10
1724:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_buff += ep->xfer_count;
 1794              		.loc 1 1724 24 view .LVU582
 1795 003a 6B64     		str	r3, [r5, #68]
1725:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1796              		.loc 1 1725 9 is_stmt 1 view .LVU583
1725:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1797              		.loc 1 1725 11 is_stmt 0 view .LVU584
 1798 003c EA6B     		ldr	r2, [r5, #60]
1725:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1799              		.loc 1 1725 23 view .LVU585
 1800 003e 1A44     		add	r2, r2, r3
 1801 0040 EA63     		str	r2, [r5, #60]
1731:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 1802              		.loc 1 1731 9 is_stmt 1 view .LVU586
 1803 0042 0021     		movs	r1, #0
 1804 0044 2846     		mov	r0, r5
 1805 0046 FFF7FEFF 		bl	HAL_PCD_DataInStageCallback
 1806              	.LVL193:
1734:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1807              		.loc 1 1734 9 view .LVU587
1734:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1808              		.loc 1 1734 18 is_stmt 0 view .LVU588
 1809 004a 95F82430 		ldrb	r3, [r5, #36]	@ zero_extendqisi2
1734:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1810              		.loc 1 1734 12 view .LVU589
 1811 004e 002B     		cmp	r3, #0
ARM GAS  /tmp/ccJPteqL.s 			page 79


 1812 0050 00F0A580 		beq	.L96
1734:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1813              		.loc 1 1734 44 discriminator 1 view .LVU590
 1814 0054 2B6C     		ldr	r3, [r5, #64]
1734:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1815              		.loc 1 1734 38 discriminator 1 view .LVU591
 1816 0056 002B     		cmp	r3, #0
 1817 0058 40F0A180 		bne	.L96
1736:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           hpcd->USB_Address = 0U;
 1818              		.loc 1 1736 11 is_stmt 1 view .LVU592
1736:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           hpcd->USB_Address = 0U;
 1819              		.loc 1 1736 50 is_stmt 0 view .LVU593
 1820 005c 95F82430 		ldrb	r3, [r5, #36]	@ zero_extendqisi2
1736:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           hpcd->USB_Address = 0U;
 1821              		.loc 1 1736 15 view .LVU594
 1822 0060 2A68     		ldr	r2, [r5]
1736:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           hpcd->USB_Address = 0U;
 1823              		.loc 1 1736 33 view .LVU595
 1824 0062 43F08003 		orr	r3, r3, #128
 1825 0066 A2F84C30 		strh	r3, [r2, #76]	@ movhi
1737:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1826              		.loc 1 1737 11 is_stmt 1 view .LVU596
1737:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 1827              		.loc 1 1737 29 is_stmt 0 view .LVU597
 1828 006a 0023     		movs	r3, #0
 1829 006c 85F82430 		strb	r3, [r5, #36]
 1830 0070 95E0     		b	.L96
 1831              	.LVL194:
 1832              	.L128:
1752:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1833              		.loc 1 1752 11 is_stmt 1 view .LVU598
1752:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1834              		.loc 1 1752 28 is_stmt 0 view .LVU599
 1835 0072 B0F85030 		ldrh	r3, [r0, #80]
 1836 0076 95F86821 		ldrb	r2, [r5, #360]	@ zero_extendqisi2
 1837              	.LVL195:
1752:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1838              		.loc 1 1752 28 view .LVU600
 1839 007a D200     		lsls	r2, r2, #3
 1840 007c 12FA83F3 		uxtah	r3, r2, r3
 1841 0080 0344     		add	r3, r3, r0
 1842 0082 B3F80634 		ldrh	r3, [r3, #1030]
 1843 0086 C3F30903 		ubfx	r3, r3, #0, #10
1752:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1844              		.loc 1 1752 26 view .LVU601
 1845 008a C5F88431 		str	r3, [r5, #388]
1754:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                       ep->pmaadress, (uint16_t)ep->xfer_count);
 1846              		.loc 1 1754 11 is_stmt 1 view .LVU602
 1847 008e B5F86E21 		ldrh	r2, [r5, #366]
 1848 0092 05F52C71 		add	r1, r5, #688
 1849 0096 FFF7FEFF 		bl	USB_ReadPMA
 1850              	.LVL196:
1758:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1851              		.loc 1 1758 11 view .LVU603
 1852              	.LBB38:
1758:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1853              		.loc 1 1758 11 view .LVU604
ARM GAS  /tmp/ccJPteqL.s 			page 80


1758:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1854              		.loc 1 1758 11 view .LVU605
 1855 009a 2A68     		ldr	r2, [r5]
 1856 009c 1388     		ldrh	r3, [r2]
 1857 009e 23F07003 		bic	r3, r3, #112
 1858 00a2 1B05     		lsls	r3, r3, #20
 1859 00a4 1B0D     		lsrs	r3, r3, #20
 1860              	.LVL197:
1758:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1861              		.loc 1 1758 11 view .LVU606
 1862 00a6 43F08003 		orr	r3, r3, #128
 1863              	.LVL198:
1758:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1864              		.loc 1 1758 11 is_stmt 0 view .LVU607
 1865 00aa 1380     		strh	r3, [r2]	@ movhi
 1866              	.LBE38:
1758:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1867              		.loc 1 1758 11 is_stmt 1 view .LVU608
1764:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 1868              		.loc 1 1764 11 view .LVU609
 1869 00ac 2846     		mov	r0, r5
 1870 00ae FFF7FEFF 		bl	HAL_PCD_SetupStageCallback
 1871              	.LVL199:
 1872 00b2 74E0     		b	.L96
 1873              	.LVL200:
 1874              	.L102:
 1875              	.LBB39:
 1876              	.LBB40:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 1877              		.loc 1 1791 13 discriminator 2 view .LVU610
 1878 00b4 89B9     		cbnz	r1, .L105
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 1879              		.loc 1 1791 13 discriminator 7 view .LVU611
 1880 00b6 B3F80624 		ldrh	r2, [r3, #1030]
 1881 00ba 92B2     		uxth	r2, r2
 1882 00bc 22F4F842 		bic	r2, r2, #31744
 1883 00c0 92B2     		uxth	r2, r2
 1884 00c2 A3F80624 		strh	r2, [r3, #1030]	@ movhi
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 1885              		.loc 1 1791 13 discriminator 7 view .LVU612
 1886 00c6 B3F80624 		ldrh	r2, [r3, #1030]
 1887 00ca 6FEA4242 		mvn	r2, r2, lsl #17
 1888 00ce 6FEA5242 		mvn	r2, r2, lsr #17
 1889 00d2 92B2     		uxth	r2, r2
 1890 00d4 A3F80624 		strh	r2, [r3, #1030]	@ movhi
 1891 00d8 BFE0     		b	.L104
 1892              	.L105:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 1893              		.loc 1 1791 13 discriminator 8 view .LVU613
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 1894              		.loc 1 1791 13 discriminator 8 view .LVU614
 1895 00da 4A08     		lsrs	r2, r1, #1
 1896              	.LVL201:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 1897              		.loc 1 1791 13 discriminator 8 view .LVU615
 1898 00dc 11F0010F 		tst	r1, #1
 1899 00e0 00D0     		beq	.L106
ARM GAS  /tmp/ccJPteqL.s 			page 81


1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 1900              		.loc 1 1791 13 discriminator 10 view .LVU616
 1901 00e2 0132     		adds	r2, r2, #1
 1902              	.LVL202:
 1903              	.L106:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 1904              		.loc 1 1791 13 discriminator 12 view .LVU617
 1905 00e4 9202     		lsls	r2, r2, #10
 1906              	.LVL203:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 1907              		.loc 1 1791 13 is_stmt 0 discriminator 12 view .LVU618
 1908 00e6 92B2     		uxth	r2, r2
 1909 00e8 A3F80624 		strh	r2, [r3, #1030]	@ movhi
 1910 00ec B5E0     		b	.L104
 1911              	.LVL204:
 1912              	.L97:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 1913              		.loc 1 1791 13 discriminator 12 view .LVU619
 1914              	.LBE40:
 1915              	.LBE39:
1801:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1916              		.loc 1 1801 7 is_stmt 1 view .LVU620
1801:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1917              		.loc 1 1801 14 is_stmt 0 view .LVU621
 1918 00ee 30F82430 		ldrh	r3, [r0, r4, lsl #2]
 1919              	.LVL205:
1801:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1920              		.loc 1 1801 14 view .LVU622
 1921 00f2 9EB2     		uxth	r6, r3
 1922              	.LVL206:
1803:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 1923              		.loc 1 1803 7 is_stmt 1 view .LVU623
1803:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 1924              		.loc 1 1803 10 is_stmt 0 view .LVU624
 1925 00f4 13F4004F 		tst	r3, #32768
 1926 00f8 40F0BE80 		bne	.L125
 1927              	.L107:
1875:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 1928              		.loc 1 1875 7 is_stmt 1 view .LVU625
1875:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 1929              		.loc 1 1875 10 is_stmt 0 view .LVU626
 1930 00fc 16F0800F 		tst	r6, #128
 1931 0100 4DD0     		beq	.L96
1877:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1932              		.loc 1 1877 9 is_stmt 1 view .LVU627
1877:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1933              		.loc 1 1877 12 is_stmt 0 view .LVU628
 1934 0102 621C     		adds	r2, r4, #1
 1935 0104 02EB8201 		add	r1, r2, r2, lsl #2
 1936 0108 05EBC101 		add	r1, r5, r1, lsl #3
 1937              	.LVL207:
1880:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1938              		.loc 1 1880 9 is_stmt 1 view .LVU629
 1939              	.LBB42:
1880:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1940              		.loc 1 1880 9 view .LVU630
1880:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 82


 1941              		.loc 1 1880 9 view .LVU631
 1942 010c 2868     		ldr	r0, [r5]
 1943 010e 30F82430 		ldrh	r3, [r0, r4, lsl #2]
 1944 0112 9BB2     		uxth	r3, r3
 1945 0114 23F4E143 		bic	r3, r3, #28800
 1946 0118 23F07003 		bic	r3, r3, #112
 1947              	.LVL208:
1880:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1948              		.loc 1 1880 9 view .LVU632
 1949 011c 6FEA4343 		mvn	r3, r3, lsl #17
 1950              	.LVL209:
1880:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1951              		.loc 1 1880 9 is_stmt 0 view .LVU633
 1952 0120 6FEA5343 		mvn	r3, r3, lsr #17
 1953 0124 9BB2     		uxth	r3, r3
 1954 0126 20F82430 		strh	r3, [r0, r4, lsl #2]	@ movhi
 1955              	.LBE42:
1880:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1956              		.loc 1 1880 9 is_stmt 1 view .LVU634
1882:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1957              		.loc 1 1882 9 view .LVU635
1882:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1958              		.loc 1 1882 15 is_stmt 0 view .LVU636
 1959 012a CB78     		ldrb	r3, [r1, #3]	@ zero_extendqisi2
1882:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 1960              		.loc 1 1882 12 view .LVU637
 1961 012c 022B     		cmp	r3, #2
 1962 012e 00F0A781 		beq	.L114
1884:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1963              		.loc 1 1884 11 is_stmt 1 view .LVU638
1884:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 1964              		.loc 1 1884 24 is_stmt 0 view .LVU639
 1965 0132 04EB8403 		add	r3, r4, r4, lsl #2
 1966 0136 05EBC303 		add	r3, r5, r3, lsl #3
 1967 013a 0022     		movs	r2, #0
 1968 013c 1A64     		str	r2, [r3, #64]
1887:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 1969              		.loc 1 1887 11 is_stmt 1 view .LVU640
1887:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 1970              		.loc 1 1887 17 is_stmt 0 view .LVU641
 1971 013e 93F83430 		ldrb	r3, [r3, #52]	@ zero_extendqisi2
1887:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 1972              		.loc 1 1887 14 view .LVU642
 1973 0142 23B3     		cbz	r3, .L115
1889:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 1974              		.loc 1 1889 13 is_stmt 1 view .LVU643
1889:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 1975              		.loc 1 1889 16 is_stmt 0 view .LVU644
 1976 0144 16F0400F 		tst	r6, #64
 1977 0148 00F06381 		beq	.L116
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 1978              		.loc 1 1891 15 is_stmt 1 view .LVU645
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 1979              		.loc 1 1891 15 view .LVU646
 1980 014c 4B78     		ldrb	r3, [r1, #1]	@ zero_extendqisi2
 1981 014e 002B     		cmp	r3, #0
 1982 0150 40F04C81 		bne	.L117
ARM GAS  /tmp/ccJPteqL.s 			page 83


1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 1983              		.loc 1 1891 15 discriminator 1 view .LVU647
 1984              	.LBB43:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 1985              		.loc 1 1891 15 discriminator 1 view .LVU648
 1986 0154 2A68     		ldr	r2, [r5]
 1987              	.LVL210:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 1988              		.loc 1 1891 15 discriminator 1 view .LVU649
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 1989              		.loc 1 1891 15 discriminator 1 view .LVU650
 1990 0156 B2F85030 		ldrh	r3, [r2, #80]
 1991 015a 12FA83F3 		uxtah	r3, r2, r3
 1992              	.LVL211:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 1993              		.loc 1 1891 15 discriminator 1 view .LVU651
 1994 015e 621C     		adds	r2, r4, #1
 1995 0160 02EB8202 		add	r2, r2, r2, lsl #2
 1996 0164 15F83220 		ldrb	r2, [r5, r2, lsl #3]	@ zero_extendqisi2
 1997 0168 03EBC203 		add	r3, r3, r2, lsl #3
 1998              	.LVL212:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 1999              		.loc 1 1891 15 discriminator 1 view .LVU652
 2000              	.LBB44:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2001              		.loc 1 1891 15 discriminator 1 view .LVU653
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2002              		.loc 1 1891 15 discriminator 1 view .LVU654
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2003              		.loc 1 1891 15 discriminator 1 view .LVU655
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2004              		.loc 1 1891 15 discriminator 1 view .LVU656
 2005 016c B3F80224 		ldrh	r2, [r3, #1026]
 2006 0170 92B2     		uxth	r2, r2
 2007 0172 22F4F842 		bic	r2, r2, #31744
 2008 0176 92B2     		uxth	r2, r2
 2009 0178 A3F80224 		strh	r2, [r3, #1026]	@ movhi
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2010              		.loc 1 1891 15 discriminator 1 view .LVU657
 2011 017c B3F80224 		ldrh	r2, [r3, #1026]
 2012 0180 6FEA4242 		mvn	r2, r2, lsl #17
 2013 0184 6FEA5242 		mvn	r2, r2, lsr #17
 2014 0188 92B2     		uxth	r2, r2
 2015 018a A3F80224 		strh	r2, [r3, #1026]	@ movhi
 2016              	.LVL213:
 2017              	.L115:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2018              		.loc 1 1891 15 is_stmt 0 discriminator 1 view .LVU658
 2019              	.LBE44:
 2020              	.LBE43:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2021              		.loc 1 1895 15 is_stmt 1 discriminator 18 view .LVU659
1904:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 2022              		.loc 1 1904 11 discriminator 18 view .LVU660
 2023 018e 0134     		adds	r4, r4, #1
 2024 0190 04EB8404 		add	r4, r4, r4, lsl #2
 2025 0194 15F83410 		ldrb	r1, [r5, r4, lsl #3]	@ zero_extendqisi2
ARM GAS  /tmp/ccJPteqL.s 			page 84


 2026              	.LVL214:
1904:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 2027              		.loc 1 1904 11 is_stmt 0 discriminator 18 view .LVU661
 2028 0198 2846     		mov	r0, r5
 2029 019a FFF7FEFF 		bl	HAL_PCD_DataInStageCallback
 2030              	.LVL215:
 2031              	.L96:
1703:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 2032              		.loc 1 1703 48 is_stmt 1 view .LVU662
1703:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 2033              		.loc 1 1703 15 is_stmt 0 view .LVU663
 2034 019e 2868     		ldr	r0, [r5]
1703:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 2035              		.loc 1 1703 25 view .LVU664
 2036 01a0 B0F84430 		ldrh	r3, [r0, #68]
1703:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 2037              		.loc 1 1703 48 view .LVU665
 2038 01a4 13F4004F 		tst	r3, #32768
 2039 01a8 00F0B281 		beq	.L126
1705:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2040              		.loc 1 1705 5 is_stmt 1 view .LVU666
1705:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2041              		.loc 1 1705 11 is_stmt 0 view .LVU667
 2042 01ac B0F84440 		ldrh	r4, [r0, #68]
 2043 01b0 A3B2     		uxth	r3, r4
 2044              	.LVL216:
1708:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2045              		.loc 1 1708 5 is_stmt 1 view .LVU668
1710:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 2046              		.loc 1 1710 5 view .LVU669
1710:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 2047              		.loc 1 1710 8 is_stmt 0 view .LVU670
 2048 01b2 14F00F04 		ands	r4, r4, #15
 2049              	.LVL217:
1710:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 2050              		.loc 1 1710 8 view .LVU671
 2051 01b6 9AD1     		bne	.L97
1715:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 2052              		.loc 1 1715 7 is_stmt 1 view .LVU672
1715:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       {
 2053              		.loc 1 1715 10 is_stmt 0 view .LVU673
 2054 01b8 13F0100F 		tst	r3, #16
 2055 01bc 3FF424AF 		beq	.L127
1746:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         wEPVal = PCD_GET_ENDPOINT(hpcd->Instance, PCD_ENDP0);
 2056              		.loc 1 1746 9 is_stmt 1 view .LVU674
 2057              	.LVL218:
1747:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2058              		.loc 1 1747 9 view .LVU675
1747:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2059              		.loc 1 1747 16 is_stmt 0 view .LVU676
 2060 01c0 0388     		ldrh	r3, [r0]
 2061              	.LVL219:
1747:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2062              		.loc 1 1747 16 view .LVU677
 2063 01c2 9AB2     		uxth	r2, r3
 2064              	.LVL220:
1749:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
ARM GAS  /tmp/ccJPteqL.s 			page 85


 2065              		.loc 1 1749 9 is_stmt 1 view .LVU678
1749:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 2066              		.loc 1 1749 12 is_stmt 0 view .LVU679
 2067 01c4 13F4006F 		tst	r3, #2048
 2068 01c8 7FF453AF 		bne	.L128
1767:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 2069              		.loc 1 1767 14 is_stmt 1 view .LVU680
1767:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 2070              		.loc 1 1767 17 is_stmt 0 view .LVU681
 2071 01cc 12F4004F 		tst	r2, #32768
 2072 01d0 E5D0     		beq	.L96
1769:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2073              		.loc 1 1769 11 is_stmt 1 view .LVU682
 2074              	.LBB45:
1769:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2075              		.loc 1 1769 11 view .LVU683
1769:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2076              		.loc 1 1769 11 view .LVU684
 2077 01d2 0388     		ldrh	r3, [r0]
 2078 01d4 23F07003 		bic	r3, r3, #112
 2079 01d8 1B05     		lsls	r3, r3, #20
 2080 01da 1B0D     		lsrs	r3, r3, #20
 2081              	.LVL221:
1769:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2082              		.loc 1 1769 11 view .LVU685
 2083 01dc 43F08003 		orr	r3, r3, #128
 2084              	.LVL222:
1769:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2085              		.loc 1 1769 11 is_stmt 0 view .LVU686
 2086 01e0 0380     		strh	r3, [r0]	@ movhi
 2087              	.LBE45:
1769:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2088              		.loc 1 1769 11 is_stmt 1 view .LVU687
1772:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2089              		.loc 1 1772 11 view .LVU688
1772:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2090              		.loc 1 1772 28 is_stmt 0 view .LVU689
 2091 01e2 2868     		ldr	r0, [r5]
 2092 01e4 B0F85030 		ldrh	r3, [r0, #80]
 2093 01e8 95F86821 		ldrb	r2, [r5, #360]	@ zero_extendqisi2
 2094              	.LVL223:
1772:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2095              		.loc 1 1772 28 view .LVU690
 2096 01ec D200     		lsls	r2, r2, #3
 2097 01ee 12FA83F3 		uxtah	r3, r2, r3
 2098 01f2 0344     		add	r3, r3, r0
 2099 01f4 B3F80634 		ldrh	r3, [r3, #1030]
 2100 01f8 C3F30903 		ubfx	r3, r3, #0, #10
1772:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2101              		.loc 1 1772 26 view .LVU691
 2102 01fc C5F88431 		str	r3, [r5, #388]
1774:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2103              		.loc 1 1774 11 is_stmt 1 view .LVU692
1774:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2104              		.loc 1 1774 14 is_stmt 0 view .LVU693
 2105 0200 8BB1     		cbz	r3, .L101
1774:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
ARM GAS  /tmp/ccJPteqL.s 			page 86


 2106              		.loc 1 1774 44 discriminator 1 view .LVU694
 2107 0202 D5F87C11 		ldr	r1, [r5, #380]
1774:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2108              		.loc 1 1774 38 discriminator 1 view .LVU695
 2109 0206 71B1     		cbz	r1, .L101
1776:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****                         ep->pmaadress, (uint16_t)ep->xfer_count);
 2110              		.loc 1 1776 13 is_stmt 1 view .LVU696
 2111 0208 B5F86E21 		ldrh	r2, [r5, #366]
 2112 020c FFF7FEFF 		bl	USB_ReadPMA
 2113              	.LVL224:
1779:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2114              		.loc 1 1779 13 view .LVU697
1779:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2115              		.loc 1 1779 15 is_stmt 0 view .LVU698
 2116 0210 D5F87C31 		ldr	r3, [r5, #380]
1779:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2117              		.loc 1 1779 32 view .LVU699
 2118 0214 D5F88421 		ldr	r2, [r5, #388]
1779:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2119              		.loc 1 1779 27 view .LVU700
 2120 0218 1344     		add	r3, r3, r2
 2121 021a C5F87C31 		str	r3, [r5, #380]
1785:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 2122              		.loc 1 1785 13 is_stmt 1 view .LVU701
 2123 021e 0021     		movs	r1, #0
 2124 0220 2846     		mov	r0, r5
 2125 0222 FFF7FEFF 		bl	HAL_PCD_DataOutStageCallback
 2126              	.LVL225:
 2127              	.L101:
1789:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2128              		.loc 1 1789 11 view .LVU702
1789:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2129              		.loc 1 1789 16 is_stmt 0 view .LVU703
 2130 0226 2B68     		ldr	r3, [r5]
 2131 0228 1A88     		ldrh	r2, [r3]
1789:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2132              		.loc 1 1789 14 view .LVU704
 2133 022a 12F4006F 		tst	r2, #2048
 2134 022e B6D1     		bne	.L96
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2135              		.loc 1 1791 13 is_stmt 1 view .LVU705
 2136              	.LBB46:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2137              		.loc 1 1791 13 view .LVU706
 2138              	.LVL226:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2139              		.loc 1 1791 13 view .LVU707
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2140              		.loc 1 1791 13 view .LVU708
 2141 0230 B3F85020 		ldrh	r2, [r3, #80]
 2142 0234 13FA82F3 		uxtah	r3, r3, r2
 2143              	.LVL227:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2144              		.loc 1 1791 13 view .LVU709
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2145              		.loc 1 1791 13 view .LVU710
 2146              	.LBB41:
ARM GAS  /tmp/ccJPteqL.s 			page 87


1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2147              		.loc 1 1791 13 view .LVU711
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2148              		.loc 1 1791 13 view .LVU712
 2149 0238 D5F87811 		ldr	r1, [r5, #376]
 2150 023c 3E29     		cmp	r1, #62
 2151 023e 7FF639AF 		bls	.L102
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2152              		.loc 1 1791 13 discriminator 1 view .LVU713
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2153              		.loc 1 1791 13 discriminator 1 view .LVU714
 2154 0242 4A09     		lsrs	r2, r1, #5
 2155              	.LVL228:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2156              		.loc 1 1791 13 discriminator 1 view .LVU715
 2157 0244 11F01F0F 		tst	r1, #31
 2158 0248 00D1     		bne	.L103
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2159              		.loc 1 1791 13 discriminator 3 view .LVU716
 2160 024a 013A     		subs	r2, r2, #1
 2161              	.LVL229:
 2162              	.L103:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2163              		.loc 1 1791 13 discriminator 5 view .LVU717
 2164 024c 6FEAC262 		mvn	r2, r2, lsl #27
 2165              	.LVL230:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2166              		.loc 1 1791 13 is_stmt 0 discriminator 5 view .LVU718
 2167 0250 6FEA5242 		mvn	r2, r2, lsr #17
 2168 0254 92B2     		uxth	r2, r2
 2169 0256 A3F80624 		strh	r2, [r3, #1030]	@ movhi
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2170              		.loc 1 1791 13 is_stmt 1 discriminator 5 view .LVU719
 2171              	.LVL231:
 2172              	.L104:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2173              		.loc 1 1791 13 discriminator 13 view .LVU720
 2174              	.LBE41:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2175              		.loc 1 1791 13 discriminator 13 view .LVU721
 2176              	.LBE46:
1791:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             PCD_SET_EP_RX_STATUS(hpcd->Instance, PCD_ENDP0, USB_EP_RX_VALID);
 2177              		.loc 1 1791 13 discriminator 13 view .LVU722
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2178              		.loc 1 1792 13 discriminator 13 view .LVU723
 2179              	.LBB47:
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2180              		.loc 1 1792 13 discriminator 13 view .LVU724
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2181              		.loc 1 1792 13 discriminator 13 view .LVU725
 2182 025a 2A68     		ldr	r2, [r5]
 2183 025c 1388     		ldrh	r3, [r2]
 2184              	.LVL232:
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2185              		.loc 1 1792 13 is_stmt 0 discriminator 13 view .LVU726
 2186 025e 9BB2     		uxth	r3, r3
 2187 0260 23F48043 		bic	r3, r3, #16384
ARM GAS  /tmp/ccJPteqL.s 			page 88


 2188 0264 23F07003 		bic	r3, r3, #112
 2189              	.LVL233:
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2190              		.loc 1 1792 13 is_stmt 1 discriminator 13 view .LVU727
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2191              		.loc 1 1792 13 discriminator 13 view .LVU728
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2192              		.loc 1 1792 13 discriminator 13 view .LVU729
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2193              		.loc 1 1792 13 discriminator 13 view .LVU730
 2194 0268 83F44053 		eor	r3, r3, #12288
 2195              	.LVL234:
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2196              		.loc 1 1792 13 discriminator 13 view .LVU731
 2197 026c 43F40043 		orr	r3, r3, #32768
 2198              	.LVL235:
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2199              		.loc 1 1792 13 is_stmt 0 discriminator 13 view .LVU732
 2200 0270 43F08003 		orr	r3, r3, #128
 2201 0274 1380     		strh	r3, [r2]	@ movhi
 2202 0276 92E7     		b	.L96
 2203              	.LVL236:
 2204              	.L125:
1792:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2205              		.loc 1 1792 13 discriminator 13 view .LVU733
 2206              	.LBE47:
1806:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->OUT_ep[epindex];
 2207              		.loc 1 1806 9 is_stmt 1 view .LVU734
 2208              	.LBB48:
1806:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->OUT_ep[epindex];
 2209              		.loc 1 1806 9 view .LVU735
1806:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->OUT_ep[epindex];
 2210              		.loc 1 1806 9 view .LVU736
 2211 0278 30F82430 		ldrh	r3, [r0, r4, lsl #2]
 2212 027c 23F07003 		bic	r3, r3, #112
 2213 0280 1B05     		lsls	r3, r3, #20
 2214 0282 1B0D     		lsrs	r3, r3, #20
 2215              	.LVL237:
1806:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->OUT_ep[epindex];
 2216              		.loc 1 1806 9 view .LVU737
 2217 0284 43F08003 		orr	r3, r3, #128
 2218              	.LVL238:
1806:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->OUT_ep[epindex];
 2219              		.loc 1 1806 9 is_stmt 0 view .LVU738
 2220 0288 20F82430 		strh	r3, [r0, r4, lsl #2]	@ movhi
 2221              	.LBE48:
1806:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep = &hpcd->OUT_ep[epindex];
 2222              		.loc 1 1806 9 is_stmt 1 view .LVU739
1807:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2223              		.loc 1 1807 9 view .LVU740
1807:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2224              		.loc 1 1807 12 is_stmt 0 view .LVU741
 2225 028c 04EB8401 		add	r1, r4, r4, lsl #2
 2226 0290 C900     		lsls	r1, r1, #3
 2227 0292 01F5B471 		add	r1, r1, #360
 2228 0296 05EB0108 		add	r8, r5, r1
 2229              	.LVL239:
ARM GAS  /tmp/ccJPteqL.s 			page 89


1810:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 2230              		.loc 1 1810 9 is_stmt 1 view .LVU742
1810:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 2231              		.loc 1 1810 15 is_stmt 0 view .LVU743
 2232 029a 04EB8403 		add	r3, r4, r4, lsl #2
 2233 029e 05EBC303 		add	r3, r5, r3, lsl #3
 2234 02a2 93F87431 		ldrb	r3, [r3, #372]	@ zero_extendqisi2
1810:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 2235              		.loc 1 1810 12 view .LVU744
 2236 02a6 002B     		cmp	r3, #0
 2237 02a8 40D1     		bne	.L108
1812:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2238              		.loc 1 1812 11 is_stmt 1 view .LVU745
1812:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2239              		.loc 1 1812 29 is_stmt 0 view .LVU746
 2240 02aa 2868     		ldr	r0, [r5]
 2241 02ac B0F85030 		ldrh	r3, [r0, #80]
 2242 02b0 04EB8402 		add	r2, r4, r4, lsl #2
 2243 02b4 05EBC202 		add	r2, r5, r2, lsl #3
 2244 02b8 92F86821 		ldrb	r2, [r2, #360]	@ zero_extendqisi2
 2245 02bc D200     		lsls	r2, r2, #3
 2246 02be 12FA83F3 		uxtah	r3, r2, r3
 2247 02c2 0344     		add	r3, r3, r0
 2248 02c4 B3F80674 		ldrh	r7, [r3, #1030]
1812:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2249              		.loc 1 1812 17 view .LVU747
 2250 02c8 C7F30907 		ubfx	r7, r7, #0, #10
 2251              	.LVL240:
1814:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2252              		.loc 1 1814 11 is_stmt 1 view .LVU748
1814:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2253              		.loc 1 1814 14 is_stmt 0 view .LVU749
 2254 02cc 17BB     		cbnz	r7, .L129
 2255              	.L109:
1857:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_buff += count;
 2256              		.loc 1 1857 9 is_stmt 1 view .LVU750
1857:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_buff += count;
 2257              		.loc 1 1857 11 is_stmt 0 view .LVU751
 2258 02ce 04EB8403 		add	r3, r4, r4, lsl #2
 2259 02d2 05EBC303 		add	r3, r5, r3, lsl #3
 2260 02d6 D3F88421 		ldr	r2, [r3, #388]
1857:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         ep->xfer_buff += count;
 2261              		.loc 1 1857 24 view .LVU752
 2262 02da 3A44     		add	r2, r2, r7
 2263 02dc C3F88421 		str	r2, [r3, #388]
1858:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2264              		.loc 1 1858 9 is_stmt 1 view .LVU753
1858:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2265              		.loc 1 1858 11 is_stmt 0 view .LVU754
 2266 02e0 D3F87C21 		ldr	r2, [r3, #380]
1858:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2267              		.loc 1 1858 23 view .LVU755
 2268 02e4 3A44     		add	r2, r2, r7
 2269 02e6 C3F87C21 		str	r2, [r3, #380]
1860:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 2270              		.loc 1 1860 9 is_stmt 1 view .LVU756
1860:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
ARM GAS  /tmp/ccJPteqL.s 			page 90


 2271              		.loc 1 1860 16 is_stmt 0 view .LVU757
 2272 02ea D3F88031 		ldr	r3, [r3, #384]
1860:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 2273              		.loc 1 1860 12 view .LVU758
 2274 02ee 3BB1     		cbz	r3, .L112
1860:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 2275              		.loc 1 1860 48 discriminator 1 view .LVU759
 2276 02f0 04EB8403 		add	r3, r4, r4, lsl #2
 2277 02f4 05EBC303 		add	r3, r5, r3, lsl #3
 2278 02f8 D3F87831 		ldr	r3, [r3, #376]
1860:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         {
 2279              		.loc 1 1860 34 discriminator 1 view .LVU760
 2280 02fc 9F42     		cmp	r7, r3
 2281 02fe 70D2     		bcs	.L113
 2282              	.L112:
1866:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 2283              		.loc 1 1866 11 is_stmt 1 view .LVU761
 2284 0300 04EB8403 		add	r3, r4, r4, lsl #2
 2285 0304 05EBC303 		add	r3, r5, r3, lsl #3
 2286 0308 93F86811 		ldrb	r1, [r3, #360]	@ zero_extendqisi2
 2287 030c 2846     		mov	r0, r5
 2288 030e FFF7FEFF 		bl	HAL_PCD_DataOutStageCallback
 2289              	.LVL241:
 2290 0312 F3E6     		b	.L107
 2291              	.L129:
1816:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2292              		.loc 1 1816 13 view .LVU762
 2293 0314 04EB8401 		add	r1, r4, r4, lsl #2
 2294 0318 05EBC101 		add	r1, r5, r1, lsl #3
 2295 031c 3B46     		mov	r3, r7
 2296 031e B1F86E21 		ldrh	r2, [r1, #366]
 2297 0322 D1F87C11 		ldr	r1, [r1, #380]
 2298 0326 FFF7FEFF 		bl	USB_ReadPMA
 2299              	.LVL242:
 2300 032a D0E7     		b	.L109
 2301              	.LVL243:
 2302              	.L108:
1823:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2303              		.loc 1 1823 11 view .LVU763
1823:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2304              		.loc 1 1823 17 is_stmt 0 view .LVU764
 2305 032c 04EB8403 		add	r3, r4, r4, lsl #2
 2306 0330 05EBC303 		add	r3, r5, r3, lsl #3
 2307 0334 93F86B31 		ldrb	r3, [r3, #363]	@ zero_extendqisi2
1823:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2308              		.loc 1 1823 14 view .LVU765
 2309 0338 022B     		cmp	r3, #2
 2310 033a 33D0     		beq	.L130
1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2311              		.loc 1 1830 13 is_stmt 1 discriminator 1 view .LVU766
1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2312              		.loc 1 1830 13 discriminator 1 view .LVU767
1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2313              		.loc 1 1830 13 discriminator 1 view .LVU768
 2314              	.LBB49:
1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2315              		.loc 1 1830 13 discriminator 1 view .LVU769
ARM GAS  /tmp/ccJPteqL.s 			page 91


1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2316              		.loc 1 1830 13 discriminator 1 view .LVU770
 2317 033c 2968     		ldr	r1, [r5]
 2318 033e 04EB8402 		add	r2, r4, r4, lsl #2
 2319 0342 05EBC202 		add	r2, r5, r2, lsl #3
 2320 0346 92F86801 		ldrb	r0, [r2, #360]	@ zero_extendqisi2
 2321 034a 31F82030 		ldrh	r3, [r1, r0, lsl #2]
 2322 034e 9BB2     		uxth	r3, r3
 2323 0350 23F4E043 		bic	r3, r3, #28672
 2324 0354 23F07003 		bic	r3, r3, #112
 2325              	.LVL244:
1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2326              		.loc 1 1830 13 discriminator 1 view .LVU771
 2327 0358 43F40043 		orr	r3, r3, #32768
 2328              	.LVL245:
1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2329              		.loc 1 1830 13 is_stmt 0 discriminator 1 view .LVU772
 2330 035c 43F0C003 		orr	r3, r3, #192
 2331 0360 21F82030 		strh	r3, [r1, r0, lsl #2]	@ movhi
 2332              	.LBE49:
1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2333              		.loc 1 1830 13 is_stmt 1 discriminator 1 view .LVU773
1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2334              		.loc 1 1830 13 discriminator 1 view .LVU774
1830:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2335              		.loc 1 1830 13 discriminator 1 view .LVU775
1832:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 2336              		.loc 1 1832 13 discriminator 1 view .LVU776
1832:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 2337              		.loc 1 1832 18 is_stmt 0 discriminator 1 view .LVU777
 2338 0364 2868     		ldr	r0, [r5]
 2339 0366 92F86831 		ldrb	r3, [r2, #360]	@ zero_extendqisi2
 2340 036a 30F82320 		ldrh	r2, [r0, r3, lsl #2]
1832:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 2341              		.loc 1 1832 16 discriminator 1 view .LVU778
 2342 036e 12F4804F 		tst	r2, #16384
 2343 0372 1ED0     		beq	.L111
1835:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2344              		.loc 1 1835 15 is_stmt 1 view .LVU779
1835:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2345              		.loc 1 1835 33 is_stmt 0 view .LVU780
 2346 0374 B0F85020 		ldrh	r2, [r0, #80]
 2347 0378 DB00     		lsls	r3, r3, #3
 2348 037a 13FA82F3 		uxtah	r3, r3, r2
 2349 037e 0344     		add	r3, r3, r0
 2350 0380 B3F80274 		ldrh	r7, [r3, #1026]
1835:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2351              		.loc 1 1835 21 view .LVU781
 2352 0384 C7F30907 		ubfx	r7, r7, #0, #10
 2353              	.LVL246:
1837:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               {
 2354              		.loc 1 1837 15 is_stmt 1 view .LVU782
1837:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               {
 2355              		.loc 1 1837 18 is_stmt 0 view .LVU783
 2356 0388 002F     		cmp	r7, #0
 2357 038a A0D0     		beq	.L109
1839:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               }
ARM GAS  /tmp/ccJPteqL.s 			page 92


 2358              		.loc 1 1839 17 is_stmt 1 view .LVU784
 2359 038c 04EB8401 		add	r1, r4, r4, lsl #2
 2360 0390 05EBC101 		add	r1, r5, r1, lsl #3
 2361 0394 3B46     		mov	r3, r7
 2362 0396 B1F87021 		ldrh	r2, [r1, #368]
 2363 039a D1F87C11 		ldr	r1, [r1, #380]
 2364 039e FFF7FEFF 		bl	USB_ReadPMA
 2365              	.LVL247:
 2366 03a2 94E7     		b	.L109
 2367              	.LVL248:
 2368              	.L130:
1825:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2369              		.loc 1 1825 13 view .LVU785
1825:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2370              		.loc 1 1825 21 is_stmt 0 view .LVU786
 2371 03a4 3246     		mov	r2, r6
 2372 03a6 4146     		mov	r1, r8
 2373 03a8 2846     		mov	r0, r5
 2374 03aa FFF7FEFF 		bl	HAL_PCD_EP_DB_Receive
 2375              	.LVL249:
 2376 03ae 0746     		mov	r7, r0
 2377              	.LVL250:
1825:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2378              		.loc 1 1825 21 view .LVU787
 2379 03b0 8DE7     		b	.L109
 2380              	.LVL251:
 2381              	.L111:
1845:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2382              		.loc 1 1845 15 is_stmt 1 view .LVU788
1845:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2383              		.loc 1 1845 33 is_stmt 0 view .LVU789
 2384 03b2 B0F85020 		ldrh	r2, [r0, #80]
 2385 03b6 DB00     		lsls	r3, r3, #3
 2386 03b8 13FA82F3 		uxtah	r3, r3, r2
 2387 03bc 0344     		add	r3, r3, r0
 2388 03be B3F80674 		ldrh	r7, [r3, #1030]
1845:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2389              		.loc 1 1845 21 view .LVU790
 2390 03c2 C7F30907 		ubfx	r7, r7, #0, #10
 2391              	.LVL252:
1847:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               {
 2392              		.loc 1 1847 15 is_stmt 1 view .LVU791
1847:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               {
 2393              		.loc 1 1847 18 is_stmt 0 view .LVU792
 2394 03c6 002F     		cmp	r7, #0
 2395 03c8 81D0     		beq	.L109
1849:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               }
 2396              		.loc 1 1849 17 is_stmt 1 view .LVU793
 2397 03ca 04EB8401 		add	r1, r4, r4, lsl #2
 2398 03ce 05EBC101 		add	r1, r5, r1, lsl #3
 2399 03d2 3B46     		mov	r3, r7
 2400 03d4 B1F87221 		ldrh	r2, [r1, #370]
 2401 03d8 D1F87C11 		ldr	r1, [r1, #380]
 2402 03dc FFF7FEFF 		bl	USB_ReadPMA
 2403              	.LVL253:
 2404 03e0 75E7     		b	.L109
 2405              	.LVL254:
ARM GAS  /tmp/ccJPteqL.s 			page 93


 2406              	.L113:
1871:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 2407              		.loc 1 1871 11 view .LVU794
1871:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****         }
 2408              		.loc 1 1871 18 is_stmt 0 view .LVU795
 2409 03e2 4146     		mov	r1, r8
 2410 03e4 2868     		ldr	r0, [r5]
 2411 03e6 FFF7FEFF 		bl	USB_EPStartXfer
 2412              	.LVL255:
 2413 03ea 87E6     		b	.L107
 2414              	.LVL256:
 2415              	.L117:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2416              		.loc 1 1891 15 is_stmt 1 discriminator 2 view .LVU796
 2417 03ec 012B     		cmp	r3, #1
 2418 03ee 7FF4CEAE 		bne	.L115
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2419              		.loc 1 1891 15 discriminator 16 view .LVU797
 2420              	.LBB50:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2421              		.loc 1 1891 15 discriminator 16 view .LVU798
 2422 03f2 2A68     		ldr	r2, [r5]
 2423              	.LVL257:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2424              		.loc 1 1891 15 discriminator 16 view .LVU799
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2425              		.loc 1 1891 15 discriminator 16 view .LVU800
 2426 03f4 B2F85030 		ldrh	r3, [r2, #80]
 2427 03f8 12FA83F3 		uxtah	r3, r2, r3
 2428              	.LVL258:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2429              		.loc 1 1891 15 discriminator 16 view .LVU801
 2430 03fc 621C     		adds	r2, r4, #1
 2431 03fe 02EB8202 		add	r2, r2, r2, lsl #2
 2432 0402 15F83220 		ldrb	r2, [r5, r2, lsl #3]	@ zero_extendqisi2
 2433 0406 03EBC203 		add	r3, r3, r2, lsl #3
 2434              	.LVL259:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2435              		.loc 1 1891 15 discriminator 16 view .LVU802
 2436 040a 0022     		movs	r2, #0
 2437 040c A3F80224 		strh	r2, [r3, #1026]	@ movhi
 2438 0410 BDE6     		b	.L115
 2439              	.LVL260:
 2440              	.L116:
1891:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2441              		.loc 1 1891 15 is_stmt 0 discriminator 16 view .LVU803
 2442              	.LBE50:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2443              		.loc 1 1895 15 is_stmt 1 view .LVU804
 2444              	.LBB51:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2445              		.loc 1 1895 15 view .LVU805
 2446 0412 2A68     		ldr	r2, [r5]
 2447              	.LVL261:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2448              		.loc 1 1895 15 view .LVU806
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
ARM GAS  /tmp/ccJPteqL.s 			page 94


 2449              		.loc 1 1895 15 view .LVU807
 2450 0414 631C     		adds	r3, r4, #1
 2451 0416 03EB8303 		add	r3, r3, r3, lsl #2
 2452 041a 05EBC303 		add	r3, r5, r3, lsl #3
 2453 041e 5B78     		ldrb	r3, [r3, #1]	@ zero_extendqisi2
 2454 0420 E3B9     		cbnz	r3, .L118
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2455              		.loc 1 1895 15 discriminator 1 view .LVU808
 2456              	.LBB52:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2457              		.loc 1 1895 15 discriminator 1 view .LVU809
 2458              	.LVL262:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2459              		.loc 1 1895 15 discriminator 1 view .LVU810
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2460              		.loc 1 1895 15 discriminator 1 view .LVU811
 2461 0422 B2F85030 		ldrh	r3, [r2, #80]
 2462 0426 12FA83F3 		uxtah	r3, r2, r3
 2463              	.LVL263:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2464              		.loc 1 1895 15 discriminator 1 view .LVU812
 2465 042a 621C     		adds	r2, r4, #1
 2466              	.LVL264:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2467              		.loc 1 1895 15 is_stmt 0 discriminator 1 view .LVU813
 2468 042c 02EB8202 		add	r2, r2, r2, lsl #2
 2469 0430 15F83220 		ldrb	r2, [r5, r2, lsl #3]	@ zero_extendqisi2
 2470 0434 03EBC203 		add	r3, r3, r2, lsl #3
 2471              	.LVL265:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2472              		.loc 1 1895 15 is_stmt 1 discriminator 1 view .LVU814
 2473              	.LBB53:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2474              		.loc 1 1895 15 discriminator 1 view .LVU815
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2475              		.loc 1 1895 15 discriminator 1 view .LVU816
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2476              		.loc 1 1895 15 discriminator 1 view .LVU817
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2477              		.loc 1 1895 15 discriminator 1 view .LVU818
 2478 0438 B3F80624 		ldrh	r2, [r3, #1030]
 2479 043c 92B2     		uxth	r2, r2
 2480 043e 22F4F842 		bic	r2, r2, #31744
 2481 0442 92B2     		uxth	r2, r2
 2482 0444 A3F80624 		strh	r2, [r3, #1030]	@ movhi
 2483              	.LVL266:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2484              		.loc 1 1895 15 discriminator 1 view .LVU819
 2485 0448 B3F80624 		ldrh	r2, [r3, #1030]
 2486 044c 6FEA4242 		mvn	r2, r2, lsl #17
 2487 0450 6FEA5242 		mvn	r2, r2, lsr #17
 2488 0454 92B2     		uxth	r2, r2
 2489 0456 A3F80624 		strh	r2, [r3, #1030]	@ movhi
 2490 045a 98E6     		b	.L115
 2491              	.LVL267:
 2492              	.L118:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
ARM GAS  /tmp/ccJPteqL.s 			page 95


 2493              		.loc 1 1895 15 is_stmt 0 discriminator 1 view .LVU820
 2494              	.LBE53:
 2495              	.LBE52:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2496              		.loc 1 1895 15 is_stmt 1 discriminator 2 view .LVU821
 2497 045c 012B     		cmp	r3, #1
 2498 045e 7FF496AE 		bne	.L115
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2499              		.loc 1 1895 15 discriminator 16 view .LVU822
 2500 0462 B2F85030 		ldrh	r3, [r2, #80]
 2501 0466 12FA83F3 		uxtah	r3, r2, r3
 2502              	.LVL268:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2503              		.loc 1 1895 15 discriminator 16 view .LVU823
 2504 046a 621C     		adds	r2, r4, #1
 2505 046c 02EB8202 		add	r2, r2, r2, lsl #2
 2506 0470 15F83220 		ldrb	r2, [r5, r2, lsl #3]	@ zero_extendqisi2
 2507 0474 03EBC203 		add	r3, r3, r2, lsl #3
 2508              	.LVL269:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2509              		.loc 1 1895 15 discriminator 16 view .LVU824
 2510 0478 0022     		movs	r2, #0
 2511 047a A3F80624 		strh	r2, [r3, #1030]	@ movhi
 2512 047e 86E6     		b	.L115
 2513              	.LVL270:
 2514              	.L114:
1895:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2515              		.loc 1 1895 15 is_stmt 0 discriminator 16 view .LVU825
 2516              	.LBE51:
1910:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2517              		.loc 1 1910 11 is_stmt 1 view .LVU826
1910:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           {
 2518              		.loc 1 1910 14 is_stmt 0 view .LVU827
 2519 0480 16F4807F 		tst	r6, #256
 2520 0484 3FD1     		bne	.L119
1913:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2521              		.loc 1 1913 13 is_stmt 1 view .LVU828
1913:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2522              		.loc 1 1913 35 is_stmt 0 view .LVU829
 2523 0486 2868     		ldr	r0, [r5]
 2524 0488 B0F85030 		ldrh	r3, [r0, #80]
 2525 048c 621C     		adds	r2, r4, #1
 2526 048e 02EB8202 		add	r2, r2, r2, lsl #2
 2527 0492 15F83260 		ldrb	r6, [r5, r2, lsl #3]	@ zero_extendqisi2
 2528              	.LVL271:
1913:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2529              		.loc 1 1913 35 view .LVU830
 2530 0496 F200     		lsls	r2, r6, #3
 2531 0498 12FA83F3 		uxtah	r3, r2, r3
 2532 049c 0344     		add	r3, r3, r0
 2533 049e B3F80234 		ldrh	r3, [r3, #1026]
1913:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2534              		.loc 1 1913 23 view .LVU831
 2535 04a2 C3F30903 		ubfx	r3, r3, #0, #10
 2536              	.LVL272:
1915:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 2537              		.loc 1 1915 13 is_stmt 1 view .LVU832
ARM GAS  /tmp/ccJPteqL.s 			page 96


1915:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 2538              		.loc 1 1915 19 is_stmt 0 view .LVU833
 2539 04a6 04EB8402 		add	r2, r4, r4, lsl #2
 2540 04aa 05EBC202 		add	r2, r5, r2, lsl #3
 2541 04ae 126C     		ldr	r2, [r2, #64]
1915:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 2542              		.loc 1 1915 16 view .LVU834
 2543 04b0 9A42     		cmp	r2, r3
 2544 04b2 10D9     		bls	.L120
1917:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2545              		.loc 1 1917 15 is_stmt 1 view .LVU835
1917:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2546              		.loc 1 1917 28 is_stmt 0 view .LVU836
 2547 04b4 04EB8407 		add	r7, r4, r4, lsl #2
 2548 04b8 05EBC707 		add	r7, r5, r7, lsl #3
 2549 04bc D21A     		subs	r2, r2, r3
 2550 04be 3A64     		str	r2, [r7, #64]
 2551              	.L121:
1925:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 2552              		.loc 1 1925 13 is_stmt 1 view .LVU837
1925:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 2553              		.loc 1 1925 19 is_stmt 0 view .LVU838
 2554 04c0 04EB8402 		add	r2, r4, r4, lsl #2
 2555 04c4 05EBC202 		add	r2, r5, r2, lsl #3
 2556 04c8 126C     		ldr	r2, [r2, #64]
1925:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             {
 2557              		.loc 1 1925 16 view .LVU839
 2558 04ca 5AB9     		cbnz	r2, .L122
1931:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 2559              		.loc 1 1931 15 is_stmt 1 view .LVU840
 2560 04cc 3146     		mov	r1, r6
 2561              	.LVL273:
1931:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 2562              		.loc 1 1931 15 is_stmt 0 view .LVU841
 2563 04ce 2846     		mov	r0, r5
 2564 04d0 FFF7FEFF 		bl	HAL_PCD_DataInStageCallback
 2565              	.LVL274:
1931:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 2566              		.loc 1 1931 15 view .LVU842
 2567 04d4 63E6     		b	.L96
 2568              	.LVL275:
 2569              	.L120:
1921:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2570              		.loc 1 1921 15 is_stmt 1 view .LVU843
1921:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2571              		.loc 1 1921 28 is_stmt 0 view .LVU844
 2572 04d6 04EB8402 		add	r2, r4, r4, lsl #2
 2573 04da 05EBC202 		add	r2, r5, r2, lsl #3
 2574 04de 0027     		movs	r7, #0
 2575 04e0 1764     		str	r7, [r2, #64]
 2576 04e2 EDE7     		b	.L121
 2577              	.L122:
1937:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               ep->xfer_count += TxPctSize;
 2578              		.loc 1 1937 15 is_stmt 1 view .LVU845
1937:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               ep->xfer_count += TxPctSize;
 2579              		.loc 1 1937 17 is_stmt 0 view .LVU846
 2580 04e4 04EB8402 		add	r2, r4, r4, lsl #2
ARM GAS  /tmp/ccJPteqL.s 			page 97


 2581 04e8 05EBC202 		add	r2, r5, r2, lsl #3
 2582 04ec D66B     		ldr	r6, [r2, #60]
1937:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               ep->xfer_count += TxPctSize;
 2583              		.loc 1 1937 29 view .LVU847
 2584 04ee 1E44     		add	r6, r6, r3
 2585 04f0 D663     		str	r6, [r2, #60]
1938:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               (void)USB_EPStartXfer(hpcd->Instance, ep);
 2586              		.loc 1 1938 15 is_stmt 1 view .LVU848
1938:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               (void)USB_EPStartXfer(hpcd->Instance, ep);
 2587              		.loc 1 1938 17 is_stmt 0 view .LVU849
 2588 04f2 526C     		ldr	r2, [r2, #68]
1938:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               (void)USB_EPStartXfer(hpcd->Instance, ep);
 2589              		.loc 1 1938 30 view .LVU850
 2590 04f4 04EB8404 		add	r4, r4, r4, lsl #2
 2591 04f8 05EBC404 		add	r4, r5, r4, lsl #3
 2592 04fc 1344     		add	r3, r3, r2
 2593              	.LVL276:
1938:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****               (void)USB_EPStartXfer(hpcd->Instance, ep);
 2594              		.loc 1 1938 30 view .LVU851
 2595 04fe 6364     		str	r3, [r4, #68]
1939:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2596              		.loc 1 1939 15 is_stmt 1 view .LVU852
1939:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2597              		.loc 1 1939 21 is_stmt 0 view .LVU853
 2598 0500 FFF7FEFF 		bl	USB_EPStartXfer
 2599              	.LVL277:
1939:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****             }
 2600              		.loc 1 1939 21 view .LVU854
 2601 0504 4BE6     		b	.L96
 2602              	.LVL278:
 2603              	.L119:
1946:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2604              		.loc 1 1946 13 is_stmt 1 view .LVU855
1946:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2605              		.loc 1 1946 19 is_stmt 0 view .LVU856
 2606 0506 3246     		mov	r2, r6
 2607 0508 2846     		mov	r0, r5
 2608 050a FFF7FEFF 		bl	HAL_PCD_EP_DB_Transmit
 2609              	.LVL279:
1946:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****           }
 2610              		.loc 1 1946 19 view .LVU857
 2611 050e 46E6     		b	.L96
 2612              	.LVL280:
 2613              	.L126:
1954:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 2614              		.loc 1 1954 3 is_stmt 1 view .LVU858
1955:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2615              		.loc 1 1955 1 is_stmt 0 view .LVU859
 2616 0510 0020     		movs	r0, #0
 2617 0512 BDE8F081 		pop	{r4, r5, r6, r7, r8, pc}
1955:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2618              		.loc 1 1955 1 view .LVU860
 2619              		.cfi_endproc
 2620              	.LFE361:
 2622              		.section	.text.HAL_PCD_SOFCallback,"ax",%progbits
 2623              		.align	1
 2624              		.weak	HAL_PCD_SOFCallback
ARM GAS  /tmp/ccJPteqL.s 			page 98


 2625              		.syntax unified
 2626              		.thumb
 2627              		.thumb_func
 2629              	HAL_PCD_SOFCallback:
 2630              	.LVL281:
 2631              	.LFB339:
1202:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 2632              		.loc 1 1202 1 is_stmt 1 view -0
 2633              		.cfi_startproc
 2634              		@ args = 0, pretend = 0, frame = 0
 2635              		@ frame_needed = 0, uses_anonymous_args = 0
 2636              		@ link register save eliminated.
1204:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2637              		.loc 1 1204 3 view .LVU862
1209:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2638              		.loc 1 1209 1 is_stmt 0 view .LVU863
 2639 0000 7047     		bx	lr
 2640              		.cfi_endproc
 2641              	.LFE339:
 2643              		.section	.text.HAL_PCD_ResetCallback,"ax",%progbits
 2644              		.align	1
 2645              		.weak	HAL_PCD_ResetCallback
 2646              		.syntax unified
 2647              		.thumb
 2648              		.thumb_func
 2650              	HAL_PCD_ResetCallback:
 2651              	.LVL282:
 2652              	.LFB340:
1217:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 2653              		.loc 1 1217 1 is_stmt 1 view -0
 2654              		.cfi_startproc
 2655              		@ args = 0, pretend = 0, frame = 0
 2656              		@ frame_needed = 0, uses_anonymous_args = 0
 2657              		@ link register save eliminated.
1219:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2658              		.loc 1 1219 3 view .LVU865
1224:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2659              		.loc 1 1224 1 is_stmt 0 view .LVU866
 2660 0000 7047     		bx	lr
 2661              		.cfi_endproc
 2662              	.LFE340:
 2664              		.section	.text.HAL_PCD_SuspendCallback,"ax",%progbits
 2665              		.align	1
 2666              		.weak	HAL_PCD_SuspendCallback
 2667              		.syntax unified
 2668              		.thumb
 2669              		.thumb_func
 2671              	HAL_PCD_SuspendCallback:
 2672              	.LVL283:
 2673              	.LFB341:
1232:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 2674              		.loc 1 1232 1 is_stmt 1 view -0
 2675              		.cfi_startproc
 2676              		@ args = 0, pretend = 0, frame = 0
 2677              		@ frame_needed = 0, uses_anonymous_args = 0
 2678              		@ link register save eliminated.
1234:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 99


 2679              		.loc 1 1234 3 view .LVU868
1239:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2680              		.loc 1 1239 1 is_stmt 0 view .LVU869
 2681 0000 7047     		bx	lr
 2682              		.cfi_endproc
 2683              	.LFE341:
 2685              		.section	.text.HAL_PCD_ResumeCallback,"ax",%progbits
 2686              		.align	1
 2687              		.weak	HAL_PCD_ResumeCallback
 2688              		.syntax unified
 2689              		.thumb
 2690              		.thumb_func
 2692              	HAL_PCD_ResumeCallback:
 2693              	.LVL284:
 2694              	.LFB342:
1247:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 2695              		.loc 1 1247 1 is_stmt 1 view -0
 2696              		.cfi_startproc
 2697              		@ args = 0, pretend = 0, frame = 0
 2698              		@ frame_needed = 0, uses_anonymous_args = 0
 2699              		@ link register save eliminated.
1249:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2700              		.loc 1 1249 3 view .LVU871
1254:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2701              		.loc 1 1254 1 is_stmt 0 view .LVU872
 2702 0000 7047     		bx	lr
 2703              		.cfi_endproc
 2704              	.LFE342:
 2706              		.section	.text.HAL_PCD_ISOOUTIncompleteCallback,"ax",%progbits
 2707              		.align	1
 2708              		.weak	HAL_PCD_ISOOUTIncompleteCallback
 2709              		.syntax unified
 2710              		.thumb
 2711              		.thumb_func
 2713              	HAL_PCD_ISOOUTIncompleteCallback:
 2714              	.LVL285:
 2715              	.LFB343:
1263:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 2716              		.loc 1 1263 1 is_stmt 1 view -0
 2717              		.cfi_startproc
 2718              		@ args = 0, pretend = 0, frame = 0
 2719              		@ frame_needed = 0, uses_anonymous_args = 0
 2720              		@ link register save eliminated.
1265:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(epnum);
 2721              		.loc 1 1265 3 view .LVU874
1266:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2722              		.loc 1 1266 3 view .LVU875
1271:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2723              		.loc 1 1271 1 is_stmt 0 view .LVU876
 2724 0000 7047     		bx	lr
 2725              		.cfi_endproc
 2726              	.LFE343:
 2728              		.section	.text.HAL_PCD_ISOINIncompleteCallback,"ax",%progbits
 2729              		.align	1
 2730              		.weak	HAL_PCD_ISOINIncompleteCallback
 2731              		.syntax unified
 2732              		.thumb
ARM GAS  /tmp/ccJPteqL.s 			page 100


 2733              		.thumb_func
 2735              	HAL_PCD_ISOINIncompleteCallback:
 2736              	.LVL286:
 2737              	.LFB344:
1280:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 2738              		.loc 1 1280 1 is_stmt 1 view -0
 2739              		.cfi_startproc
 2740              		@ args = 0, pretend = 0, frame = 0
 2741              		@ frame_needed = 0, uses_anonymous_args = 0
 2742              		@ link register save eliminated.
1282:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(epnum);
 2743              		.loc 1 1282 3 view .LVU878
1283:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2744              		.loc 1 1283 3 view .LVU879
1288:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2745              		.loc 1 1288 1 is_stmt 0 view .LVU880
 2746 0000 7047     		bx	lr
 2747              		.cfi_endproc
 2748              	.LFE344:
 2750              		.section	.text.HAL_PCD_ConnectCallback,"ax",%progbits
 2751              		.align	1
 2752              		.weak	HAL_PCD_ConnectCallback
 2753              		.syntax unified
 2754              		.thumb
 2755              		.thumb_func
 2757              	HAL_PCD_ConnectCallback:
 2758              	.LVL287:
 2759              	.LFB345:
1296:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 2760              		.loc 1 1296 1 is_stmt 1 view -0
 2761              		.cfi_startproc
 2762              		@ args = 0, pretend = 0, frame = 0
 2763              		@ frame_needed = 0, uses_anonymous_args = 0
 2764              		@ link register save eliminated.
1298:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2765              		.loc 1 1298 3 view .LVU882
1303:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2766              		.loc 1 1303 1 is_stmt 0 view .LVU883
 2767 0000 7047     		bx	lr
 2768              		.cfi_endproc
 2769              	.LFE345:
 2771              		.section	.text.HAL_PCD_DisconnectCallback,"ax",%progbits
 2772              		.align	1
 2773              		.weak	HAL_PCD_DisconnectCallback
 2774              		.syntax unified
 2775              		.thumb
 2776              		.thumb_func
 2778              	HAL_PCD_DisconnectCallback:
 2779              	.LVL288:
 2780              	.LFB346:
1311:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 2781              		.loc 1 1311 1 is_stmt 1 view -0
 2782              		.cfi_startproc
 2783              		@ args = 0, pretend = 0, frame = 0
 2784              		@ frame_needed = 0, uses_anonymous_args = 0
 2785              		@ link register save eliminated.
1313:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 101


 2786              		.loc 1 1313 3 view .LVU885
1318:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2787              		.loc 1 1318 1 is_stmt 0 view .LVU886
 2788 0000 7047     		bx	lr
 2789              		.cfi_endproc
 2790              	.LFE346:
 2792              		.section	.text.HAL_PCD_DevConnect,"ax",%progbits
 2793              		.align	1
 2794              		.global	HAL_PCD_DevConnect
 2795              		.syntax unified
 2796              		.thumb
 2797              		.thumb_func
 2799              	HAL_PCD_DevConnect:
 2800              	.LVL289:
 2801              	.LFB347:
1345:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 2802              		.loc 1 1345 1 is_stmt 1 view -0
 2803              		.cfi_startproc
 2804              		@ args = 0, pretend = 0, frame = 0
 2805              		@ frame_needed = 0, uses_anonymous_args = 0
1346:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevConnect(hpcd->Instance);
 2806              		.loc 1 1346 3 view .LVU888
1346:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevConnect(hpcd->Instance);
 2807              		.loc 1 1346 3 view .LVU889
 2808 0000 90F8A832 		ldrb	r3, [r0, #680]	@ zero_extendqisi2
 2809 0004 012B     		cmp	r3, #1
 2810 0006 0BD0     		beq	.L141
1345:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 2811              		.loc 1 1345 1 is_stmt 0 discriminator 2 view .LVU890
 2812 0008 10B5     		push	{r4, lr}
 2813              	.LCFI13:
 2814              		.cfi_def_cfa_offset 8
 2815              		.cfi_offset 4, -8
 2816              		.cfi_offset 14, -4
 2817 000a 0446     		mov	r4, r0
1346:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevConnect(hpcd->Instance);
 2818              		.loc 1 1346 3 is_stmt 1 discriminator 2 view .LVU891
 2819 000c 0123     		movs	r3, #1
 2820 000e 80F8A832 		strb	r3, [r0, #680]
1346:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevConnect(hpcd->Instance);
 2821              		.loc 1 1346 3 discriminator 2 view .LVU892
1347:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 2822              		.loc 1 1347 3 discriminator 2 view .LVU893
1347:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 2823              		.loc 1 1347 9 is_stmt 0 discriminator 2 view .LVU894
 2824 0012 0068     		ldr	r0, [r0]
 2825              	.LVL290:
1347:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 2826              		.loc 1 1347 9 discriminator 2 view .LVU895
 2827 0014 FFF7FEFF 		bl	USB_DevConnect
 2828              	.LVL291:
1348:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2829              		.loc 1 1348 3 is_stmt 1 discriminator 2 view .LVU896
1348:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2830              		.loc 1 1348 3 discriminator 2 view .LVU897
 2831 0018 0020     		movs	r0, #0
 2832 001a 84F8A802 		strb	r0, [r4, #680]
ARM GAS  /tmp/ccJPteqL.s 			page 102


1348:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2833              		.loc 1 1348 3 discriminator 2 view .LVU898
1350:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 2834              		.loc 1 1350 3 discriminator 2 view .LVU899
1351:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2835              		.loc 1 1351 1 is_stmt 0 discriminator 2 view .LVU900
 2836 001e 10BD     		pop	{r4, pc}
 2837              	.LVL292:
 2838              	.L141:
 2839              	.LCFI14:
 2840              		.cfi_def_cfa_offset 0
 2841              		.cfi_restore 4
 2842              		.cfi_restore 14
1346:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevConnect(hpcd->Instance);
 2843              		.loc 1 1346 3 view .LVU901
 2844 0020 0220     		movs	r0, #2
 2845              	.LVL293:
1351:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2846              		.loc 1 1351 1 view .LVU902
 2847 0022 7047     		bx	lr
 2848              		.cfi_endproc
 2849              	.LFE347:
 2851              		.section	.text.HAL_PCD_DevDisconnect,"ax",%progbits
 2852              		.align	1
 2853              		.global	HAL_PCD_DevDisconnect
 2854              		.syntax unified
 2855              		.thumb
 2856              		.thumb_func
 2858              	HAL_PCD_DevDisconnect:
 2859              	.LVL294:
 2860              	.LFB348:
1359:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 2861              		.loc 1 1359 1 is_stmt 1 view -0
 2862              		.cfi_startproc
 2863              		@ args = 0, pretend = 0, frame = 0
 2864              		@ frame_needed = 0, uses_anonymous_args = 0
1360:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevDisconnect(hpcd->Instance);
 2865              		.loc 1 1360 3 view .LVU904
1360:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevDisconnect(hpcd->Instance);
 2866              		.loc 1 1360 3 view .LVU905
 2867 0000 90F8A832 		ldrb	r3, [r0, #680]	@ zero_extendqisi2
 2868 0004 012B     		cmp	r3, #1
 2869 0006 0BD0     		beq	.L148
1359:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 2870              		.loc 1 1359 1 is_stmt 0 discriminator 2 view .LVU906
 2871 0008 10B5     		push	{r4, lr}
 2872              	.LCFI15:
 2873              		.cfi_def_cfa_offset 8
 2874              		.cfi_offset 4, -8
 2875              		.cfi_offset 14, -4
 2876 000a 0446     		mov	r4, r0
1360:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevDisconnect(hpcd->Instance);
 2877              		.loc 1 1360 3 is_stmt 1 discriminator 2 view .LVU907
 2878 000c 0123     		movs	r3, #1
 2879 000e 80F8A832 		strb	r3, [r0, #680]
1360:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevDisconnect(hpcd->Instance);
 2880              		.loc 1 1360 3 discriminator 2 view .LVU908
ARM GAS  /tmp/ccJPteqL.s 			page 103


1361:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 2881              		.loc 1 1361 3 discriminator 2 view .LVU909
1361:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 2882              		.loc 1 1361 9 is_stmt 0 discriminator 2 view .LVU910
 2883 0012 0068     		ldr	r0, [r0]
 2884              	.LVL295:
1361:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 2885              		.loc 1 1361 9 discriminator 2 view .LVU911
 2886 0014 FFF7FEFF 		bl	USB_DevDisconnect
 2887              	.LVL296:
1362:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2888              		.loc 1 1362 3 is_stmt 1 discriminator 2 view .LVU912
1362:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2889              		.loc 1 1362 3 discriminator 2 view .LVU913
 2890 0018 0020     		movs	r0, #0
 2891 001a 84F8A802 		strb	r0, [r4, #680]
1362:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2892              		.loc 1 1362 3 discriminator 2 view .LVU914
1364:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 2893              		.loc 1 1364 3 discriminator 2 view .LVU915
1365:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2894              		.loc 1 1365 1 is_stmt 0 discriminator 2 view .LVU916
 2895 001e 10BD     		pop	{r4, pc}
 2896              	.LVL297:
 2897              	.L148:
 2898              	.LCFI16:
 2899              		.cfi_def_cfa_offset 0
 2900              		.cfi_restore 4
 2901              		.cfi_restore 14
1360:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DevDisconnect(hpcd->Instance);
 2902              		.loc 1 1360 3 view .LVU917
 2903 0020 0220     		movs	r0, #2
 2904              	.LVL298:
1365:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2905              		.loc 1 1365 1 view .LVU918
 2906 0022 7047     		bx	lr
 2907              		.cfi_endproc
 2908              	.LFE348:
 2910              		.section	.text.HAL_PCD_SetAddress,"ax",%progbits
 2911              		.align	1
 2912              		.global	HAL_PCD_SetAddress
 2913              		.syntax unified
 2914              		.thumb
 2915              		.thumb_func
 2917              	HAL_PCD_SetAddress:
 2918              	.LVL299:
 2919              	.LFB349:
1374:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 2920              		.loc 1 1374 1 is_stmt 1 view -0
 2921              		.cfi_startproc
 2922              		@ args = 0, pretend = 0, frame = 0
 2923              		@ frame_needed = 0, uses_anonymous_args = 0
1375:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->USB_Address = address;
 2924              		.loc 1 1375 3 view .LVU920
1375:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->USB_Address = address;
 2925              		.loc 1 1375 3 view .LVU921
 2926 0000 90F8A832 		ldrb	r3, [r0, #680]	@ zero_extendqisi2
ARM GAS  /tmp/ccJPteqL.s 			page 104


 2927 0004 012B     		cmp	r3, #1
 2928 0006 0DD0     		beq	.L155
1374:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_LOCK(hpcd);
 2929              		.loc 1 1374 1 is_stmt 0 discriminator 2 view .LVU922
 2930 0008 10B5     		push	{r4, lr}
 2931              	.LCFI17:
 2932              		.cfi_def_cfa_offset 8
 2933              		.cfi_offset 4, -8
 2934              		.cfi_offset 14, -4
 2935 000a 0446     		mov	r4, r0
1375:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->USB_Address = address;
 2936              		.loc 1 1375 3 is_stmt 1 discriminator 2 view .LVU923
 2937 000c 0123     		movs	r3, #1
 2938 000e 80F8A832 		strb	r3, [r0, #680]
1375:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->USB_Address = address;
 2939              		.loc 1 1375 3 discriminator 2 view .LVU924
1376:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_SetDevAddress(hpcd->Instance, address);
 2940              		.loc 1 1376 3 discriminator 2 view .LVU925
1376:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_SetDevAddress(hpcd->Instance, address);
 2941              		.loc 1 1376 21 is_stmt 0 discriminator 2 view .LVU926
 2942 0012 80F82410 		strb	r1, [r0, #36]
1377:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 2943              		.loc 1 1377 3 is_stmt 1 discriminator 2 view .LVU927
1377:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 2944              		.loc 1 1377 9 is_stmt 0 discriminator 2 view .LVU928
 2945 0016 0068     		ldr	r0, [r0]
 2946              	.LVL300:
1377:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 2947              		.loc 1 1377 9 discriminator 2 view .LVU929
 2948 0018 FFF7FEFF 		bl	USB_SetDevAddress
 2949              	.LVL301:
1378:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2950              		.loc 1 1378 3 is_stmt 1 discriminator 2 view .LVU930
1378:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2951              		.loc 1 1378 3 discriminator 2 view .LVU931
 2952 001c 0020     		movs	r0, #0
 2953 001e 84F8A802 		strb	r0, [r4, #680]
1378:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2954              		.loc 1 1378 3 discriminator 2 view .LVU932
1380:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 2955              		.loc 1 1380 3 discriminator 2 view .LVU933
1381:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 2956              		.loc 1 1381 1 is_stmt 0 discriminator 2 view .LVU934
 2957 0022 10BD     		pop	{r4, pc}
 2958              	.LVL302:
 2959              	.L155:
 2960              	.LCFI18:
 2961              		.cfi_def_cfa_offset 0
 2962              		.cfi_restore 4
 2963              		.cfi_restore 14
1375:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   hpcd->USB_Address = address;
 2964              		.loc 1 1375 3 view .LVU935
 2965 0024 0220     		movs	r0, #2
 2966              	.LVL303:
1381:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 2967              		.loc 1 1381 1 view .LVU936
 2968 0026 7047     		bx	lr
ARM GAS  /tmp/ccJPteqL.s 			page 105


 2969              		.cfi_endproc
 2970              	.LFE349:
 2972              		.section	.text.HAL_PCD_IRQHandler,"ax",%progbits
 2973              		.align	1
 2974              		.global	HAL_PCD_IRQHandler
 2975              		.syntax unified
 2976              		.thumb
 2977              		.thumb_func
 2979              	HAL_PCD_IRQHandler:
 2980              	.LVL304:
 2981              	.LFB335:
1009:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint32_t wIstr = USB_ReadInterrupts(hpcd->Instance);
 2982              		.loc 1 1009 1 is_stmt 1 view -0
 2983              		.cfi_startproc
 2984              		@ args = 0, pretend = 0, frame = 0
 2985              		@ frame_needed = 0, uses_anonymous_args = 0
1009:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   uint32_t wIstr = USB_ReadInterrupts(hpcd->Instance);
 2986              		.loc 1 1009 1 is_stmt 0 view .LVU938
 2987 0000 10B5     		push	{r4, lr}
 2988              	.LCFI19:
 2989              		.cfi_def_cfa_offset 8
 2990              		.cfi_offset 4, -8
 2991              		.cfi_offset 14, -4
 2992 0002 0446     		mov	r4, r0
1010:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2993              		.loc 1 1010 3 is_stmt 1 view .LVU939
1010:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2994              		.loc 1 1010 20 is_stmt 0 view .LVU940
 2995 0004 0068     		ldr	r0, [r0]
 2996              	.LVL305:
1010:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 2997              		.loc 1 1010 20 view .LVU941
 2998 0006 FFF7FEFF 		bl	USB_ReadInterrupts
 2999              	.LVL306:
1012:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3000              		.loc 1 1012 3 is_stmt 1 view .LVU942
1012:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3001              		.loc 1 1012 6 is_stmt 0 view .LVU943
 3002 000a 10F4004F 		tst	r0, #32768
 3003 000e 23D1     		bne	.L174
1021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3004              		.loc 1 1021 3 is_stmt 1 view .LVU944
1021:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3005              		.loc 1 1021 6 is_stmt 0 view .LVU945
 3006 0010 10F4806F 		tst	r0, #1024
 3007 0014 24D1     		bne	.L175
1036:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3008              		.loc 1 1036 3 is_stmt 1 view .LVU946
1036:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3009              		.loc 1 1036 6 is_stmt 0 view .LVU947
 3010 0016 10F4804F 		tst	r0, #16384
 3011 001a 32D1     		bne	.L176
1043:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3012              		.loc 1 1043 3 is_stmt 1 view .LVU948
1043:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3013              		.loc 1 1043 6 is_stmt 0 view .LVU949
 3014 001c 10F4005F 		tst	r0, #8192
ARM GAS  /tmp/ccJPteqL.s 			page 106


 3015 0020 39D1     		bne	.L177
1050:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3016              		.loc 1 1050 3 is_stmt 1 view .LVU950
1050:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3017              		.loc 1 1050 6 is_stmt 0 view .LVU951
 3018 0022 10F4805F 		tst	r0, #4096
 3019 0026 40D1     		bne	.L178
1076:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3020              		.loc 1 1076 3 is_stmt 1 view .LVU952
1076:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3021              		.loc 1 1076 6 is_stmt 0 view .LVU953
 3022 0028 10F4006F 		tst	r0, #2048
 3023 002c 67D1     		bne	.L179
1096:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3024              		.loc 1 1096 3 is_stmt 1 view .LVU954
1096:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3025              		.loc 1 1096 6 is_stmt 0 view .LVU955
 3026 002e 10F0800F 		tst	r0, #128
 3027 0032 40F08180 		bne	.L180
1125:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3028              		.loc 1 1125 3 is_stmt 1 view .LVU956
1125:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3029              		.loc 1 1125 6 is_stmt 0 view .LVU957
 3030 0036 10F4007F 		tst	r0, #512
 3031 003a 40F0AD80 		bne	.L181
1138:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3032              		.loc 1 1138 3 is_stmt 1 view .LVU958
1138:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3033              		.loc 1 1138 6 is_stmt 0 view .LVU959
 3034 003e 10F4807F 		tst	r0, #256
 3035 0042 27D0     		beq	.L160
1141:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3036              		.loc 1 1141 5 is_stmt 1 view .LVU960
 3037 0044 2268     		ldr	r2, [r4]
 3038 0046 B2F84430 		ldrh	r3, [r2, #68]
 3039 004a 9BB2     		uxth	r3, r3
 3040 004c 23F48073 		bic	r3, r3, #256
 3041 0050 9BB2     		uxth	r3, r3
 3042 0052 A2F84430 		strh	r3, [r2, #68]	@ movhi
1143:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3043              		.loc 1 1143 5 view .LVU961
 3044 0056 1DE0     		b	.L160
 3045              	.L174:
1016:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3046              		.loc 1 1016 5 view .LVU962
1016:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3047              		.loc 1 1016 11 is_stmt 0 view .LVU963
 3048 0058 2046     		mov	r0, r4
 3049              	.LVL307:
1016:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3050              		.loc 1 1016 11 view .LVU964
 3051 005a FFF7FEFF 		bl	PCD_EP_ISR_Handler
 3052              	.LVL308:
1018:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3053              		.loc 1 1018 5 is_stmt 1 view .LVU965
 3054 005e 19E0     		b	.L160
 3055              	.LVL309:
ARM GAS  /tmp/ccJPteqL.s 			page 107


 3056              	.L175:
1023:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3057              		.loc 1 1023 5 view .LVU966
 3058 0060 2268     		ldr	r2, [r4]
 3059 0062 B2F84430 		ldrh	r3, [r2, #68]
 3060 0066 9BB2     		uxth	r3, r3
 3061 0068 23F48063 		bic	r3, r3, #1024
 3062 006c 9BB2     		uxth	r3, r3
 3063 006e A2F84430 		strh	r3, [r2, #68]	@ movhi
1028:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3064              		.loc 1 1028 5 view .LVU967
 3065 0072 2046     		mov	r0, r4
 3066              	.LVL310:
1028:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3067              		.loc 1 1028 5 is_stmt 0 view .LVU968
 3068 0074 FFF7FEFF 		bl	HAL_PCD_ResetCallback
 3069              	.LVL311:
1031:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3070              		.loc 1 1031 5 is_stmt 1 view .LVU969
1031:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3071              		.loc 1 1031 11 is_stmt 0 view .LVU970
 3072 0078 0021     		movs	r1, #0
 3073 007a 2046     		mov	r0, r4
 3074 007c FFF7FEFF 		bl	HAL_PCD_SetAddress
 3075              	.LVL312:
1033:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3076              		.loc 1 1033 5 is_stmt 1 view .LVU971
 3077 0080 08E0     		b	.L160
 3078              	.LVL313:
 3079              	.L176:
1038:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3080              		.loc 1 1038 5 view .LVU972
 3081 0082 2268     		ldr	r2, [r4]
 3082 0084 B2F84430 		ldrh	r3, [r2, #68]
 3083 0088 9BB2     		uxth	r3, r3
 3084 008a 23F48043 		bic	r3, r3, #16384
 3085 008e 9BB2     		uxth	r3, r3
 3086 0090 A2F84430 		strh	r3, [r2, #68]	@ movhi
1040:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3087              		.loc 1 1040 5 view .LVU973
 3088              	.LVL314:
 3089              	.L160:
1145:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3090              		.loc 1 1145 1 is_stmt 0 view .LVU974
 3091 0094 10BD     		pop	{r4, pc}
 3092              	.LVL315:
 3093              	.L177:
1045:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3094              		.loc 1 1045 5 is_stmt 1 view .LVU975
 3095 0096 2268     		ldr	r2, [r4]
 3096 0098 B2F84430 		ldrh	r3, [r2, #68]
 3097 009c 9BB2     		uxth	r3, r3
 3098 009e 23F40053 		bic	r3, r3, #8192
 3099 00a2 9BB2     		uxth	r3, r3
 3100 00a4 A2F84430 		strh	r3, [r2, #68]	@ movhi
1047:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3101              		.loc 1 1047 5 view .LVU976
ARM GAS  /tmp/ccJPteqL.s 			page 108


 3102 00a8 F4E7     		b	.L160
 3103              	.L178:
1052:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->Instance->CNTR &= (uint16_t) ~(USB_CNTR_FSUSP);
 3104              		.loc 1 1052 5 view .LVU977
1052:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->Instance->CNTR &= (uint16_t) ~(USB_CNTR_FSUSP);
 3105              		.loc 1 1052 9 is_stmt 0 view .LVU978
 3106 00aa 2268     		ldr	r2, [r4]
1052:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->Instance->CNTR &= (uint16_t) ~(USB_CNTR_FSUSP);
 3107              		.loc 1 1052 19 view .LVU979
 3108 00ac B2F84030 		ldrh	r3, [r2, #64]
 3109 00b0 9BB2     		uxth	r3, r3
1052:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     hpcd->Instance->CNTR &= (uint16_t) ~(USB_CNTR_FSUSP);
 3110              		.loc 1 1052 26 view .LVU980
 3111 00b2 23F00403 		bic	r3, r3, #4
 3112 00b6 9BB2     		uxth	r3, r3
 3113 00b8 A2F84030 		strh	r3, [r2, #64]	@ movhi
1053:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3114              		.loc 1 1053 5 is_stmt 1 view .LVU981
1053:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3115              		.loc 1 1053 9 is_stmt 0 view .LVU982
 3116 00bc 2268     		ldr	r2, [r4]
1053:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3117              		.loc 1 1053 19 view .LVU983
 3118 00be B2F84030 		ldrh	r3, [r2, #64]
 3119 00c2 9BB2     		uxth	r3, r3
1053:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3120              		.loc 1 1053 26 view .LVU984
 3121 00c4 23F00803 		bic	r3, r3, #8
 3122 00c8 9BB2     		uxth	r3, r3
 3123 00ca A2F84030 		strh	r3, [r2, #64]	@ movhi
1055:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 3124              		.loc 1 1055 5 is_stmt 1 view .LVU985
1055:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 3125              		.loc 1 1055 13 is_stmt 0 view .LVU986
 3126 00ce 94F8E032 		ldrb	r3, [r4, #736]	@ zero_extendqisi2
1055:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 3127              		.loc 1 1055 8 view .LVU987
 3128 00d2 012B     		cmp	r3, #1
 3129 00d4 0CD0     		beq	.L182
 3130              	.LVL316:
 3131              	.L167:
1068:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3132              		.loc 1 1068 5 is_stmt 1 view .LVU988
 3133 00d6 2046     		mov	r0, r4
 3134 00d8 FFF7FEFF 		bl	HAL_PCD_ResumeCallback
 3135              	.LVL317:
1071:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3136              		.loc 1 1071 5 view .LVU989
 3137 00dc 2268     		ldr	r2, [r4]
 3138 00de B2F84430 		ldrh	r3, [r2, #68]
 3139 00e2 9BB2     		uxth	r3, r3
 3140 00e4 23F48053 		bic	r3, r3, #4096
 3141 00e8 9BB2     		uxth	r3, r3
 3142 00ea A2F84430 		strh	r3, [r2, #68]	@ movhi
1073:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3143              		.loc 1 1073 5 view .LVU990
 3144 00ee D1E7     		b	.L160
ARM GAS  /tmp/ccJPteqL.s 			page 109


 3145              	.LVL318:
 3146              	.L182:
1057:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
 3147              		.loc 1 1057 7 view .LVU991
1057:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
 3148              		.loc 1 1057 23 is_stmt 0 view .LVU992
 3149 00f0 0021     		movs	r1, #0
 3150 00f2 84F8E012 		strb	r1, [r4, #736]
1061:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3151              		.loc 1 1061 7 is_stmt 1 view .LVU993
 3152 00f6 2046     		mov	r0, r4
 3153              	.LVL319:
1061:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3154              		.loc 1 1061 7 is_stmt 0 view .LVU994
 3155 00f8 FFF7FEFF 		bl	HAL_PCDEx_LPM_Callback
 3156              	.LVL320:
 3157 00fc EBE7     		b	.L167
 3158              	.LVL321:
 3159              	.L179:
1079:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3160              		.loc 1 1079 5 is_stmt 1 view .LVU995
1079:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3161              		.loc 1 1079 9 is_stmt 0 view .LVU996
 3162 00fe 2268     		ldr	r2, [r4]
1079:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3163              		.loc 1 1079 19 view .LVU997
 3164 0100 B2F84030 		ldrh	r3, [r2, #64]
 3165 0104 9BB2     		uxth	r3, r3
1079:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3166              		.loc 1 1079 26 view .LVU998
 3167 0106 43F00803 		orr	r3, r3, #8
 3168 010a A2F84030 		strh	r3, [r2, #64]	@ movhi
1082:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3169              		.loc 1 1082 5 is_stmt 1 view .LVU999
 3170 010e 2268     		ldr	r2, [r4]
 3171 0110 B2F84430 		ldrh	r3, [r2, #68]
 3172 0114 9BB2     		uxth	r3, r3
 3173 0116 23F40063 		bic	r3, r3, #2048
 3174 011a 9BB2     		uxth	r3, r3
 3175 011c A2F84430 		strh	r3, [r2, #68]	@ movhi
1084:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3176              		.loc 1 1084 5 view .LVU1000
1084:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3177              		.loc 1 1084 9 is_stmt 0 view .LVU1001
 3178 0120 2268     		ldr	r2, [r4]
1084:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3179              		.loc 1 1084 19 view .LVU1002
 3180 0122 B2F84030 		ldrh	r3, [r2, #64]
 3181 0126 9BB2     		uxth	r3, r3
1084:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3182              		.loc 1 1084 26 view .LVU1003
 3183 0128 43F00403 		orr	r3, r3, #4
 3184 012c A2F84030 		strh	r3, [r2, #64]	@ movhi
1089:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3185              		.loc 1 1089 5 is_stmt 1 view .LVU1004
 3186 0130 2046     		mov	r0, r4
 3187              	.LVL322:
ARM GAS  /tmp/ccJPteqL.s 			page 110


1089:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3188              		.loc 1 1089 5 is_stmt 0 view .LVU1005
 3189 0132 FFF7FEFF 		bl	HAL_PCD_SuspendCallback
 3190              	.LVL323:
1092:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3191              		.loc 1 1092 5 is_stmt 1 view .LVU1006
 3192 0136 ADE7     		b	.L160
 3193              	.LVL324:
 3194              	.L180:
1098:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     if (hpcd->LPM_State == LPM_L0)
 3195              		.loc 1 1098 5 view .LVU1007
 3196 0138 2268     		ldr	r2, [r4]
 3197 013a B2F84430 		ldrh	r3, [r2, #68]
 3198 013e 9BB2     		uxth	r3, r3
 3199 0140 23F08003 		bic	r3, r3, #128
 3200 0144 9BB2     		uxth	r3, r3
 3201 0146 A2F84430 		strh	r3, [r2, #68]	@ movhi
1099:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 3202              		.loc 1 1099 5 view .LVU1008
1099:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 3203              		.loc 1 1099 13 is_stmt 0 view .LVU1009
 3204 014a 94F8E032 		ldrb	r3, [r4, #736]	@ zero_extendqisi2
1099:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     {
 3205              		.loc 1 1099 8 view .LVU1010
 3206 014e FBB9     		cbnz	r3, .L170
1102:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->Instance->CNTR |= (uint16_t)USB_CNTR_FSUSP;
 3207              		.loc 1 1102 7 is_stmt 1 view .LVU1011
1102:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->Instance->CNTR |= (uint16_t)USB_CNTR_FSUSP;
 3208              		.loc 1 1102 11 is_stmt 0 view .LVU1012
 3209 0150 2268     		ldr	r2, [r4]
1102:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->Instance->CNTR |= (uint16_t)USB_CNTR_FSUSP;
 3210              		.loc 1 1102 21 view .LVU1013
 3211 0152 B2F84030 		ldrh	r3, [r2, #64]
 3212 0156 9BB2     		uxth	r3, r3
1102:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->Instance->CNTR |= (uint16_t)USB_CNTR_FSUSP;
 3213              		.loc 1 1102 28 view .LVU1014
 3214 0158 43F00403 		orr	r3, r3, #4
 3215 015c A2F84030 		strh	r3, [r2, #64]	@ movhi
1103:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3216              		.loc 1 1103 7 is_stmt 1 view .LVU1015
1103:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3217              		.loc 1 1103 11 is_stmt 0 view .LVU1016
 3218 0160 2268     		ldr	r2, [r4]
1103:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3219              		.loc 1 1103 21 view .LVU1017
 3220 0162 B2F84030 		ldrh	r3, [r2, #64]
 3221 0166 9BB2     		uxth	r3, r3
1103:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3222              		.loc 1 1103 28 view .LVU1018
 3223 0168 43F00803 		orr	r3, r3, #8
 3224 016c A2F84030 		strh	r3, [r2, #64]	@ movhi
1105:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->BESL = ((uint32_t)hpcd->Instance->LPMCSR & USB_LPMCSR_BESL) >> 2;
 3225              		.loc 1 1105 7 is_stmt 1 view .LVU1019
1105:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****       hpcd->BESL = ((uint32_t)hpcd->Instance->LPMCSR & USB_LPMCSR_BESL) >> 2;
 3226              		.loc 1 1105 23 is_stmt 0 view .LVU1020
 3227 0170 0121     		movs	r1, #1
 3228 0172 84F8E012 		strb	r1, [r4, #736]
ARM GAS  /tmp/ccJPteqL.s 			page 111


1106:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
 3229              		.loc 1 1106 7 is_stmt 1 view .LVU1021
1106:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
 3230              		.loc 1 1106 35 is_stmt 0 view .LVU1022
 3231 0176 2368     		ldr	r3, [r4]
1106:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
 3232              		.loc 1 1106 45 view .LVU1023
 3233 0178 B3F85430 		ldrh	r3, [r3, #84]
1106:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
 3234              		.loc 1 1106 73 view .LVU1024
 3235 017c C3F38D03 		ubfx	r3, r3, #2, #14
 3236 0180 03F03C03 		and	r3, r3, #60
1106:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #if (USE_HAL_PCD_REGISTER_CALLBACKS == 1U)
 3237              		.loc 1 1106 18 view .LVU1025
 3238 0184 C4F8E432 		str	r3, [r4, #740]
1110:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3239              		.loc 1 1110 7 is_stmt 1 view .LVU1026
 3240 0188 2046     		mov	r0, r4
 3241              	.LVL325:
1110:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3242              		.loc 1 1110 7 is_stmt 0 view .LVU1027
 3243 018a FFF7FEFF 		bl	HAL_PCDEx_LPM_Callback
 3244              	.LVL326:
 3245 018e 81E7     		b	.L160
 3246              	.LVL327:
 3247              	.L170:
1118:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3248              		.loc 1 1118 7 is_stmt 1 view .LVU1028
 3249 0190 2046     		mov	r0, r4
 3250              	.LVL328:
1118:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3251              		.loc 1 1118 7 is_stmt 0 view .LVU1029
 3252 0192 FFF7FEFF 		bl	HAL_PCD_SuspendCallback
 3253              	.LVL329:
1122:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3254              		.loc 1 1122 5 is_stmt 1 view .LVU1030
 3255 0196 7DE7     		b	.L160
 3256              	.LVL330:
 3257              	.L181:
1127:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3258              		.loc 1 1127 5 view .LVU1031
 3259 0198 2268     		ldr	r2, [r4]
 3260 019a B2F84430 		ldrh	r3, [r2, #68]
 3261 019e 9BB2     		uxth	r3, r3
 3262 01a0 23F40073 		bic	r3, r3, #512
 3263 01a4 9BB2     		uxth	r3, r3
 3264 01a6 A2F84430 		strh	r3, [r2, #68]	@ movhi
1132:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3265              		.loc 1 1132 5 view .LVU1032
 3266 01aa 2046     		mov	r0, r4
 3267              	.LVL331:
1132:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** #endif /* USE_HAL_PCD_REGISTER_CALLBACKS */
 3268              		.loc 1 1132 5 is_stmt 0 view .LVU1033
 3269 01ac FFF7FEFF 		bl	HAL_PCD_SOFCallback
 3270              	.LVL332:
1135:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3271              		.loc 1 1135 5 is_stmt 1 view .LVU1034
ARM GAS  /tmp/ccJPteqL.s 			page 112


 3272 01b0 70E7     		b	.L160
 3273              		.cfi_endproc
 3274              	.LFE335:
 3276              		.section	.text.HAL_PCD_EP_Open,"ax",%progbits
 3277              		.align	1
 3278              		.global	HAL_PCD_EP_Open
 3279              		.syntax unified
 3280              		.thumb
 3281              		.thumb_func
 3283              	HAL_PCD_EP_Open:
 3284              	.LVL333:
 3285              	.LFB350:
1392:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef  ret = HAL_OK;
 3286              		.loc 1 1392 1 view -0
 3287              		.cfi_startproc
 3288              		@ args = 0, pretend = 0, frame = 0
 3289              		@ frame_needed = 0, uses_anonymous_args = 0
1392:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   HAL_StatusTypeDef  ret = HAL_OK;
 3290              		.loc 1 1392 1 is_stmt 0 view .LVU1036
 3291 0000 10B5     		push	{r4, lr}
 3292              	.LCFI20:
 3293              		.cfi_def_cfa_offset 8
 3294              		.cfi_offset 4, -8
 3295              		.cfi_offset 14, -4
 3296 0002 0446     		mov	r4, r0
 3297 0004 8C46     		mov	ip, r1
1393:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3298              		.loc 1 1393 3 is_stmt 1 view .LVU1037
 3299              	.LVL334:
1394:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3300              		.loc 1 1394 3 view .LVU1038
1396:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3301              		.loc 1 1396 3 view .LVU1039
1396:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3302              		.loc 1 1396 6 is_stmt 0 view .LVU1040
 3303 0006 11F0800F 		tst	r1, #128
 3304 000a 2AD1     		bne	.L191
1403:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3305              		.loc 1 1403 5 is_stmt 1 view .LVU1041
1403:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3306              		.loc 1 1403 32 is_stmt 0 view .LVU1042
 3307 000c 01F00700 		and	r0, r1, #7
 3308              	.LVL335:
1403:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3309              		.loc 1 1403 8 view .LVU1043
 3310 0010 00EB8001 		add	r1, r0, r0, lsl #2
 3311              	.LVL336:
1403:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3312              		.loc 1 1403 8 view .LVU1044
 3313 0014 C900     		lsls	r1, r1, #3
 3314 0016 01F5B47E 		add	lr, r1, #360
 3315 001a 04EB0E01 		add	r1, r4, lr
 3316              	.LVL337:
1404:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3317              		.loc 1 1404 5 is_stmt 1 view .LVU1045
1404:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3318              		.loc 1 1404 15 is_stmt 0 view .LVU1046
ARM GAS  /tmp/ccJPteqL.s 			page 113


 3319 001e 00EB8000 		add	r0, r0, r0, lsl #2
 3320 0022 04EBC000 		add	r0, r4, r0, lsl #3
 3321 0026 4FF0000E 		mov	lr, #0
 3322 002a 80F869E1 		strb	lr, [r0, #361]
 3323              	.L185:
1407:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->maxpacket = ep_mps;
 3324              		.loc 1 1407 3 is_stmt 1 view .LVU1047
1407:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->maxpacket = ep_mps;
 3325              		.loc 1 1407 21 is_stmt 0 view .LVU1048
 3326 002e 0CF0070C 		and	ip, ip, #7
1407:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->maxpacket = ep_mps;
 3327              		.loc 1 1407 11 view .LVU1049
 3328 0032 81F800C0 		strb	ip, [r1]
1408:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->type = ep_type;
 3329              		.loc 1 1408 3 is_stmt 1 view .LVU1050
1408:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->type = ep_type;
 3330              		.loc 1 1408 17 is_stmt 0 view .LVU1051
 3331 0036 0A61     		str	r2, [r1, #16]
1409:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3332              		.loc 1 1409 3 is_stmt 1 view .LVU1052
1409:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3333              		.loc 1 1409 12 is_stmt 0 view .LVU1053
 3334 0038 CB70     		strb	r3, [r1, #3]
1411:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3335              		.loc 1 1411 3 is_stmt 1 view .LVU1054
1411:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3336              		.loc 1 1411 9 is_stmt 0 view .LVU1055
 3337 003a 4A78     		ldrb	r2, [r1, #1]	@ zero_extendqisi2
 3338              	.LVL338:
1411:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3339              		.loc 1 1411 6 view .LVU1056
 3340 003c 0AB1     		cbz	r2, .L186
1414:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3341              		.loc 1 1414 5 is_stmt 1 view .LVU1057
1414:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3342              		.loc 1 1414 21 is_stmt 0 view .LVU1058
 3343 003e A1F80EC0 		strh	ip, [r1, #14]	@ movhi
 3344              	.L186:
1417:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3345              		.loc 1 1417 3 is_stmt 1 view .LVU1059
1417:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3346              		.loc 1 1417 6 is_stmt 0 view .LVU1060
 3347 0042 022B     		cmp	r3, #2
 3348 0044 19D0     		beq	.L192
 3349              	.LVL339:
 3350              	.L187:
1422:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_ActivateEndpoint(hpcd->Instance, ep);
 3351              		.loc 1 1422 3 is_stmt 1 view .LVU1061
1422:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_ActivateEndpoint(hpcd->Instance, ep);
 3352              		.loc 1 1422 3 view .LVU1062
 3353 0046 94F8A832 		ldrb	r3, [r4, #680]	@ zero_extendqisi2
 3354 004a 012B     		cmp	r3, #1
 3355 004c 18D0     		beq	.L189
1422:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_ActivateEndpoint(hpcd->Instance, ep);
 3356              		.loc 1 1422 3 discriminator 2 view .LVU1063
 3357 004e 0123     		movs	r3, #1
 3358 0050 84F8A832 		strb	r3, [r4, #680]
ARM GAS  /tmp/ccJPteqL.s 			page 114


 3359              	.LVL340:
1422:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_ActivateEndpoint(hpcd->Instance, ep);
 3360              		.loc 1 1422 3 discriminator 2 view .LVU1064
1423:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 3361              		.loc 1 1423 3 discriminator 2 view .LVU1065
1423:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 3362              		.loc 1 1423 9 is_stmt 0 discriminator 2 view .LVU1066
 3363 0054 2068     		ldr	r0, [r4]
 3364 0056 FFF7FEFF 		bl	USB_ActivateEndpoint
 3365              	.LVL341:
1424:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3366              		.loc 1 1424 3 is_stmt 1 discriminator 2 view .LVU1067
1424:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3367              		.loc 1 1424 3 discriminator 2 view .LVU1068
 3368 005a 0020     		movs	r0, #0
 3369 005c 84F8A802 		strb	r0, [r4, #680]
1424:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3370              		.loc 1 1424 3 discriminator 2 view .LVU1069
1426:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 3371              		.loc 1 1426 3 discriminator 2 view .LVU1070
 3372              	.L188:
1427:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3373              		.loc 1 1427 1 is_stmt 0 view .LVU1071
 3374 0060 10BD     		pop	{r4, pc}
 3375              	.LVL342:
 3376              	.L191:
1398:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3377              		.loc 1 1398 5 is_stmt 1 view .LVU1072
1398:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3378              		.loc 1 1398 31 is_stmt 0 view .LVU1073
 3379 0062 01F00700 		and	r0, r1, #7
 3380              	.LVL343:
1398:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3381              		.loc 1 1398 8 view .LVU1074
 3382 0066 0130     		adds	r0, r0, #1
 3383 0068 00EB8001 		add	r1, r0, r0, lsl #2
 3384              	.LVL344:
1398:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3385              		.loc 1 1398 8 view .LVU1075
 3386 006c 04EBC101 		add	r1, r4, r1, lsl #3
 3387              	.LVL345:
1399:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3388              		.loc 1 1399 5 is_stmt 1 view .LVU1076
1399:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3389              		.loc 1 1399 15 is_stmt 0 view .LVU1077
 3390 0070 4FF0010E 		mov	lr, #1
 3391 0074 81F801E0 		strb	lr, [r1, #1]
 3392 0078 D9E7     		b	.L185
 3393              	.LVL346:
 3394              	.L192:
1419:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3395              		.loc 1 1419 5 is_stmt 1 view .LVU1078
1419:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3396              		.loc 1 1419 24 is_stmt 0 view .LVU1079
 3397 007a 0023     		movs	r3, #0
 3398              	.LVL347:
1419:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
ARM GAS  /tmp/ccJPteqL.s 			page 115


 3399              		.loc 1 1419 24 view .LVU1080
 3400 007c 0B71     		strb	r3, [r1, #4]
 3401 007e E2E7     		b	.L187
 3402              	.L189:
1422:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_ActivateEndpoint(hpcd->Instance, ep);
 3403              		.loc 1 1422 3 view .LVU1081
 3404 0080 0220     		movs	r0, #2
 3405 0082 EDE7     		b	.L188
 3406              		.cfi_endproc
 3407              	.LFE350:
 3409              		.section	.text.HAL_PCD_EP_Close,"ax",%progbits
 3410              		.align	1
 3411              		.global	HAL_PCD_EP_Close
 3412              		.syntax unified
 3413              		.thumb
 3414              		.thumb_func
 3416              	HAL_PCD_EP_Close:
 3417              	.LVL348:
 3418              	.LFB351:
1436:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3419              		.loc 1 1436 1 is_stmt 1 view -0
 3420              		.cfi_startproc
 3421              		@ args = 0, pretend = 0, frame = 0
 3422              		@ frame_needed = 0, uses_anonymous_args = 0
1436:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3423              		.loc 1 1436 1 is_stmt 0 view .LVU1083
 3424 0000 10B5     		push	{r4, lr}
 3425              	.LCFI21:
 3426              		.cfi_def_cfa_offset 8
 3427              		.cfi_offset 4, -8
 3428              		.cfi_offset 14, -4
 3429 0002 0446     		mov	r4, r0
 3430 0004 0B46     		mov	r3, r1
1437:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3431              		.loc 1 1437 3 is_stmt 1 view .LVU1084
1439:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3432              		.loc 1 1439 3 view .LVU1085
1439:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3433              		.loc 1 1439 6 is_stmt 0 view .LVU1086
 3434 0006 11F0800F 		tst	r1, #128
 3435 000a 1FD1     		bne	.L199
1446:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3436              		.loc 1 1446 5 is_stmt 1 view .LVU1087
1446:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3437              		.loc 1 1446 32 is_stmt 0 view .LVU1088
 3438 000c 01F00702 		and	r2, r1, #7
1446:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3439              		.loc 1 1446 8 view .LVU1089
 3440 0010 02EB8201 		add	r1, r2, r2, lsl #2
 3441              	.LVL349:
1446:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3442              		.loc 1 1446 8 view .LVU1090
 3443 0014 C900     		lsls	r1, r1, #3
 3444 0016 01F5B471 		add	r1, r1, #360
 3445 001a 0144     		add	r1, r1, r0
 3446              	.LVL350:
1447:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
ARM GAS  /tmp/ccJPteqL.s 			page 116


 3447              		.loc 1 1447 5 is_stmt 1 view .LVU1091
1447:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3448              		.loc 1 1447 15 is_stmt 0 view .LVU1092
 3449 001c 02EB8202 		add	r2, r2, r2, lsl #2
 3450 0020 00EBC202 		add	r2, r0, r2, lsl #3
 3451 0024 0020     		movs	r0, #0
 3452              	.LVL351:
1447:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3453              		.loc 1 1447 15 view .LVU1093
 3454 0026 82F86901 		strb	r0, [r2, #361]
 3455              	.L195:
1449:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3456              		.loc 1 1449 3 is_stmt 1 view .LVU1094
1449:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3457              		.loc 1 1449 23 is_stmt 0 view .LVU1095
 3458 002a 03F00703 		and	r3, r3, #7
1449:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3459              		.loc 1 1449 13 view .LVU1096
 3460 002e 0B70     		strb	r3, [r1]
1451:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DeactivateEndpoint(hpcd->Instance, ep);
 3461              		.loc 1 1451 3 is_stmt 1 view .LVU1097
1451:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DeactivateEndpoint(hpcd->Instance, ep);
 3462              		.loc 1 1451 3 view .LVU1098
 3463 0030 94F8A832 		ldrb	r3, [r4, #680]	@ zero_extendqisi2
 3464 0034 012B     		cmp	r3, #1
 3465 0036 13D0     		beq	.L197
1451:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DeactivateEndpoint(hpcd->Instance, ep);
 3466              		.loc 1 1451 3 discriminator 2 view .LVU1099
 3467 0038 0123     		movs	r3, #1
 3468 003a 84F8A832 		strb	r3, [r4, #680]
1451:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DeactivateEndpoint(hpcd->Instance, ep);
 3469              		.loc 1 1451 3 discriminator 2 view .LVU1100
1452:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 3470              		.loc 1 1452 3 discriminator 2 view .LVU1101
1452:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 3471              		.loc 1 1452 9 is_stmt 0 discriminator 2 view .LVU1102
 3472 003e 2068     		ldr	r0, [r4]
 3473 0040 FFF7FEFF 		bl	USB_DeactivateEndpoint
 3474              	.LVL352:
1453:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
 3475              		.loc 1 1453 3 is_stmt 1 discriminator 2 view .LVU1103
1453:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
 3476              		.loc 1 1453 3 discriminator 2 view .LVU1104
 3477 0044 0020     		movs	r0, #0
 3478 0046 84F8A802 		strb	r0, [r4, #680]
1453:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return HAL_OK;
 3479              		.loc 1 1453 3 discriminator 2 view .LVU1105
1454:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 3480              		.loc 1 1454 3 discriminator 2 view .LVU1106
 3481              	.L196:
1455:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3482              		.loc 1 1455 1 is_stmt 0 view .LVU1107
 3483 004a 10BD     		pop	{r4, pc}
 3484              	.LVL353:
 3485              	.L199:
1441:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3486              		.loc 1 1441 5 is_stmt 1 view .LVU1108
ARM GAS  /tmp/ccJPteqL.s 			page 117


1441:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3487              		.loc 1 1441 31 is_stmt 0 view .LVU1109
 3488 004c 01F00702 		and	r2, r1, #7
1441:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3489              		.loc 1 1441 8 view .LVU1110
 3490 0050 0132     		adds	r2, r2, #1
 3491 0052 02EB8201 		add	r1, r2, r2, lsl #2
 3492              	.LVL354:
1441:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3493              		.loc 1 1441 8 view .LVU1111
 3494 0056 00EBC101 		add	r1, r0, r1, lsl #3
 3495              	.LVL355:
1442:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3496              		.loc 1 1442 5 is_stmt 1 view .LVU1112
1442:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3497              		.loc 1 1442 15 is_stmt 0 view .LVU1113
 3498 005a 0120     		movs	r0, #1
 3499              	.LVL356:
1442:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3500              		.loc 1 1442 15 view .LVU1114
 3501 005c 4870     		strb	r0, [r1, #1]
 3502 005e E4E7     		b	.L195
 3503              	.L197:
1451:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_DeactivateEndpoint(hpcd->Instance, ep);
 3504              		.loc 1 1451 3 view .LVU1115
 3505 0060 0220     		movs	r0, #2
 3506 0062 F2E7     		b	.L196
 3507              		.cfi_endproc
 3508              	.LFE351:
 3510              		.section	.text.HAL_PCD_EP_Receive,"ax",%progbits
 3511              		.align	1
 3512              		.global	HAL_PCD_EP_Receive
 3513              		.syntax unified
 3514              		.thumb
 3515              		.thumb_func
 3517              	HAL_PCD_EP_Receive:
 3518              	.LVL357:
 3519              	.LFB352:
1467:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3520              		.loc 1 1467 1 is_stmt 1 view -0
 3521              		.cfi_startproc
 3522              		@ args = 0, pretend = 0, frame = 0
 3523              		@ frame_needed = 0, uses_anonymous_args = 0
1467:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3524              		.loc 1 1467 1 is_stmt 0 view .LVU1117
 3525 0000 10B5     		push	{r4, lr}
 3526              	.LCFI22:
 3527              		.cfi_def_cfa_offset 8
 3528              		.cfi_offset 4, -8
 3529              		.cfi_offset 14, -4
1468:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3530              		.loc 1 1468 3 is_stmt 1 view .LVU1118
1470:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3531              		.loc 1 1470 3 view .LVU1119
 3532 0002 01F00704 		and	r4, r1, #7
1470:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3533              		.loc 1 1470 6 is_stmt 0 view .LVU1120
ARM GAS  /tmp/ccJPteqL.s 			page 118


 3534 0006 04EB8401 		add	r1, r4, r4, lsl #2
 3535              	.LVL358:
1470:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3536              		.loc 1 1470 6 view .LVU1121
 3537 000a C900     		lsls	r1, r1, #3
 3538 000c 01F5B471 		add	r1, r1, #360
 3539 0010 0144     		add	r1, r1, r0
 3540              	.LVL359:
1473:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_len = len;
 3541              		.loc 1 1473 3 is_stmt 1 view .LVU1122
1473:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_len = len;
 3542              		.loc 1 1473 17 is_stmt 0 view .LVU1123
 3543 0012 04EB840C 		add	ip, r4, r4, lsl #2
 3544 0016 00EBCC0C 		add	ip, r0, ip, lsl #3
 3545 001a CCF87C21 		str	r2, [ip, #380]
1474:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_count = 0U;
 3546              		.loc 1 1474 3 is_stmt 1 view .LVU1124
1474:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_count = 0U;
 3547              		.loc 1 1474 16 is_stmt 0 view .LVU1125
 3548 001e CCF88031 		str	r3, [ip, #384]
1475:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->is_in = 0U;
 3549              		.loc 1 1475 3 is_stmt 1 view .LVU1126
1475:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->is_in = 0U;
 3550              		.loc 1 1475 18 is_stmt 0 view .LVU1127
 3551 0022 0023     		movs	r3, #0
 3552              	.LVL360:
1475:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->is_in = 0U;
 3553              		.loc 1 1475 18 view .LVU1128
 3554 0024 CCF88431 		str	r3, [ip, #388]
1476:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
 3555              		.loc 1 1476 3 is_stmt 1 view .LVU1129
1476:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
 3556              		.loc 1 1476 13 is_stmt 0 view .LVU1130
 3557 0028 8CF86931 		strb	r3, [ip, #361]
1477:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3558              		.loc 1 1477 3 is_stmt 1 view .LVU1131
1477:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3559              		.loc 1 1477 11 is_stmt 0 view .LVU1132
 3560 002c 8CF86841 		strb	r4, [ip, #360]
1479:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3561              		.loc 1 1479 3 is_stmt 1 view .LVU1133
1479:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3562              		.loc 1 1479 6 is_stmt 0 view .LVU1134
 3563 0030 24B9     		cbnz	r4, .L201
1481:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3564              		.loc 1 1481 5 is_stmt 1 view .LVU1135
1481:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3565              		.loc 1 1481 11 is_stmt 0 view .LVU1136
 3566 0032 0068     		ldr	r0, [r0]
 3567              	.LVL361:
1481:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3568              		.loc 1 1481 11 view .LVU1137
 3569 0034 FFF7FEFF 		bl	USB_EPStartXfer
 3570              	.LVL362:
 3571              	.L202:
1488:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 3572              		.loc 1 1488 3 is_stmt 1 view .LVU1138
ARM GAS  /tmp/ccJPteqL.s 			page 119


1489:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3573              		.loc 1 1489 1 is_stmt 0 view .LVU1139
 3574 0038 0020     		movs	r0, #0
 3575 003a 10BD     		pop	{r4, pc}
 3576              	.LVL363:
 3577              	.L201:
1485:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3578              		.loc 1 1485 5 is_stmt 1 view .LVU1140
1485:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3579              		.loc 1 1485 11 is_stmt 0 view .LVU1141
 3580 003c 0068     		ldr	r0, [r0]
 3581              	.LVL364:
1485:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3582              		.loc 1 1485 11 view .LVU1142
 3583 003e FFF7FEFF 		bl	USB_EPStartXfer
 3584              	.LVL365:
1485:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3585              		.loc 1 1485 11 view .LVU1143
 3586 0042 F9E7     		b	.L202
 3587              		.cfi_endproc
 3588              	.LFE352:
 3590              		.section	.text.HAL_PCD_EP_GetRxCount,"ax",%progbits
 3591              		.align	1
 3592              		.global	HAL_PCD_EP_GetRxCount
 3593              		.syntax unified
 3594              		.thumb
 3595              		.thumb_func
 3597              	HAL_PCD_EP_GetRxCount:
 3598              	.LVL366:
 3599              	.LFB353:
1498:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return hpcd->OUT_ep[ep_addr & EP_ADDR_MSK].xfer_count;
 3600              		.loc 1 1498 1 is_stmt 1 view -0
 3601              		.cfi_startproc
 3602              		@ args = 0, pretend = 0, frame = 0
 3603              		@ frame_needed = 0, uses_anonymous_args = 0
 3604              		@ link register save eliminated.
1499:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 3605              		.loc 1 1499 3 view .LVU1145
1499:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 3606              		.loc 1 1499 31 is_stmt 0 view .LVU1146
 3607 0000 01F00701 		and	r1, r1, #7
 3608              	.LVL367:
1499:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 3609              		.loc 1 1499 45 view .LVU1147
 3610 0004 01EB8101 		add	r1, r1, r1, lsl #2
 3611 0008 00EBC100 		add	r0, r0, r1, lsl #3
 3612              	.LVL368:
1500:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** /**
 3613              		.loc 1 1500 1 view .LVU1148
 3614 000c D0F88401 		ldr	r0, [r0, #388]
 3615 0010 7047     		bx	lr
 3616              		.cfi_endproc
 3617              	.LFE353:
 3619              		.section	.text.HAL_PCD_EP_Transmit,"ax",%progbits
 3620              		.align	1
 3621              		.global	HAL_PCD_EP_Transmit
 3622              		.syntax unified
ARM GAS  /tmp/ccJPteqL.s 			page 120


 3623              		.thumb
 3624              		.thumb_func
 3626              	HAL_PCD_EP_Transmit:
 3627              	.LVL369:
 3628              	.LFB354:
1510:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3629              		.loc 1 1510 1 is_stmt 1 view -0
 3630              		.cfi_startproc
 3631              		@ args = 0, pretend = 0, frame = 0
 3632              		@ frame_needed = 0, uses_anonymous_args = 0
1510:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3633              		.loc 1 1510 1 is_stmt 0 view .LVU1150
 3634 0000 10B5     		push	{r4, lr}
 3635              	.LCFI23:
 3636              		.cfi_def_cfa_offset 8
 3637              		.cfi_offset 4, -8
 3638              		.cfi_offset 14, -4
1511:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3639              		.loc 1 1511 3 is_stmt 1 view .LVU1151
1513:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3640              		.loc 1 1513 3 view .LVU1152
 3641 0002 01F00704 		and	r4, r1, #7
1513:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3642              		.loc 1 1513 6 is_stmt 0 view .LVU1153
 3643 0006 04F1010C 		add	ip, r4, #1
 3644 000a 0CEB8C01 		add	r1, ip, ip, lsl #2
 3645              	.LVL370:
1513:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3646              		.loc 1 1513 6 view .LVU1154
 3647 000e 00EBC101 		add	r1, r0, r1, lsl #3
 3648              	.LVL371:
1516:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_len = len;
 3649              		.loc 1 1516 3 is_stmt 1 view .LVU1155
1516:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_len = len;
 3650              		.loc 1 1516 17 is_stmt 0 view .LVU1156
 3651 0012 04EB840E 		add	lr, r4, r4, lsl #2
 3652 0016 00EBCE0E 		add	lr, r0, lr, lsl #3
 3653 001a CEF83C20 		str	r2, [lr, #60]
1517:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_fill_db = 1U;
 3654              		.loc 1 1517 3 is_stmt 1 view .LVU1157
1517:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_fill_db = 1U;
 3655              		.loc 1 1517 16 is_stmt 0 view .LVU1158
 3656 001e CEF84030 		str	r3, [lr, #64]
1518:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_len_db = len;
 3657              		.loc 1 1518 3 is_stmt 1 view .LVU1159
1518:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_len_db = len;
 3658              		.loc 1 1518 20 is_stmt 0 view .LVU1160
 3659 0022 0122     		movs	r2, #1
 3660              	.LVL372:
1518:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_len_db = len;
 3661              		.loc 1 1518 20 view .LVU1161
 3662 0024 8EF84C20 		strb	r2, [lr, #76]
1519:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_count = 0U;
 3663              		.loc 1 1519 3 is_stmt 1 view .LVU1162
1519:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->xfer_count = 0U;
 3664              		.loc 1 1519 19 is_stmt 0 view .LVU1163
 3665 0028 CEF84830 		str	r3, [lr, #72]
ARM GAS  /tmp/ccJPteqL.s 			page 121


1520:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->is_in = 1U;
 3666              		.loc 1 1520 3 is_stmt 1 view .LVU1164
1520:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->is_in = 1U;
 3667              		.loc 1 1520 18 is_stmt 0 view .LVU1165
 3668 002c 0023     		movs	r3, #0
 3669              	.LVL373:
1520:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->is_in = 1U;
 3670              		.loc 1 1520 18 view .LVU1166
 3671 002e CEF84430 		str	r3, [lr, #68]
1521:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
 3672              		.loc 1 1521 3 is_stmt 1 view .LVU1167
1521:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
 3673              		.loc 1 1521 13 is_stmt 0 view .LVU1168
 3674 0032 4A70     		strb	r2, [r1, #1]
 3675              	.LVL374:
1522:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3676              		.loc 1 1522 3 is_stmt 1 view .LVU1169
1522:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3677              		.loc 1 1522 11 is_stmt 0 view .LVU1170
 3678 0034 0CEB8C0C 		add	ip, ip, ip, lsl #2
 3679 0038 00F83C40 		strb	r4, [r0, ip, lsl #3]
1524:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3680              		.loc 1 1524 3 is_stmt 1 view .LVU1171
1524:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3681              		.loc 1 1524 6 is_stmt 0 view .LVU1172
 3682 003c 24B9     		cbnz	r4, .L206
1526:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3683              		.loc 1 1526 5 is_stmt 1 view .LVU1173
1526:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3684              		.loc 1 1526 11 is_stmt 0 view .LVU1174
 3685 003e 0068     		ldr	r0, [r0]
 3686              	.LVL375:
1526:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3687              		.loc 1 1526 11 view .LVU1175
 3688 0040 FFF7FEFF 		bl	USB_EPStartXfer
 3689              	.LVL376:
 3690              	.L207:
1533:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 3691              		.loc 1 1533 3 is_stmt 1 view .LVU1176
1534:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3692              		.loc 1 1534 1 is_stmt 0 view .LVU1177
 3693 0044 0020     		movs	r0, #0
 3694 0046 10BD     		pop	{r4, pc}
 3695              	.LVL377:
 3696              	.L206:
1530:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3697              		.loc 1 1530 5 is_stmt 1 view .LVU1178
1530:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3698              		.loc 1 1530 11 is_stmt 0 view .LVU1179
 3699 0048 0068     		ldr	r0, [r0]
 3700              	.LVL378:
1530:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3701              		.loc 1 1530 11 view .LVU1180
 3702 004a FFF7FEFF 		bl	USB_EPStartXfer
 3703              	.LVL379:
1530:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3704              		.loc 1 1530 11 view .LVU1181
ARM GAS  /tmp/ccJPteqL.s 			page 122


 3705 004e F9E7     		b	.L207
 3706              		.cfi_endproc
 3707              	.LFE354:
 3709              		.section	.text.HAL_PCD_EP_SetStall,"ax",%progbits
 3710              		.align	1
 3711              		.global	HAL_PCD_EP_SetStall
 3712              		.syntax unified
 3713              		.thumb
 3714              		.thumb_func
 3716              	HAL_PCD_EP_SetStall:
 3717              	.LVL380:
 3718              	.LFB355:
1543:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3719              		.loc 1 1543 1 is_stmt 1 view -0
 3720              		.cfi_startproc
 3721              		@ args = 0, pretend = 0, frame = 0
 3722              		@ frame_needed = 0, uses_anonymous_args = 0
1543:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3723              		.loc 1 1543 1 is_stmt 0 view .LVU1183
 3724 0000 0B46     		mov	r3, r1
1544:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3725              		.loc 1 1544 3 is_stmt 1 view .LVU1184
1546:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3726              		.loc 1 1546 3 view .LVU1185
 3727 0002 01F00702 		and	r2, r1, #7
1546:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3728              		.loc 1 1546 53 is_stmt 0 view .LVU1186
 3729 0006 4168     		ldr	r1, [r0, #4]
 3730              	.LVL381:
1546:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3731              		.loc 1 1546 6 view .LVU1187
 3732 0008 8A42     		cmp	r2, r1
 3733 000a 2AD8     		bhi	.L213
1543:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3734              		.loc 1 1543 1 view .LVU1188
 3735 000c 10B5     		push	{r4, lr}
 3736              	.LCFI24:
 3737              		.cfi_def_cfa_offset 8
 3738              		.cfi_offset 4, -8
 3739              		.cfi_offset 14, -4
 3740 000e 0446     		mov	r4, r0
1551:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3741              		.loc 1 1551 3 is_stmt 1 view .LVU1189
1551:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3742              		.loc 1 1551 6 is_stmt 0 view .LVU1190
 3743 0010 13F0800F 		tst	r3, #128
 3744 0014 1DD1     		bne	.L219
1558:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3745              		.loc 1 1558 5 is_stmt 1 view .LVU1191
1558:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3746              		.loc 1 1558 8 is_stmt 0 view .LVU1192
 3747 0016 03EB8301 		add	r1, r3, r3, lsl #2
 3748 001a C900     		lsls	r1, r1, #3
 3749 001c 01F5B471 		add	r1, r1, #360
 3750 0020 0144     		add	r1, r1, r0
 3751              	.LVL382:
1559:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
ARM GAS  /tmp/ccJPteqL.s 			page 123


 3752              		.loc 1 1559 5 is_stmt 1 view .LVU1193
1559:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3753              		.loc 1 1559 15 is_stmt 0 view .LVU1194
 3754 0022 03EB8303 		add	r3, r3, r3, lsl #2
 3755 0026 00EBC303 		add	r3, r0, r3, lsl #3
 3756 002a 0020     		movs	r0, #0
 3757              	.LVL383:
1559:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3758              		.loc 1 1559 15 view .LVU1195
 3759 002c 83F86901 		strb	r0, [r3, #361]
 3760              	.L212:
1562:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
 3761              		.loc 1 1562 3 is_stmt 1 view .LVU1196
1562:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
 3762              		.loc 1 1562 16 is_stmt 0 view .LVU1197
 3763 0030 0123     		movs	r3, #1
 3764 0032 8B70     		strb	r3, [r1, #2]
1563:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3765              		.loc 1 1563 3 is_stmt 1 view .LVU1198
1563:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3766              		.loc 1 1563 11 is_stmt 0 view .LVU1199
 3767 0034 0A70     		strb	r2, [r1]
1565:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3768              		.loc 1 1565 3 is_stmt 1 view .LVU1200
1565:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3769              		.loc 1 1565 3 view .LVU1201
 3770 0036 94F8A832 		ldrb	r3, [r4, #680]	@ zero_extendqisi2
 3771 003a 012B     		cmp	r3, #1
 3772 003c 13D0     		beq	.L214
1565:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3773              		.loc 1 1565 3 discriminator 2 view .LVU1202
 3774 003e 0123     		movs	r3, #1
 3775 0040 84F8A832 		strb	r3, [r4, #680]
1565:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3776              		.loc 1 1565 3 discriminator 2 view .LVU1203
1567:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3777              		.loc 1 1567 3 discriminator 2 view .LVU1204
1567:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3778              		.loc 1 1567 9 is_stmt 0 discriminator 2 view .LVU1205
 3779 0044 2068     		ldr	r0, [r4]
 3780 0046 FFF7FEFF 		bl	USB_EPSetStall
 3781              	.LVL384:
1569:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3782              		.loc 1 1569 3 is_stmt 1 discriminator 2 view .LVU1206
1569:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3783              		.loc 1 1569 3 discriminator 2 view .LVU1207
 3784 004a 0020     		movs	r0, #0
 3785 004c 84F8A802 		strb	r0, [r4, #680]
1569:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3786              		.loc 1 1569 3 discriminator 2 view .LVU1208
1571:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 3787              		.loc 1 1571 3 discriminator 2 view .LVU1209
 3788              	.L210:
1572:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3789              		.loc 1 1572 1 is_stmt 0 view .LVU1210
 3790 0050 10BD     		pop	{r4, pc}
 3791              	.LVL385:
ARM GAS  /tmp/ccJPteqL.s 			page 124


 3792              	.L219:
1553:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3793              		.loc 1 1553 5 is_stmt 1 view .LVU1211
1553:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3794              		.loc 1 1553 8 is_stmt 0 view .LVU1212
 3795 0052 531C     		adds	r3, r2, #1
 3796 0054 03EB8301 		add	r1, r3, r3, lsl #2
 3797 0058 00EBC101 		add	r1, r0, r1, lsl #3
 3798              	.LVL386:
1554:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3799              		.loc 1 1554 5 is_stmt 1 view .LVU1213
1554:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3800              		.loc 1 1554 15 is_stmt 0 view .LVU1214
 3801 005c 0120     		movs	r0, #1
 3802              	.LVL387:
1554:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3803              		.loc 1 1554 15 view .LVU1215
 3804 005e 4870     		strb	r0, [r1, #1]
 3805 0060 E6E7     		b	.L212
 3806              	.LVL388:
 3807              	.L213:
 3808              	.LCFI25:
 3809              		.cfi_def_cfa_offset 0
 3810              		.cfi_restore 4
 3811              		.cfi_restore 14
1548:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3812              		.loc 1 1548 12 view .LVU1216
 3813 0062 0120     		movs	r0, #1
 3814              	.LVL389:
1572:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3815              		.loc 1 1572 1 view .LVU1217
 3816 0064 7047     		bx	lr
 3817              	.LVL390:
 3818              	.L214:
 3819              	.LCFI26:
 3820              		.cfi_def_cfa_offset 8
 3821              		.cfi_offset 4, -8
 3822              		.cfi_offset 14, -4
1565:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3823              		.loc 1 1565 3 view .LVU1218
 3824 0066 0220     		movs	r0, #2
 3825 0068 F2E7     		b	.L210
 3826              		.cfi_endproc
 3827              	.LFE355:
 3829              		.section	.text.HAL_PCD_EP_ClrStall,"ax",%progbits
 3830              		.align	1
 3831              		.global	HAL_PCD_EP_ClrStall
 3832              		.syntax unified
 3833              		.thumb
 3834              		.thumb_func
 3836              	HAL_PCD_EP_ClrStall:
 3837              	.LVL391:
 3838              	.LFB356:
1581:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3839              		.loc 1 1581 1 is_stmt 1 view -0
 3840              		.cfi_startproc
 3841              		@ args = 0, pretend = 0, frame = 0
ARM GAS  /tmp/ccJPteqL.s 			page 125


 3842              		@ frame_needed = 0, uses_anonymous_args = 0
1581:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3843              		.loc 1 1581 1 is_stmt 0 view .LVU1220
 3844 0000 0B46     		mov	r3, r1
1582:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3845              		.loc 1 1582 3 is_stmt 1 view .LVU1221
1584:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3846              		.loc 1 1584 3 view .LVU1222
1584:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3847              		.loc 1 1584 26 is_stmt 0 view .LVU1223
 3848 0002 01F00F01 		and	r1, r1, #15
 3849              	.LVL392:
1584:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3850              		.loc 1 1584 47 view .LVU1224
 3851 0006 4268     		ldr	r2, [r0, #4]
1584:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3852              		.loc 1 1584 6 view .LVU1225
 3853 0008 9142     		cmp	r1, r2
 3854 000a 30D8     		bhi	.L224
1581:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   PCD_EPTypeDef *ep;
 3855              		.loc 1 1581 1 view .LVU1226
 3856 000c 10B5     		push	{r4, lr}
 3857              	.LCFI27:
 3858              		.cfi_def_cfa_offset 8
 3859              		.cfi_offset 4, -8
 3860              		.cfi_offset 14, -4
 3861 000e 0446     		mov	r4, r0
1589:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3862              		.loc 1 1589 3 is_stmt 1 view .LVU1227
1589:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   {
 3863              		.loc 1 1589 6 is_stmt 0 view .LVU1228
 3864 0010 13F0800F 		tst	r3, #128
 3865 0014 21D1     		bne	.L230
1596:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3866              		.loc 1 1596 5 is_stmt 1 view .LVU1229
1596:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3867              		.loc 1 1596 32 is_stmt 0 view .LVU1230
 3868 0016 03F00702 		and	r2, r3, #7
1596:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 0U;
 3869              		.loc 1 1596 8 view .LVU1231
 3870 001a 02EB8201 		add	r1, r2, r2, lsl #2
 3871 001e C900     		lsls	r1, r1, #3
 3872 0020 01F5B471 		add	r1, r1, #360
 3873 0024 0144     		add	r1, r1, r0
 3874              	.LVL393:
1597:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3875              		.loc 1 1597 5 is_stmt 1 view .LVU1232
1597:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3876              		.loc 1 1597 15 is_stmt 0 view .LVU1233
 3877 0026 02EB8202 		add	r2, r2, r2, lsl #2
 3878 002a 00EBC202 		add	r2, r0, r2, lsl #3
 3879 002e 0020     		movs	r0, #0
 3880              	.LVL394:
1597:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3881              		.loc 1 1597 15 view .LVU1234
 3882 0030 82F86901 		strb	r0, [r2, #361]
 3883              	.L223:
ARM GAS  /tmp/ccJPteqL.s 			page 126


1600:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
 3884              		.loc 1 1600 3 is_stmt 1 view .LVU1235
1600:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   ep->num = ep_addr & EP_ADDR_MSK;
 3885              		.loc 1 1600 16 is_stmt 0 view .LVU1236
 3886 0034 0022     		movs	r2, #0
 3887 0036 8A70     		strb	r2, [r1, #2]
1601:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3888              		.loc 1 1601 3 is_stmt 1 view .LVU1237
1601:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3889              		.loc 1 1601 21 is_stmt 0 view .LVU1238
 3890 0038 03F00703 		and	r3, r3, #7
1601:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3891              		.loc 1 1601 11 view .LVU1239
 3892 003c 0B70     		strb	r3, [r1]
1603:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_EPClearStall(hpcd->Instance, ep);
 3893              		.loc 1 1603 3 is_stmt 1 view .LVU1240
1603:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_EPClearStall(hpcd->Instance, ep);
 3894              		.loc 1 1603 3 view .LVU1241
 3895 003e 94F8A832 		ldrb	r3, [r4, #680]	@ zero_extendqisi2
 3896 0042 012B     		cmp	r3, #1
 3897 0044 15D0     		beq	.L225
1603:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_EPClearStall(hpcd->Instance, ep);
 3898              		.loc 1 1603 3 discriminator 2 view .LVU1242
 3899 0046 0123     		movs	r3, #1
 3900 0048 84F8A832 		strb	r3, [r4, #680]
1603:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_EPClearStall(hpcd->Instance, ep);
 3901              		.loc 1 1603 3 discriminator 2 view .LVU1243
1604:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 3902              		.loc 1 1604 3 discriminator 2 view .LVU1244
1604:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   __HAL_UNLOCK(hpcd);
 3903              		.loc 1 1604 9 is_stmt 0 discriminator 2 view .LVU1245
 3904 004c 2068     		ldr	r0, [r4]
 3905 004e FFF7FEFF 		bl	USB_EPClearStall
 3906              	.LVL395:
1605:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3907              		.loc 1 1605 3 is_stmt 1 discriminator 2 view .LVU1246
1605:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3908              		.loc 1 1605 3 discriminator 2 view .LVU1247
 3909 0052 0020     		movs	r0, #0
 3910 0054 84F8A802 		strb	r0, [r4, #680]
1605:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3911              		.loc 1 1605 3 discriminator 2 view .LVU1248
1607:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 3912              		.loc 1 1607 3 discriminator 2 view .LVU1249
 3913              	.L221:
1608:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3914              		.loc 1 1608 1 is_stmt 0 view .LVU1250
 3915 0058 10BD     		pop	{r4, pc}
 3916              	.LVL396:
 3917              	.L230:
1591:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3918              		.loc 1 1591 5 is_stmt 1 view .LVU1251
1591:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3919              		.loc 1 1591 31 is_stmt 0 view .LVU1252
 3920 005a 03F00702 		and	r2, r3, #7
1591:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****     ep->is_in = 1U;
 3921              		.loc 1 1591 8 view .LVU1253
ARM GAS  /tmp/ccJPteqL.s 			page 127


 3922 005e 0132     		adds	r2, r2, #1
 3923 0060 02EB8201 		add	r1, r2, r2, lsl #2
 3924 0064 00EBC101 		add	r1, r0, r1, lsl #3
 3925              	.LVL397:
1592:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3926              		.loc 1 1592 5 is_stmt 1 view .LVU1254
1592:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3927              		.loc 1 1592 15 is_stmt 0 view .LVU1255
 3928 0068 0120     		movs	r0, #1
 3929              	.LVL398:
1592:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3930              		.loc 1 1592 15 view .LVU1256
 3931 006a 4870     		strb	r0, [r1, #1]
 3932 006c E2E7     		b	.L223
 3933              	.LVL399:
 3934              	.L224:
 3935              	.LCFI28:
 3936              		.cfi_def_cfa_offset 0
 3937              		.cfi_restore 4
 3938              		.cfi_restore 14
1586:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   }
 3939              		.loc 1 1586 12 view .LVU1257
 3940 006e 0120     		movs	r0, #1
 3941              	.LVL400:
1608:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3942              		.loc 1 1608 1 view .LVU1258
 3943 0070 7047     		bx	lr
 3944              	.LVL401:
 3945              	.L225:
 3946              	.LCFI29:
 3947              		.cfi_def_cfa_offset 8
 3948              		.cfi_offset 4, -8
 3949              		.cfi_offset 14, -4
1603:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   (void)USB_EPClearStall(hpcd->Instance, ep);
 3950              		.loc 1 1603 3 view .LVU1259
 3951 0072 0220     		movs	r0, #2
 3952 0074 F0E7     		b	.L221
 3953              		.cfi_endproc
 3954              	.LFE356:
 3956              		.section	.text.HAL_PCD_EP_Flush,"ax",%progbits
 3957              		.align	1
 3958              		.global	HAL_PCD_EP_Flush
 3959              		.syntax unified
 3960              		.thumb
 3961              		.thumb_func
 3963              	HAL_PCD_EP_Flush:
 3964              	.LVL402:
 3965              	.LFB357:
1617:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   /* Prevent unused argument(s) compilation warning */
 3966              		.loc 1 1617 1 is_stmt 1 view -0
 3967              		.cfi_startproc
 3968              		@ args = 0, pretend = 0, frame = 0
 3969              		@ frame_needed = 0, uses_anonymous_args = 0
 3970              		@ link register save eliminated.
1619:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   UNUSED(ep_addr);
 3971              		.loc 1 1619 3 view .LVU1261
1620:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
ARM GAS  /tmp/ccJPteqL.s 			page 128


 3972              		.loc 1 1620 3 view .LVU1262
1622:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 3973              		.loc 1 1622 3 view .LVU1263
1623:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3974              		.loc 1 1623 1 is_stmt 0 view .LVU1264
 3975 0000 0020     		movs	r0, #0
 3976              	.LVL403:
1623:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 3977              		.loc 1 1623 1 view .LVU1265
 3978 0002 7047     		bx	lr
 3979              		.cfi_endproc
 3980              	.LFE357:
 3982              		.section	.text.HAL_PCD_ActivateRemoteWakeup,"ax",%progbits
 3983              		.align	1
 3984              		.global	HAL_PCD_ActivateRemoteWakeup
 3985              		.syntax unified
 3986              		.thumb
 3987              		.thumb_func
 3989              	HAL_PCD_ActivateRemoteWakeup:
 3990              	.LVL404:
 3991              	.LFB358:
1631:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return (USB_ActivateRemoteWakeup(hpcd->Instance));
 3992              		.loc 1 1631 1 is_stmt 1 view -0
 3993              		.cfi_startproc
 3994              		@ args = 0, pretend = 0, frame = 0
 3995              		@ frame_needed = 0, uses_anonymous_args = 0
1631:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return (USB_ActivateRemoteWakeup(hpcd->Instance));
 3996              		.loc 1 1631 1 is_stmt 0 view .LVU1267
 3997 0000 08B5     		push	{r3, lr}
 3998              	.LCFI30:
 3999              		.cfi_def_cfa_offset 8
 4000              		.cfi_offset 3, -8
 4001              		.cfi_offset 14, -4
1632:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 4002              		.loc 1 1632 3 is_stmt 1 view .LVU1268
1632:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 4003              		.loc 1 1632 11 is_stmt 0 view .LVU1269
 4004 0002 0068     		ldr	r0, [r0]
 4005              	.LVL405:
1632:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 4006              		.loc 1 1632 11 view .LVU1270
 4007 0004 FFF7FEFF 		bl	USB_ActivateRemoteWakeup
 4008              	.LVL406:
1633:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 4009              		.loc 1 1633 1 view .LVU1271
 4010 0008 08BD     		pop	{r3, pc}
 4011              		.cfi_endproc
 4012              	.LFE358:
 4014              		.section	.text.HAL_PCD_DeActivateRemoteWakeup,"ax",%progbits
 4015              		.align	1
 4016              		.global	HAL_PCD_DeActivateRemoteWakeup
 4017              		.syntax unified
 4018              		.thumb
 4019              		.thumb_func
 4021              	HAL_PCD_DeActivateRemoteWakeup:
 4022              	.LVL407:
 4023              	.LFB359:
ARM GAS  /tmp/ccJPteqL.s 			page 129


1641:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return (USB_DeActivateRemoteWakeup(hpcd->Instance));
 4024              		.loc 1 1641 1 is_stmt 1 view -0
 4025              		.cfi_startproc
 4026              		@ args = 0, pretend = 0, frame = 0
 4027              		@ frame_needed = 0, uses_anonymous_args = 0
1641:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return (USB_DeActivateRemoteWakeup(hpcd->Instance));
 4028              		.loc 1 1641 1 is_stmt 0 view .LVU1273
 4029 0000 08B5     		push	{r3, lr}
 4030              	.LCFI31:
 4031              		.cfi_def_cfa_offset 8
 4032              		.cfi_offset 3, -8
 4033              		.cfi_offset 14, -4
1642:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 4034              		.loc 1 1642 3 is_stmt 1 view .LVU1274
1642:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 4035              		.loc 1 1642 11 is_stmt 0 view .LVU1275
 4036 0002 0068     		ldr	r0, [r0]
 4037              	.LVL408:
1642:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 4038              		.loc 1 1642 11 view .LVU1276
 4039 0004 FFF7FEFF 		bl	USB_DeActivateRemoteWakeup
 4040              	.LVL409:
1643:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 4041              		.loc 1 1643 1 view .LVU1277
 4042 0008 08BD     		pop	{r3, pc}
 4043              		.cfi_endproc
 4044              	.LFE359:
 4046              		.section	.text.HAL_PCD_GetState,"ax",%progbits
 4047              		.align	1
 4048              		.global	HAL_PCD_GetState
 4049              		.syntax unified
 4050              		.thumb
 4051              		.thumb_func
 4053              	HAL_PCD_GetState:
 4054              	.LVL410:
 4055              	.LFB360:
1670:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c ****   return hpcd->State;
 4056              		.loc 1 1670 1 is_stmt 1 view -0
 4057              		.cfi_startproc
 4058              		@ args = 0, pretend = 0, frame = 0
 4059              		@ frame_needed = 0, uses_anonymous_args = 0
 4060              		@ link register save eliminated.
1671:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 4061              		.loc 1 1671 3 view .LVU1279
1671:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** }
 4062              		.loc 1 1671 14 is_stmt 0 view .LVU1280
 4063 0000 90F8A902 		ldrb	r0, [r0, #681]	@ zero_extendqisi2
 4064              	.LVL411:
1672:Drivers/STM32G4xx_HAL_Driver/Src/stm32g4xx_hal_pcd.c **** 
 4065              		.loc 1 1672 1 view .LVU1281
 4066 0004 7047     		bx	lr
 4067              		.cfi_endproc
 4068              	.LFE360:
 4070              		.text
 4071              	.Letext0:
 4072              		.file 2 "/usr/lib/gcc/arm-none-eabi/12.2.1/include/stdint.h"
 4073              		.file 3 "Drivers/CMSIS/Device/ST/STM32G4xx/Include/stm32g431xx.h"
ARM GAS  /tmp/ccJPteqL.s 			page 130


 4074              		.file 4 "Drivers/STM32G4xx_HAL_Driver/Inc/stm32g4xx_hal_def.h"
 4075              		.file 5 "Drivers/STM32G4xx_HAL_Driver/Inc/stm32g4xx_ll_usb.h"
 4076              		.file 6 "Drivers/STM32G4xx_HAL_Driver/Inc/stm32g4xx_hal_pcd.h"
 4077              		.file 7 "Drivers/STM32G4xx_HAL_Driver/Inc/stm32g4xx_hal_pcd_ex.h"
ARM GAS  /tmp/ccJPteqL.s 			page 131


DEFINED SYMBOLS
                            *ABS*:00000000 stm32g4xx_hal_pcd.c
     /tmp/ccJPteqL.s:21     .text.HAL_PCD_EP_DB_Receive:00000000 $t
     /tmp/ccJPteqL.s:26     .text.HAL_PCD_EP_DB_Receive:00000000 HAL_PCD_EP_DB_Receive
     /tmp/ccJPteqL.s:275    .text.HAL_PCD_MspInit:00000000 $t
     /tmp/ccJPteqL.s:281    .text.HAL_PCD_MspInit:00000000 HAL_PCD_MspInit
     /tmp/ccJPteqL.s:296    .text.HAL_PCD_Init:00000000 $t
     /tmp/ccJPteqL.s:302    .text.HAL_PCD_Init:00000000 HAL_PCD_Init
     /tmp/ccJPteqL.s:508    .text.HAL_PCD_MspDeInit:00000000 $t
     /tmp/ccJPteqL.s:514    .text.HAL_PCD_MspDeInit:00000000 HAL_PCD_MspDeInit
     /tmp/ccJPteqL.s:529    .text.HAL_PCD_DeInit:00000000 $t
     /tmp/ccJPteqL.s:535    .text.HAL_PCD_DeInit:00000000 HAL_PCD_DeInit
     /tmp/ccJPteqL.s:597    .text.HAL_PCD_Start:00000000 $t
     /tmp/ccJPteqL.s:603    .text.HAL_PCD_Start:00000000 HAL_PCD_Start
     /tmp/ccJPteqL.s:660    .text.HAL_PCD_Stop:00000000 $t
     /tmp/ccJPteqL.s:666    .text.HAL_PCD_Stop:00000000 HAL_PCD_Stop
     /tmp/ccJPteqL.s:723    .text.HAL_PCD_DataOutStageCallback:00000000 $t
     /tmp/ccJPteqL.s:729    .text.HAL_PCD_DataOutStageCallback:00000000 HAL_PCD_DataOutStageCallback
     /tmp/ccJPteqL.s:745    .text.HAL_PCD_DataInStageCallback:00000000 $t
     /tmp/ccJPteqL.s:751    .text.HAL_PCD_DataInStageCallback:00000000 HAL_PCD_DataInStageCallback
     /tmp/ccJPteqL.s:767    .text.HAL_PCD_EP_DB_Transmit:00000000 $t
     /tmp/ccJPteqL.s:772    .text.HAL_PCD_EP_DB_Transmit:00000000 HAL_PCD_EP_DB_Transmit
     /tmp/ccJPteqL.s:1707   .text.HAL_PCD_SetupStageCallback:00000000 $t
     /tmp/ccJPteqL.s:1713   .text.HAL_PCD_SetupStageCallback:00000000 HAL_PCD_SetupStageCallback
     /tmp/ccJPteqL.s:1728   .text.PCD_EP_ISR_Handler:00000000 $t
     /tmp/ccJPteqL.s:1733   .text.PCD_EP_ISR_Handler:00000000 PCD_EP_ISR_Handler
     /tmp/ccJPteqL.s:2623   .text.HAL_PCD_SOFCallback:00000000 $t
     /tmp/ccJPteqL.s:2629   .text.HAL_PCD_SOFCallback:00000000 HAL_PCD_SOFCallback
     /tmp/ccJPteqL.s:2644   .text.HAL_PCD_ResetCallback:00000000 $t
     /tmp/ccJPteqL.s:2650   .text.HAL_PCD_ResetCallback:00000000 HAL_PCD_ResetCallback
     /tmp/ccJPteqL.s:2665   .text.HAL_PCD_SuspendCallback:00000000 $t
     /tmp/ccJPteqL.s:2671   .text.HAL_PCD_SuspendCallback:00000000 HAL_PCD_SuspendCallback
     /tmp/ccJPteqL.s:2686   .text.HAL_PCD_ResumeCallback:00000000 $t
     /tmp/ccJPteqL.s:2692   .text.HAL_PCD_ResumeCallback:00000000 HAL_PCD_ResumeCallback
     /tmp/ccJPteqL.s:2707   .text.HAL_PCD_ISOOUTIncompleteCallback:00000000 $t
     /tmp/ccJPteqL.s:2713   .text.HAL_PCD_ISOOUTIncompleteCallback:00000000 HAL_PCD_ISOOUTIncompleteCallback
     /tmp/ccJPteqL.s:2729   .text.HAL_PCD_ISOINIncompleteCallback:00000000 $t
     /tmp/ccJPteqL.s:2735   .text.HAL_PCD_ISOINIncompleteCallback:00000000 HAL_PCD_ISOINIncompleteCallback
     /tmp/ccJPteqL.s:2751   .text.HAL_PCD_ConnectCallback:00000000 $t
     /tmp/ccJPteqL.s:2757   .text.HAL_PCD_ConnectCallback:00000000 HAL_PCD_ConnectCallback
     /tmp/ccJPteqL.s:2772   .text.HAL_PCD_DisconnectCallback:00000000 $t
     /tmp/ccJPteqL.s:2778   .text.HAL_PCD_DisconnectCallback:00000000 HAL_PCD_DisconnectCallback
     /tmp/ccJPteqL.s:2793   .text.HAL_PCD_DevConnect:00000000 $t
     /tmp/ccJPteqL.s:2799   .text.HAL_PCD_DevConnect:00000000 HAL_PCD_DevConnect
     /tmp/ccJPteqL.s:2852   .text.HAL_PCD_DevDisconnect:00000000 $t
     /tmp/ccJPteqL.s:2858   .text.HAL_PCD_DevDisconnect:00000000 HAL_PCD_DevDisconnect
     /tmp/ccJPteqL.s:2911   .text.HAL_PCD_SetAddress:00000000 $t
     /tmp/ccJPteqL.s:2917   .text.HAL_PCD_SetAddress:00000000 HAL_PCD_SetAddress
     /tmp/ccJPteqL.s:2973   .text.HAL_PCD_IRQHandler:00000000 $t
     /tmp/ccJPteqL.s:2979   .text.HAL_PCD_IRQHandler:00000000 HAL_PCD_IRQHandler
     /tmp/ccJPteqL.s:3277   .text.HAL_PCD_EP_Open:00000000 $t
     /tmp/ccJPteqL.s:3283   .text.HAL_PCD_EP_Open:00000000 HAL_PCD_EP_Open
     /tmp/ccJPteqL.s:3410   .text.HAL_PCD_EP_Close:00000000 $t
     /tmp/ccJPteqL.s:3416   .text.HAL_PCD_EP_Close:00000000 HAL_PCD_EP_Close
     /tmp/ccJPteqL.s:3511   .text.HAL_PCD_EP_Receive:00000000 $t
     /tmp/ccJPteqL.s:3517   .text.HAL_PCD_EP_Receive:00000000 HAL_PCD_EP_Receive
     /tmp/ccJPteqL.s:3591   .text.HAL_PCD_EP_GetRxCount:00000000 $t
ARM GAS  /tmp/ccJPteqL.s 			page 132


     /tmp/ccJPteqL.s:3597   .text.HAL_PCD_EP_GetRxCount:00000000 HAL_PCD_EP_GetRxCount
     /tmp/ccJPteqL.s:3620   .text.HAL_PCD_EP_Transmit:00000000 $t
     /tmp/ccJPteqL.s:3626   .text.HAL_PCD_EP_Transmit:00000000 HAL_PCD_EP_Transmit
     /tmp/ccJPteqL.s:3710   .text.HAL_PCD_EP_SetStall:00000000 $t
     /tmp/ccJPteqL.s:3716   .text.HAL_PCD_EP_SetStall:00000000 HAL_PCD_EP_SetStall
     /tmp/ccJPteqL.s:3830   .text.HAL_PCD_EP_ClrStall:00000000 $t
     /tmp/ccJPteqL.s:3836   .text.HAL_PCD_EP_ClrStall:00000000 HAL_PCD_EP_ClrStall
     /tmp/ccJPteqL.s:3957   .text.HAL_PCD_EP_Flush:00000000 $t
     /tmp/ccJPteqL.s:3963   .text.HAL_PCD_EP_Flush:00000000 HAL_PCD_EP_Flush
     /tmp/ccJPteqL.s:3983   .text.HAL_PCD_ActivateRemoteWakeup:00000000 $t
     /tmp/ccJPteqL.s:3989   .text.HAL_PCD_ActivateRemoteWakeup:00000000 HAL_PCD_ActivateRemoteWakeup
     /tmp/ccJPteqL.s:4015   .text.HAL_PCD_DeActivateRemoteWakeup:00000000 $t
     /tmp/ccJPteqL.s:4021   .text.HAL_PCD_DeActivateRemoteWakeup:00000000 HAL_PCD_DeActivateRemoteWakeup
     /tmp/ccJPteqL.s:4047   .text.HAL_PCD_GetState:00000000 $t
     /tmp/ccJPteqL.s:4053   .text.HAL_PCD_GetState:00000000 HAL_PCD_GetState

UNDEFINED SYMBOLS
USB_ReadPMA
USB_DisableGlobalInt
USB_DevInit
HAL_PCDEx_ActivateLPM
USB_StopDevice
USB_EnableGlobalInt
USB_DevConnect
USB_DevDisconnect
USB_WritePMA
USB_EPStartXfer
USB_SetDevAddress
USB_ReadInterrupts
HAL_PCDEx_LPM_Callback
USB_ActivateEndpoint
USB_DeactivateEndpoint
USB_EPSetStall
USB_EPClearStall
USB_ActivateRemoteWakeup
USB_DeActivateRemoteWakeup
