(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 46.9825 16.51)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "GND")
  (net 2 "unconnected-(U4-Pad2)")
  (net 3 "unconnected-(U3-Pad2)")
  (net 4 "unconnected-(U2-Pad2)")
  (net 5 "unconnected-(U1-Pad2)")
  (net 6 "Net-(R4-Pad1)")
  (net 7 "Net-(R3-Pad1)")
  (net 8 "Net-(R2-Pad1)")
  (net 9 "Net-(R1-Pad1)")
  (net 10 "Net-(Q4-Pad1)")
  (net 11 "Net-(Q3-Pad1)")
  (net 12 "Net-(Q2-Pad1)")
  (net 13 "Net-(Q1-Pad1)")
  (net 14 "Net-(J6-Pad5)")
  (net 15 "Net-(J6-Pad4)")
  (net 16 "Net-(J6-Pad3)")
  (net 17 "Net-(J6-Pad2)")
  (net 18 "Net-(J6-Pad1)")
  (net 19 "Net-(D3-Pad2)")
  (net 20 "Net-(D2-Pad2)")
  (net 21 "Net-(D1-Pad2)")
  (net 22 "Net-(D1-Pad1)")
  (net 23 "Net-(C4-Pad2)")
  (net 24 "Net-(C4-Pad1)")
  (net 25 "Net-(C3-Pad2)")
  (net 26 "Net-(C3-Pad1)")
  (net 27 "Net-(C2-Pad2)")
  (net 28 "Net-(C2-Pad1)")
  (net 29 "Net-(C1-Pad2)")
  (net 30 "Net-(C1-Pad1)")

  (footprint "Package_TO_SOT_THT:TO-220F-3_Horizontal_TabDown" (layer "F.Cu")
    (tstamp 0134792b-1e2a-48a7-a29d-5d883dfcafa1)
    (at 50.96 78.105 90)
    (descr "TO-220F-3, Horizontal, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf")
    (tags "TO-220F-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/34aa2012-1c68-4d57-95ca-133c293530aa")
    (attr through_hole)
    (fp_text reference "D1" (at 2.54 -20.22 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e3cbea0c-3e3c-4c91-bd43-134aefdd0b3b)
    )
    (fp_text value "D_Schottky_x2_ACom_KAK" (at 2.54 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b07c43bc-2dc9-40f9-b67c-733c12c28e89)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -20.22 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5e18aa30-42c6-4779-b0a4-198e1d2e7920)
    )
    (fp_line (start -2.71 -19.22) (end -2.71 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1280474a-d464-4628-ac8a-ba042b748218))
    (fp_line (start -2.71 -19.22) (end 7.79 -19.22)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2758f51d-88e4-4a26-84e9-468c10e23893))
    (fp_line (start -2.71 -3.11) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 24384664-1687-4ac0-b427-039bea4352d1))
    (fp_line (start 0 -3.11) (end 0 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 56c6d66b-7881-437d-bd78-ddbe778a837b))
    (fp_line (start 2.54 -3.11) (end 2.54 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1e51a8eb-6b78-4968-8de7-1c5c6b641502))
    (fp_line (start 5.08 -3.11) (end 5.08 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 46bf5099-aec9-425d-8b68-7b96afaa808e))
    (fp_line (start 7.79 -19.22) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f2734a8f-a8d8-4c8c-b519-ec774889b5c1))
    (fp_line (start -2.84 -19.35) (end -2.84 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9455c583-9e9d-48e5-8402-f710adc30ae9))
    (fp_line (start -2.84 1.25) (end 7.92 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 75a2c46e-9c38-482f-9172-eb3ab9aa58bd))
    (fp_line (start 7.92 -19.35) (end -2.84 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 37707259-b10d-4ea4-bb47-568b4aca40dd))
    (fp_line (start 7.92 1.25) (end 7.92 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp edb06c86-1504-4d02-80ea-e81f4b54a65b))
    (fp_line (start -2.59 -19.1) (end 7.67 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6d1443db-7dd1-4e9a-a04f-c6b98cb23bd6))
    (fp_line (start -2.59 -12.42) (end -2.59 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 01db896a-4bda-4675-9782-46df674fb533))
    (fp_line (start -2.59 -12.42) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8b3e527d-8d66-4991-8d2b-1a8326be1a0d))
    (fp_line (start -2.59 -3.23) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 66d08652-6a53-4787-8021-6373e88d8726))
    (fp_line (start 0 -3.23) (end 0 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ecd04929-5506-4809-8eb1-c0236b3280e6))
    (fp_line (start 2.54 -3.23) (end 2.54 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1854b995-84f6-4b14-8acc-96ea4383d78f))
    (fp_line (start 5.08 -3.23) (end 5.08 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2303ea9-3693-4829-a0a0-a961b59990ae))
    (fp_line (start 7.67 -19.1) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b1b0ba7c-8cf3-47b5-a767-3d16a01a6b79))
    (fp_line (start 7.67 -12.42) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bc94777e-87c2-4bf2-afd0-cbbf2a77260d))
    (fp_line (start 7.67 -12.42) (end 7.67 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d2e892c-cb1d-436b-864e-0a7d83672a6e))
    (fp_line (start 7.67 -3.23) (end -2.59 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e2ca9b92-3f8c-489c-a05e-d7f325c8a050))
    (fp_circle (center 2.54 -15.8) (end 4.39 -15.8)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 6c382f61-70e9-4ffe-9fc0-93b057466a6f))
    (pad "" np_thru_hole oval (at 2.54 -15.8 90) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask") (tstamp 5ad2c2ff-9091-4864-b93d-fa98dba663cc))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 1fd42927-ed8d-4a5f-8eee-0e4e0bc7ab81))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive") (tstamp a0ff0e29-8c3d-4fdd-982b-49de8517f75a))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(C1-Pad2)") (pinfunction "K") (pintype "passive") (tstamp 3543b231-1dc8-46db-b9ef-2708e19c1568))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220F-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_Pad_D4.0mm" (layer "F.Cu")
    (tstamp 064ca189-16b6-4691-bae0-eb00c29e37cf)
    (at 55 53.975)
    (descr "SMD pad as test Point, diameter 4.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/6d3f0d01-965d-4fe9-a041-9c00fe7ab86b")
    (attr exclude_from_pos_files)
    (fp_text reference "J3" (at 0 -2.898) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 587963ac-a622-4e94-9962-d8b2f25a7a96)
    )
    (fp_text value "Vrail" (at 0 3.1) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2ef93c45-83c8-402b-8110-d5f21bd44c19)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.9) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4528a258-c607-447b-b0b2-68270459cbba)
    )
    (fp_circle (center 0 0) (end 0 2.25)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 7f2d40d6-f552-4c88-9613-243ecbbfee1b))
    (fp_circle (center 0 0) (end 2.5 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 0dda22fd-1168-449d-a3e4-e726665405a8))
    (pad "1" smd circle (at 0 0) (size 4 4) (layers "F.Cu" "F.Mask")
      (net 20 "Net-(D2-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp 996b87b5-ad28-48c1-aaa7-866aa525fba3))
  )

  (footprint "Package_SO:SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm" (layer "F.Cu")
    (tstamp 07180bcb-243a-4aa3-98f7-cd5e27d49a9b)
    (at 62.23 45.72 180)
    (descr "8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true")
    (tags "SSO Stretched SO SOIC 1.27")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/6b993f44-9809-4ab0-ba6c-69600c51226b")
    (attr smd)
    (fp_text reference "U3" (at 0.1 -3.265) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0ffdcd23-190c-406f-8796-0231a5dfd359)
    )
    (fp_text value "UCC23313" (at 0.05 3.385) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ba6844ba-c309-4d63-ad44-c6142c287819)
    )
    (fp_text user "${REFERENCE}" (at 0 -0.065) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a20359b2-3903-4b7d-994d-75e249c0e4fa)
    )
    (fp_line (start -3.55 -2.465) (end -3.55 -1.815)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a7b61e43-73ee-4c3e-a9f9-65129227e7eb))
    (fp_line (start -3.55 -1.8) (end -5.3 -1.8)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e206c237-7925-4f31-b8cc-8b8aca5888cd))
    (fp_line (start -3.5 1.785) (end -3.5 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee427d55-6234-4f42-8cf8-aae144a13e4b))
    (fp_line (start -3.5 2.435) (end 3.55 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c42468f2-41db-4dab-8d69-fe2ce169151a))
    (fp_line (start 3.5 -2.465) (end -3.55 -2.465)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 73473acb-0463-48a5-a4e3-52cbe6c5f522))
    (fp_line (start 3.5 -2.465) (end 3.5 -1.815)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cf9d9942-246a-43ac-bd78-d6da1eb40d5e))
    (fp_line (start 3.55 1.785) (end 3.55 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 086cf38f-cebe-4608-aa3a-795efa4f09a8))
    (fp_line (start -5.6 -2.56) (end -5.6 2.54)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 69c25bdf-e74c-4391-894e-4bee948851e1))
    (fp_line (start -5.6 -2.56) (end 5.6 -2.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3ae97d42-7742-47b1-9056-fda311838746))
    (fp_line (start 5.6 2.54) (end -5.6 2.54)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 298c1ff8-81ff-4cb9-bc3f-bc5c2de5fcd0))
    (fp_line (start 5.6 2.54) (end 5.6 -2.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 17a15af0-f872-40fb-a5f2-e02dfdf41b61))
    (fp_line (start -3.4 2.285) (end -3.4 -1.265)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 2812461e-5d71-45f0-8e69-c198ce3e4063))
    (fp_line (start -2.3 -2.315) (end -3.4 -1.215)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 6219c2a2-51a9-41cd-b60d-34f9d404254f))
    (fp_line (start 3.4 -2.315) (end -2.3 -2.315)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp a809f7eb-9c5e-453b-a414-6230b72e2b1b))
    (fp_line (start 3.4 -2.315) (end 3.4 2.285)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 64b35d4c-fbf2-4452-a600-0d7287274968))
    (fp_line (start 3.4 2.285) (end -3.4 2.285)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 001d40bd-c4e0-4b9b-9bb3-d949110308aa))
    (pad "1" smd rect (at -4.27 -1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(R3-Pad1)") (pinfunction "A") (pintype "passive") (tstamp 94d1693e-7c7c-4011-93c5-5217d3f06e03))
    (pad "2" smd rect (at -4.27 0 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "unconnected-(U3-Pad2)") (pinfunction "NC") (pintype "no_connect") (tstamp af5a3493-bb45-4029-b7da-61c71b4a90f9))
    (pad "3" smd rect (at -4.27 1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive") (tstamp 5dd065ba-351d-4405-b861-edaaf483efc5))
    (pad "4" smd rect (at 4.27 1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(C3-Pad2)") (pinfunction "VEE") (pintype "power_in") (tstamp 6d2ce772-cb84-4cbd-b63c-17a25ad069d0))
    (pad "5" smd rect (at 4.27 0 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(Q3-Pad1)") (pinfunction "VO") (pintype "output") (tstamp 342a5963-ad54-4fd5-aa27-052e7364623d))
    (pad "6" smd rect (at 4.27 -1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(C3-Pad1)") (pinfunction "VCC") (pintype "power_in") (tstamp 0d5c140c-93cd-4671-ad98-e79c2c9e34e1))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-220F-3_Horizontal_TabDown" (layer "F.Cu")
    (tstamp 08e0a802-a54b-442f-a08f-1ec59df5f42a)
    (at 50.96 45.72 90)
    (descr "TO-220F-3, Horizontal, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf")
    (tags "TO-220F-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/0d61e049-a1cc-43d3-bace-605701fbf208")
    (attr through_hole)
    (fp_text reference "Q3" (at 2.54 -20.22 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 244d1ad9-b197-4a57-b87f-5fc20c6cc260)
    )
    (fp_text value "IRF540N" (at 2.54 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ad69574d-324e-4acc-b01b-87bb830d8bca)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -20.22 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c1942837-af42-4cc1-8a69-60adc4750ed5)
    )
    (fp_line (start -2.71 -19.22) (end -2.71 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4072f1d1-1c5b-4175-9883-c16c0678365d))
    (fp_line (start -2.71 -19.22) (end 7.79 -19.22)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5f5b0cce-847e-4ec2-99e8-5e23a27ea9a3))
    (fp_line (start -2.71 -3.11) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6e83bebd-c026-4192-9db7-d3e17bf7486c))
    (fp_line (start 0 -3.11) (end 0 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dfffef38-2045-479a-aa44-2909b232fa6b))
    (fp_line (start 2.54 -3.11) (end 2.54 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5dad9623-8779-4bac-a8e4-0f39c6e75189))
    (fp_line (start 5.08 -3.11) (end 5.08 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 594195fd-c4ce-4a82-a40b-ea46184dc92e))
    (fp_line (start 7.79 -19.22) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4f1f67c0-7171-427d-a963-6588b05dcba6))
    (fp_line (start -2.84 -19.35) (end -2.84 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6bb4f794-4cf6-40b0-8f72-12026af53926))
    (fp_line (start -2.84 1.25) (end 7.92 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dba9052f-5809-4d32-a61a-7eadb6ac0d6a))
    (fp_line (start 7.92 -19.35) (end -2.84 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 266ec22a-44ce-4e15-979a-2ca1af8eb165))
    (fp_line (start 7.92 1.25) (end 7.92 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d7579216-a7e1-4c4f-938b-9c7c1b9450b6))
    (fp_line (start -2.59 -19.1) (end 7.67 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 37be10e0-eca0-49dd-bb55-9f285e0e968a))
    (fp_line (start -2.59 -12.42) (end -2.59 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fa14d27a-e090-476e-a430-595ea34f2c41))
    (fp_line (start -2.59 -12.42) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cbf9234d-3a4e-4422-87b7-750ad8aa2a11))
    (fp_line (start -2.59 -3.23) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 52c4de90-3a03-4a02-92d1-f4350575810e))
    (fp_line (start 0 -3.23) (end 0 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15c30325-5bc7-4fa3-8b00-dbb7143684d1))
    (fp_line (start 2.54 -3.23) (end 2.54 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b0e37dd8-ed33-40cf-a524-905c798240b2))
    (fp_line (start 5.08 -3.23) (end 5.08 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d2f6d16-c7c5-4756-ad9c-f8fa4eb4179b))
    (fp_line (start 7.67 -19.1) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e6b87b87-19de-464f-bbcb-77ac5d06ac1a))
    (fp_line (start 7.67 -12.42) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d7455fb3-fa19-42ec-955d-0ec35b4e4620))
    (fp_line (start 7.67 -12.42) (end 7.67 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b98abdb-edcc-4829-8287-8602f542ce22))
    (fp_line (start 7.67 -3.23) (end -2.59 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d0bb3619-1d0b-4f18-9ffb-aecccedf27b6))
    (fp_circle (center 2.54 -15.8) (end 4.39 -15.8)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp f69d4d6e-3bdb-4541-8022-2418a761679b))
    (pad "" np_thru_hole oval (at 2.54 -15.8 90) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask") (tstamp f4a2123a-5f9c-4130-ab38-b81e4ec5416c))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(Q3-Pad1)") (pinfunction "G") (pintype "input") (tstamp 026cbaf3-52af-4b23-afef-55d5efe82292))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(C2-Pad2)") (pinfunction "D") (pintype "passive") (tstamp e428abd2-ded7-457d-b9cf-7de4d6a426a3))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(C3-Pad2)") (pinfunction "S") (pintype "passive") (tstamp b2bd6327-8355-423a-b6b5-0ee8906e35a8))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220F-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-220F-3_Horizontal_TabDown" (layer "F.Cu")
    (tstamp 155b276b-c973-4ce9-9f73-d1783a8ad9df)
    (at 50.96 34.925 90)
    (descr "TO-220F-3, Horizontal, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf")
    (tags "TO-220F-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/103c19ff-f952-4a8e-8808-6443742e17dc")
    (attr through_hole)
    (fp_text reference "D3" (at 2.54 -20.22 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 70bcceca-1e2e-4179-9af7-27bac1f2e8e5)
    )
    (fp_text value "D_Schottky_x2_ACom_KAK" (at 2.54 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 104596e8-99bc-4abd-8ade-0869551562b4)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -20.22 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e8291a78-10f1-46a1-a970-58296236130d)
    )
    (fp_line (start -2.71 -19.22) (end -2.71 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2f8f487d-1f6d-43ea-bc44-9336e070edb8))
    (fp_line (start -2.71 -19.22) (end 7.79 -19.22)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ca2e4e77-82f7-4802-8227-f7845503dbd7))
    (fp_line (start -2.71 -3.11) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a209be30-a79a-45da-950b-65ff43d30e07))
    (fp_line (start 0 -3.11) (end 0 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0714b3ff-7377-40ca-be87-76d6f184388f))
    (fp_line (start 2.54 -3.11) (end 2.54 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp af7422e3-4805-4023-8aa6-175e9a456a4f))
    (fp_line (start 5.08 -3.11) (end 5.08 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 475ec497-fedb-4f03-9e26-6f2a9eaa7e12))
    (fp_line (start 7.79 -19.22) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3986f4ab-2840-46d3-8ae8-d8c073398faa))
    (fp_line (start -2.84 -19.35) (end -2.84 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 033cf201-5b0c-4bf5-a6e1-b4f1e8105abd))
    (fp_line (start -2.84 1.25) (end 7.92 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 14deaf3b-5c9c-434c-9e64-adda854f848f))
    (fp_line (start 7.92 -19.35) (end -2.84 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f41e2ff1-b5f6-4bf8-b2f4-af3fb8c76658))
    (fp_line (start 7.92 1.25) (end 7.92 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0268ac4a-f8c1-42d8-b983-cb48439836d1))
    (fp_line (start -2.59 -19.1) (end 7.67 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bb708fc5-d849-46b8-a863-ca5781db28b2))
    (fp_line (start -2.59 -12.42) (end -2.59 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5135795c-5c10-4e6f-9cfd-55d4a4dd8aa0))
    (fp_line (start -2.59 -12.42) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 907974fa-acda-4c61-8609-1767e13b8dc3))
    (fp_line (start -2.59 -3.23) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc103442-c35b-4f40-9b0b-1ca2a24f0738))
    (fp_line (start 0 -3.23) (end 0 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 13fccc96-e4e9-4b11-8aa8-f0090cd8155d))
    (fp_line (start 2.54 -3.23) (end 2.54 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 901de756-1dc8-4a95-b306-b63fc1cf58d1))
    (fp_line (start 5.08 -3.23) (end 5.08 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 223e933f-232e-44cc-aa2e-4c3038de432d))
    (fp_line (start 7.67 -19.1) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9664dde9-97de-438f-befb-6b9d7b842886))
    (fp_line (start 7.67 -12.42) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5ab5af88-3bf6-44df-a774-0a628dcd86a6))
    (fp_line (start 7.67 -12.42) (end 7.67 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1be204dc-3319-40ac-8058-57ab7adae2f6))
    (fp_line (start 7.67 -3.23) (end -2.59 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 271e9d90-4dda-4c1c-a358-33b9d96f400d))
    (fp_circle (center 2.54 -15.8) (end 4.39 -15.8)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 15a163a4-dd3c-47ca-ba18-dbd9bbe57f2e))
    (pad "" np_thru_hole oval (at 2.54 -15.8 90) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask") (tstamp 119cc021-b26e-4209-bb5b-4cacc3f13982))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(D2-Pad2)") (pinfunction "K") (pintype "passive") (tstamp 68711c1d-a710-4c6d-865c-e0a1244a80bc))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 0e6b4af1-74ea-4109-91d0-14740826b4c9))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(C3-Pad2)") (pinfunction "K") (pintype "passive") (tstamp d382d052-17d6-497e-bbc1-50c130216d14))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220F-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tstamp 236cba4d-4807-4f56-ae75-bc38ce4a6c34)
    (at 66.04 55.245)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/b22770e1-2648-4c8d-b87d-ef343367423e")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.82) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d8dfb146-e504-403c-9a97-15e41a879078)
    )
    (fp_text value "220" (at 0 1.82) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fffbcea0-42a3-4de9-a6c8-53dc28efe808)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp 607040c7-c820-47bd-8743-924eacb648fb)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a11ebb11-63df-4d7c-ac72-48ea9058bb7a))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 52fa3a05-7d69-4f8d-863d-0e81bddd93c0))
    (fp_line (start -2.45 -1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5ca178ac-7c6c-4bc0-8f96-be11aa3caab6))
    (fp_line (start -2.45 1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9cc34fda-40ee-4ddd-b3d9-3300542cb50a))
    (fp_line (start 2.45 -1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp aca439ef-ae42-4274-addc-9fed401b8c3e))
    (fp_line (start 2.45 1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 46777f40-90b8-4dc9-826d-ead7c88c83d9))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 12d1378a-22c2-408f-9bcc-0b5773a55be3))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 03e054b3-a3a6-4aef-b6d5-74d170891428))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8aeb544b-c91d-46d0-a47b-7377d062de64))
    (fp_line (start 1.6 0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 65c5b9df-4b90-49b7-b7d4-59d218dc724b))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 7 "Net-(R3-Pad1)") (pintype "passive") (tstamp 88442e5f-5978-4e63-b0e9-ac21ac88bba8))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 16 "Net-(J6-Pad3)") (pintype "passive") (tstamp c566ef56-bf43-4a3b-b1d5-77f911700680))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-220F-3_Horizontal_TabDown" (layer "F.Cu")
    (tstamp 34542926-7590-4d8e-b130-268f2cd652ce)
    (at 50.96 56.515 90)
    (descr "TO-220F-3, Horizontal, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf")
    (tags "TO-220F-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/64948c2c-60ab-4071-b2db-801b68debbc6")
    (attr through_hole)
    (fp_text reference "D2" (at 2.54 -20.22 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 254638cc-6d34-4755-9fe0-1d3325a783f0)
    )
    (fp_text value "D_Schottky_x2_ACom_KAK" (at 2.54 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d4a2051d-93b6-480b-87bb-ff7be67e8023)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -20.22 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a13cab7f-b57a-43fe-a3e7-3b903dc3defc)
    )
    (fp_line (start -2.71 -19.22) (end -2.71 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 592e5bd6-01ee-438a-ae77-bde572e9cdfd))
    (fp_line (start -2.71 -19.22) (end 7.79 -19.22)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1dc36414-f65a-47b5-b923-d485a3054496))
    (fp_line (start -2.71 -3.11) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 831ef416-ca88-4eeb-b6e9-89fef542ebb2))
    (fp_line (start 0 -3.11) (end 0 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 32d52f3e-0460-4048-93d3-a4dedd7b159b))
    (fp_line (start 2.54 -3.11) (end 2.54 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 388ce84c-bedc-4c29-b1c3-8e5cb89ddd0a))
    (fp_line (start 5.08 -3.11) (end 5.08 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cd99407a-00b3-4380-91d5-74de41a74e10))
    (fp_line (start 7.79 -19.22) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 04375c67-1dd9-48a5-965b-17e37c0adefb))
    (fp_line (start -2.84 -19.35) (end -2.84 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 216eec76-26bd-4ac6-8a0a-eea04db2ccc5))
    (fp_line (start -2.84 1.25) (end 7.92 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9ed62a8b-b179-439f-9f44-fc2abf8085d1))
    (fp_line (start 7.92 -19.35) (end -2.84 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d931cbaf-b29a-480d-a39a-fb25b8f44ed2))
    (fp_line (start 7.92 1.25) (end 7.92 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8fd0158e-0d9f-4be2-b451-99aa15397779))
    (fp_line (start -2.59 -19.1) (end 7.67 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e7b826e6-d7e8-46d9-a7bb-2ec9398940f3))
    (fp_line (start -2.59 -12.42) (end -2.59 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e74d7087-f41f-43d9-96ba-11cab9ce3803))
    (fp_line (start -2.59 -12.42) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d63e045-24f2-4d2d-a227-41d4744be147))
    (fp_line (start -2.59 -3.23) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3f94b805-c0d5-4c01-9cca-2a6c467cac2a))
    (fp_line (start 0 -3.23) (end 0 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8e12b4b5-5a5c-4616-89e6-3eb36abc57c3))
    (fp_line (start 2.54 -3.23) (end 2.54 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 111c51b1-92b4-4eff-835f-ac49724bcc2c))
    (fp_line (start 5.08 -3.23) (end 5.08 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 42192c9e-60ee-436d-9f74-d1992ca8ba83))
    (fp_line (start 7.67 -19.1) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 38fdc61d-4197-41f9-8d5f-e113672937d8))
    (fp_line (start 7.67 -12.42) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9fc00cc8-996c-48fd-91d6-c68df330a708))
    (fp_line (start 7.67 -12.42) (end 7.67 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 030dd199-a669-465e-af14-f475ca690f7a))
    (fp_line (start 7.67 -3.23) (end -2.59 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f112a52-bb9a-43ff-8b96-c2de319945ce))
    (fp_circle (center 2.54 -15.8) (end 4.39 -15.8)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 11c1f3ba-0648-4fc0-869f-bba9656d23eb))
    (pad "" np_thru_hole oval (at 2.54 -15.8 90) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask") (tstamp 1e214a4c-22d7-429c-8a0b-06e5384574cb))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(D1-Pad2)") (pinfunction "K") (pintype "passive") (tstamp 6e38c492-2714-4a47-9186-8454b83b1658))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 65b8e643-8099-4abe-9292-fae36848c236))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(C2-Pad2)") (pinfunction "K") (pintype "passive") (tstamp 242d7af2-5c9b-48cc-abd5-fc4dedac9e68))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220F-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tstamp 380e6c3d-42fd-48b3-b4b0-46f3d0a61210)
    (at 54.61 67.31 90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/b8d86064-8231-4a32-a836-0812f376effb")
    (attr smd)
    (fp_text reference "C2" (at 0 -2.65 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7304b172-6116-4493-a877-3e987779413f)
    )
    (fp_text value "1uF" (at 0 2.65 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2483ef18-3a66-4572-9917-cf285917a76c)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8677ddd2-1d0d-4911-bf6c-a9f334533289)
    )
    (fp_line (start -1.161252 -1.71) (end 1.161252 -1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8b4a5bae-9cfb-4b1a-9635-19735a6017ba))
    (fp_line (start -1.161252 1.71) (end 1.161252 1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5009cc08-822c-4ae4-942b-e5c0ae7bd3f5))
    (fp_line (start -3.18 -1.95) (end 3.18 -1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 67003e2e-22ea-4f22-b32a-75128bf98bc5))
    (fp_line (start -3.18 1.95) (end -3.18 -1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp da1637a1-d2e8-4c7f-9977-5d0ba6eba38f))
    (fp_line (start 3.18 -1.95) (end 3.18 1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2105787c-4d0e-4eac-8b3b-7e9fed129bcc))
    (fp_line (start 3.18 1.95) (end -3.18 1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e8704a19-b7c3-44a2-a1e2-97751a9b079e))
    (fp_line (start -2.25 -1.6) (end 2.25 -1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b05bf438-cf55-4249-9493-3e2ff83978c3))
    (fp_line (start -2.25 1.6) (end -2.25 -1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 14fa4467-70f7-4424-a13c-3561aa4775a2))
    (fp_line (start 2.25 -1.6) (end 2.25 1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 84889299-d82c-46df-9c86-e4f70810a814))
    (fp_line (start 2.25 1.6) (end -2.25 1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c3ed7613-1e69-4fd3-b305-053b1e91c355))
    (pad "1" smd roundrect (at -2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 28 "Net-(C2-Pad1)") (pintype "passive") (tstamp 76ce3683-e7b2-4924-93be-ed621369fed3))
    (pad "2" smd roundrect (at 2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 27 "Net-(C2-Pad2)") (pintype "passive") (tstamp 5660b9c4-33db-4ef2-87f4-66c90b5abfdd))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tstamp 4060cd7d-0607-40d9-a62a-f67818471c63)
    (at 54.61 24.13 90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/9ae6bedd-433b-4493-89c7-3cd9212b806f")
    (attr smd)
    (fp_text reference "C4" (at 0 -2.65 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61c3fbe2-6643-4f7d-8a57-2e51e0591463)
    )
    (fp_text value "1uF" (at 0 2.65 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b9dce5de-8266-4f6c-a4c3-c2f94d7b5490)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d0a70ce9-dddb-4c59-a233-4109ce8fe632)
    )
    (fp_line (start -1.161252 -1.71) (end 1.161252 -1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 94759f03-015e-48ce-b046-10614a0cf873))
    (fp_line (start -1.161252 1.71) (end 1.161252 1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1218dd94-7fb5-47e2-b349-50b001e98d9c))
    (fp_line (start -3.18 -1.95) (end 3.18 -1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2f375179-01e7-4169-a0b4-d637968bc89f))
    (fp_line (start -3.18 1.95) (end -3.18 -1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 25a8154d-6bba-40db-9e47-04df32a72d66))
    (fp_line (start 3.18 -1.95) (end 3.18 1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ec4fe1d4-c0c0-4b63-9e35-50d20949d61b))
    (fp_line (start 3.18 1.95) (end -3.18 1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a5276c0d-84e8-49d6-b62b-449c364ddebe))
    (fp_line (start -2.25 -1.6) (end 2.25 -1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f5fe79f5-9277-44e9-a70b-e3c53bc62957))
    (fp_line (start -2.25 1.6) (end -2.25 -1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ab6d769a-cdd9-4f96-a2f3-f7a4af9a4d5a))
    (fp_line (start 2.25 -1.6) (end 2.25 1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ebc2ba75-98ea-4ee6-bc6c-8523a2619d97))
    (fp_line (start 2.25 1.6) (end -2.25 1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f2802a12-4de6-4c9f-a208-7b83d995afb7))
    (pad "1" smd roundrect (at -2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 24 "Net-(C4-Pad1)") (pintype "passive") (tstamp 7d5841ab-5e79-4fd3-a8bf-6a2048d97f3a))
    (pad "2" smd roundrect (at 2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 23 "Net-(C4-Pad2)") (pintype "passive") (tstamp 1f53430a-3d81-41fe-92f1-a0a2812c8eaa))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp 462168a7-32c6-42c7-801d-ca46b2d804df)
    (at 71.12 60.325 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/ea88743b-b375-4483-b60f-b0dba05dcdb1")
    (attr through_hole)
    (fp_text reference "J6" (at 0 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a3abd79-d729-4b70-abc4-8114e37ebab3)
    )
    (fp_text value "Conn_01x05_Male" (at 0 12.49) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9899c9d1-36fd-4160-b5c0-681741540ed7)
    )
    (fp_text user "${REFERENCE}" (at 0 5.08 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0a130cdb-0b8a-4b3b-b604-e37e65473948)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e348fdb-40c6-4b55-988f-2e80c8bf8730))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d8c5ff68-810a-48ef-b161-a0d33b2273b1))
    (fp_line (start -1.33 1.27) (end -1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 01f0bbc3-879b-45c5-a8df-9c372b135659))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c931def2-7605-4f81-bdfc-f6f7594c1494))
    (fp_line (start -1.33 11.49) (end 1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 21ecd30f-e316-4c00-94db-c7f93871453b))
    (fp_line (start 1.33 1.27) (end 1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec49d5f3-52e3-4ab3-8df5-e5a386f00329))
    (fp_line (start -1.8 -1.8) (end -1.8 11.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6cd0be82-aaa1-4351-855f-da3b097f3cbb))
    (fp_line (start -1.8 11.95) (end 1.8 11.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7b86819d-c1e9-4e11-9bad-be6ec1059ac7))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 19ca4d52-f46e-4934-9f13-95d3fce8019a))
    (fp_line (start 1.8 11.95) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7343ee50-199e-48e3-9cd6-5b871aa8ee08))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3c9fb010-e05d-4d99-8fd3-468956f32620))
    (fp_line (start -1.27 11.43) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 924e6779-17e6-4212-8f71-b5791743fc4a))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 21cbcf9f-ebd3-459a-a5aa-656529971202))
    (fp_line (start 1.27 -1.27) (end 1.27 11.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c4feed95-eca1-487a-b4b8-432e7b0f62d2))
    (fp_line (start 1.27 11.43) (end -1.27 11.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 664cdfaa-d346-42a8-a619-c3539f5e2b4a))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(J6-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 60e3db67-2672-4a2d-82c9-a22afbb57405))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(J6-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp fba5f783-6313-4f76-8a4c-322e55d83211))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J6-Pad3)") (pinfunction "Pin_3") (pintype "passive") (tstamp d9a45f09-1018-43a0-86ab-0f12a1148906))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(J6-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 7ba6b9e9-72f7-4ed6-a58f-b59908a4b13a))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(J6-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp 49aefd72-8039-4941-a278-b923c390b982))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_Pad_D4.0mm" (layer "F.Cu")
    (tstamp 4e6772e2-68e9-4ec8-8f69-3a144566a700)
    (at 55 75.565)
    (descr "SMD pad as test Point, diameter 4.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/dcede888-71fe-46c8-a547-f334235f12e3")
    (attr exclude_from_pos_files)
    (fp_text reference "J2" (at 0 -2.898) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8011f26a-966e-4d21-ad41-b2fee8b6bda3)
    )
    (fp_text value "Vrail" (at 0 3.1) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1ca22912-1a0f-459e-8f62-aa4472acfaf9)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.9) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1ded3dd0-0503-4ca2-b381-17db0d3b64fd)
    )
    (fp_circle (center 0 0) (end 0 2.25)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp f1667fbe-2c60-497e-ad85-e6af4fe16735))
    (fp_circle (center 0 0) (end 2.5 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp d8a365be-8560-49d0-b931-1cc1bd088e03))
    (pad "1" smd circle (at 0 0) (size 4 4) (layers "F.Cu" "F.Mask")
      (net 21 "Net-(D1-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp be26b5f9-cf18-4af0-b74c-bdfe20e52ce7))
  )

  (footprint "TestPoint:TestPoint_Pad_D4.0mm" (layer "F.Cu")
    (tstamp 50b8fd33-52bd-4eb3-bd3b-0863f1d258bf)
    (at 55 32.385)
    (descr "SMD pad as test Point, diameter 4.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/2714a589-d508-4a73-a7c9-0c477ea7458b")
    (attr exclude_from_pos_files)
    (fp_text reference "J4" (at 0 -2.898) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bd05f3fd-a169-47c9-8ba4-38caa44190b2)
    )
    (fp_text value "Vrail" (at 0 3.1) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7f2f98ea-7859-45a9-bebf-9de194d082d1)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.9) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ce1f0d05-126c-4f42-81e3-7329543affdf)
    )
    (fp_circle (center 0 0) (end 0 2.25)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 34e6ca43-c210-4d7b-baff-e477fed158e6))
    (fp_circle (center 0 0) (end 2.5 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 6e173f69-75a5-48fb-80ea-634dbdb7260e))
    (pad "1" smd circle (at 0 0) (size 4 4) (layers "F.Cu" "F.Mask")
      (net 19 "Net-(D3-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp 0d74f634-4a46-4e90-926f-5791719bf785))
  )

  (footprint "Diode_SMD:D_SOD-323" (layer "F.Cu")
    (tstamp 5463c1dd-1328-4484-9b76-26638cbbefb2)
    (at 55.88 50.165)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/0a3e9348-2132-40e8-9662-35d174d54215")
    (attr smd)
    (fp_text reference "D6" (at 0 -1.85) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13f68a44-2042-4162-a7ae-ee6892b000a0)
    )
    (fp_text value "1N4148WS" (at 0.1 1.9) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 27744a30-fa62-461d-8802-89fb3c28486b)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.85) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp addb1c8a-6fd5-475b-8366-63ff919f1a44)
    )
    (fp_line (start -1.5 -0.85) (end -1.5 0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp abf96c63-004b-417f-8320-1446d45f9382))
    (fp_line (start -1.5 -0.85) (end 1.05 -0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9611f581-c436-4777-965a-e4520733cd96))
    (fp_line (start -1.5 0.85) (end 1.05 0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6dd997ad-fb05-4e73-a3cd-6b08d4be4a6f))
    (fp_line (start -1.6 -0.95) (end -1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bf939759-86d2-4991-8c9f-170588a94669))
    (fp_line (start -1.6 -0.95) (end 1.6 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f5802252-eb88-40a6-9985-71764496aa8e))
    (fp_line (start -1.6 0.95) (end 1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ba6070a5-2853-4d53-862a-a9c1dd935340))
    (fp_line (start 1.6 -0.95) (end 1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 277a91bb-6f37-4fc6-9ef6-7a582f9268f8))
    (fp_line (start -0.9 -0.7) (end 0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d659b0da-d469-47a0-b529-fc9525e200a6))
    (fp_line (start -0.9 0.7) (end -0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 78f822e5-ffa9-4e54-8696-73f35bcd539f))
    (fp_line (start -0.3 -0.35) (end -0.3 0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 08391d2f-cb36-4866-be23-c73ff49d914a))
    (fp_line (start -0.3 0) (end -0.5 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3739dee9-724a-46e6-a771-8a301c81c1b5))
    (fp_line (start -0.3 0) (end 0.2 -0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb2dfbc8-97e7-4673-a5b7-8bb94f878375))
    (fp_line (start 0.2 -0.35) (end 0.2 0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e5e0efd9-62a7-4f30-90c1-f55acceea91d))
    (fp_line (start 0.2 0) (end 0.45 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 84ceef47-872c-4273-bd51-9c99564e3a4f))
    (fp_line (start 0.2 0.35) (end -0.3 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8a805154-0a10-4493-8201-a6768aa49b71))
    (fp_line (start 0.9 -0.7) (end 0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bd4e8554-6a1c-40f0-bfe9-9a94f35c7ed0))
    (fp_line (start 0.9 0.7) (end -0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 541bc26f-5171-4578-b5b9-dc2d92cead4a))
    (pad "1" smd rect (at -1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(C3-Pad1)") (pinfunction "K") (pintype "passive") (tstamp cefef4e2-df30-4fd9-87ae-baa96ad36df1))
    (pad "2" smd rect (at 1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 2db59cad-1790-44c4-8f12-76ed8ec40a57))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_Pad_D4.0mm" (layer "F.Cu")
    (tstamp 579a02b7-18fe-48da-a9d3-961850f062a4)
    (at 55 19.05)
    (descr "SMD pad as test Point, diameter 4.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/6c7744a1-d107-4098-aeda-4a0e18b23c66")
    (attr exclude_from_pos_files)
    (fp_text reference "J5" (at 0 -2.898) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 644bea4c-e7d7-491c-9d18-7b978cd5c951)
    )
    (fp_text value "Vrail" (at 0 3.1) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1288a721-64c9-4957-8902-ed75fc8c46f8)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.9) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 09458b0c-9a39-4b0c-bb96-3d05d2d7da32)
    )
    (fp_circle (center 0 0) (end 0 2.25)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp ef4b0dc8-d1bf-4d8f-8a65-7ec4745f50db))
    (fp_circle (center 0 0) (end 2.5 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 1623a861-d17d-4c83-a0cf-ce189f216617))
    (pad "1" smd circle (at 0 0) (size 4 4) (layers "F.Cu" "F.Mask")
      (net 23 "Net-(C4-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp e529e155-4ec5-4a6d-9cdf-938c9accea16))
  )

  (footprint "Diode_SMD:D_SOD-323" (layer "F.Cu")
    (tstamp 5ea149ce-c08b-45c8-8601-614ff488ad27)
    (at 55.88 28.575)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/79504c3b-fee1-4e04-94d0-83e4de817446")
    (attr smd)
    (fp_text reference "D7" (at 0 -1.85) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0b354613-0b73-44e6-b290-0c13af83f0d3)
    )
    (fp_text value "1N4148WS" (at 0.1 1.9) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 142655ef-75c6-4cde-83ad-437dd8ea0e78)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.85) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d1626866-dc55-41f0-b4dd-0a4b52c90bdf)
    )
    (fp_line (start -1.5 -0.85) (end -1.5 0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 09d976b1-0d74-4a62-9c78-83d0dcde6dcf))
    (fp_line (start -1.5 -0.85) (end 1.05 -0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eca507f5-eb96-40a6-8230-8fe094c08e2e))
    (fp_line (start -1.5 0.85) (end 1.05 0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec6e0f5d-f138-4aaf-b991-fcea5bbfd958))
    (fp_line (start -1.6 -0.95) (end -1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3080fc15-eb39-4ebb-bdab-1caede128279))
    (fp_line (start -1.6 -0.95) (end 1.6 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f974dc01-d54b-4ae7-9fb9-f3b110bf5a4e))
    (fp_line (start -1.6 0.95) (end 1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8491d17d-5404-4b7c-8a05-2bc59be3589f))
    (fp_line (start 1.6 -0.95) (end 1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a48c8506-b70f-42e8-a1ac-4ddc2fcaa841))
    (fp_line (start -0.9 -0.7) (end 0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ffa67015-8f37-449c-887a-779df27f82c2))
    (fp_line (start -0.9 0.7) (end -0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 81bc70f4-cc31-4d2d-9563-a207b0baecac))
    (fp_line (start -0.3 -0.35) (end -0.3 0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 21385ccc-c7b8-450a-9747-d153f2a77254))
    (fp_line (start -0.3 0) (end -0.5 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bf8c41a6-4c17-499d-8073-43c9608e70bc))
    (fp_line (start -0.3 0) (end 0.2 -0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48b6ec3a-9404-4b25-9e9c-437fb1af25c3))
    (fp_line (start 0.2 -0.35) (end 0.2 0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fcd5cb79-8c2b-419b-a669-e6c1de1c1600))
    (fp_line (start 0.2 0) (end 0.45 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1bb7f379-5af7-4819-b8db-85c3a3490d11))
    (fp_line (start 0.2 0.35) (end -0.3 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 41a49a43-5c51-4f2a-8435-9c90e7f43791))
    (fp_line (start 0.9 -0.7) (end 0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b41197fa-bde5-4a41-8f46-c4218f36fc10))
    (fp_line (start 0.9 0.7) (end -0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 42c08329-aa68-4c50-984e-b2fe13b90403))
    (pad "1" smd rect (at -1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(C4-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 6aaf8c2d-19b2-4ee2-8e9b-3af413c50741))
    (pad "2" smd rect (at 1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 7b9a9211-774e-47c5-9d78-c0001639e370))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tstamp 638df845-dead-4768-b608-f0a829544613)
    (at 54.61 45.72 90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/d2387b1e-b412-4b02-8003-d9451de9b077")
    (attr smd)
    (fp_text reference "C3" (at 0 -2.65 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1ffde10a-d7f5-4b57-ad0a-797f639096d3)
    )
    (fp_text value "1uF" (at 0 2.65 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f14aac3d-c8ad-49a3-9058-bd08e9897b58)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 40f6d5ba-d3e5-4ada-b260-a8d96bcc753f)
    )
    (fp_line (start -1.161252 -1.71) (end 1.161252 -1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d759d2d-fb85-463c-a50e-92b9d8c7f576))
    (fp_line (start -1.161252 1.71) (end 1.161252 1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e236fe21-e530-48e4-bd2f-1e4b01f107b0))
    (fp_line (start -3.18 -1.95) (end 3.18 -1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7371d0fb-f8b3-44f1-b0af-fb488536e353))
    (fp_line (start -3.18 1.95) (end -3.18 -1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a544f869-36be-4651-937d-0a8f07f2dd0b))
    (fp_line (start 3.18 -1.95) (end 3.18 1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 543467c3-34d8-4e0f-8cff-c7f4e78eb7d8))
    (fp_line (start 3.18 1.95) (end -3.18 1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9d3d7746-fbb5-423e-9afa-9acf9c888087))
    (fp_line (start -2.25 -1.6) (end 2.25 -1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb6fb0cd-46cd-4d60-958e-986ab9195019))
    (fp_line (start -2.25 1.6) (end -2.25 -1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 72af9104-3bbf-49ff-97fb-0ea78187c097))
    (fp_line (start 2.25 -1.6) (end 2.25 1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e58ba01d-3634-4779-8388-133c09375a3f))
    (fp_line (start 2.25 1.6) (end -2.25 1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec6ee90c-989b-4f43-8a73-3e221124c44c))
    (pad "1" smd roundrect (at -2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 26 "Net-(C3-Pad1)") (pintype "passive") (tstamp 601a0d1c-055f-49d2-a040-0d413c6c7fdd))
    (pad "2" smd roundrect (at 2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 25 "Net-(C3-Pad2)") (pintype "passive") (tstamp 67a3b5c7-12d0-42e3-98f3-cc71f7edfb2b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tstamp 66db1ee0-bb01-454c-8e2e-5e25ffa7dfb8)
    (at 54.61 88.9 90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/78342f3e-150e-4758-bb17-bb08aac44f14")
    (attr smd)
    (fp_text reference "C1" (at 0 -2.65 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0c718d80-629f-4dc1-a708-ac99a6ff4be4)
    )
    (fp_text value "1uF" (at 0 2.65 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b97d4b6d-01a4-4f1f-98d1-9290d81e26d7)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 48404b1e-6193-4c0d-b82a-e3c956c76791)
    )
    (fp_line (start -1.161252 -1.71) (end 1.161252 -1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5ab7424d-7a2c-4b6b-b9fb-0df31a938546))
    (fp_line (start -1.161252 1.71) (end 1.161252 1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b63ad90e-a594-4f6a-92ad-e649b5e656f9))
    (fp_line (start -3.18 -1.95) (end 3.18 -1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp faf8b046-33bf-45da-ae22-97f36ebf0672))
    (fp_line (start -3.18 1.95) (end -3.18 -1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 569c1c27-85da-4113-9093-be2de03339b6))
    (fp_line (start 3.18 -1.95) (end 3.18 1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9291d982-303c-4c72-a1d2-7216d8aa8b64))
    (fp_line (start 3.18 1.95) (end -3.18 1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 367fed3f-d058-4e76-8d1e-d5d7a4f480c7))
    (fp_line (start -2.25 -1.6) (end 2.25 -1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d76a0ffb-c0ad-46b8-b762-deb83fae5322))
    (fp_line (start -2.25 1.6) (end -2.25 -1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1a15d5a2-4419-4021-811e-072dbb4e146d))
    (fp_line (start 2.25 -1.6) (end 2.25 1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6f9fe4a0-b3d3-4938-9498-8456a677dc14))
    (fp_line (start 2.25 1.6) (end -2.25 1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f688224-0374-4644-85da-55536a79d685))
    (pad "1" smd roundrect (at -2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 30 "Net-(C1-Pad1)") (pintype "passive") (tstamp 9f2e9778-43c9-47d4-a2ce-592bc734cce7))
    (pad "2" smd roundrect (at 2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 29 "Net-(C1-Pad2)") (pintype "passive") (tstamp 16702f6a-8b7f-497f-8833-01bdb30e7b7f))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm" (layer "F.Cu")
    (tstamp 6b0a3fd6-7a08-4cc4-bcd8-19cc36fd4d9f)
    (at 62.23 24.13 180)
    (descr "8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true")
    (tags "SSO Stretched SO SOIC 1.27")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/d1880de2-4770-45c9-9426-3250938971af")
    (attr smd)
    (fp_text reference "U4" (at 0.1 -3.265) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5a6e20ef-98e0-4286-ad17-e34874804e67)
    )
    (fp_text value "UCC23313" (at 0.05 3.385) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 015ba8be-3a70-4f8d-a452-45a43e1727aa)
    )
    (fp_text user "${REFERENCE}" (at 0 -0.065) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c6e07da2-c4f2-4362-878d-9334df94c5d0)
    )
    (fp_line (start -3.55 -2.465) (end -3.55 -1.815)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b2d6b2a6-5d7c-435f-8b95-378a83db3109))
    (fp_line (start -3.55 -1.8) (end -5.3 -1.8)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e4d6c244-e91f-4d69-be06-f57690c6fea4))
    (fp_line (start -3.5 1.785) (end -3.5 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 18cc4b23-2fcb-4824-b616-c040b6056cf4))
    (fp_line (start -3.5 2.435) (end 3.55 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 173b1d61-de4f-4117-a3a2-0852cc695dbe))
    (fp_line (start 3.5 -2.465) (end -3.55 -2.465)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 71cb7672-77f7-4e41-9b08-03a2851d65e4))
    (fp_line (start 3.5 -2.465) (end 3.5 -1.815)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8d745565-3e1b-457d-881f-d56e1af60e31))
    (fp_line (start 3.55 1.785) (end 3.55 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cec4ddcc-4aa3-436d-8069-9681675a2e12))
    (fp_line (start -5.6 -2.56) (end -5.6 2.54)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6c946640-66f3-4365-a0e0-2ba6a1107d4e))
    (fp_line (start -5.6 -2.56) (end 5.6 -2.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c81b8ada-5c05-40ac-8d3b-36fec6acc806))
    (fp_line (start 5.6 2.54) (end -5.6 2.54)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6ea2e355-c8d4-4fb9-a241-2b2a596ad8ef))
    (fp_line (start 5.6 2.54) (end 5.6 -2.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a4d01c3d-7afc-400e-b1af-95429cc0cb1c))
    (fp_line (start -3.4 2.285) (end -3.4 -1.265)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 28e4e130-0cb5-4153-9274-3394bb5b3c22))
    (fp_line (start -2.3 -2.315) (end -3.4 -1.215)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 116b155e-6427-4ba1-a6d1-3ab1d34e59db))
    (fp_line (start 3.4 -2.315) (end -2.3 -2.315)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 315841d9-89c7-42f7-ad7e-f223cef2c182))
    (fp_line (start 3.4 -2.315) (end 3.4 2.285)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 4080e639-64f6-48d9-bfa9-c97c06bbeb37))
    (fp_line (start 3.4 2.285) (end -3.4 2.285)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 220fd1ec-df36-4e52-9082-56d274b37e2f))
    (pad "1" smd rect (at -4.27 -1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(R4-Pad1)") (pinfunction "A") (pintype "passive") (tstamp 01b8239e-bb9e-44a8-b458-57600c11c092))
    (pad "2" smd rect (at -4.27 0 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "unconnected-(U4-Pad2)") (pinfunction "NC") (pintype "no_connect") (tstamp 9ee5f7e9-46da-4f51-b31d-7308302caf52))
    (pad "3" smd rect (at -4.27 1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive") (tstamp aebc29a3-8766-4a4d-b6b9-8a7d51ce157a))
    (pad "4" smd rect (at 4.27 1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(C4-Pad2)") (pinfunction "VEE") (pintype "power_in") (tstamp adf8e68f-d2bb-49e2-9275-2b719e183d42))
    (pad "5" smd rect (at 4.27 0 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(Q4-Pad1)") (pinfunction "VO") (pintype "output") (tstamp 78290c2e-6132-4a03-8582-4527dbf732b8))
    (pad "6" smd rect (at 4.27 -1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(C4-Pad1)") (pinfunction "VCC") (pintype "power_in") (tstamp 4fca1bab-a619-481d-b1ce-6c33d724c1b9))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tstamp 6c939d27-efc9-443a-ba44-92b8fdb3a204)
    (at 66.04 52.705)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/e97640da-bd7c-4fbc-b49d-4ea42bdf9f26")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.82) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 416434f7-5bea-46ba-9411-f89518a99dba)
    )
    (fp_text value "220" (at 0 1.82) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp eba39d76-6585-4c12-aa6c-ec02a609d836)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp cf201b3a-e270-4569-8e0a-c294a938ba9e)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 98530bf7-e475-4583-b899-bac0a6e7dd36))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aaf62aaa-bfc5-4bc0-b5cf-0b2cc481d35d))
    (fp_line (start -2.45 -1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8c0238e8-8b06-463f-a3e0-1623ea7ff0ae))
    (fp_line (start -2.45 1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fd2545e8-7cdc-41ac-9a22-6bd47ddb25d8))
    (fp_line (start 2.45 -1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c624d2dd-a083-4fcf-b07d-55aaa8d99f52))
    (fp_line (start 2.45 1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fa8678aa-9773-4e68-8a4f-1e4ce2fe3663))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 111ad5d2-968c-40f1-b260-995e0dc10974))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77c35469-729a-44e3-a813-0370b813c630))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c5cd4e3d-9056-4628-8b06-75c93ad6aa48))
    (fp_line (start 1.6 0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1e2dc1a0-db6d-49c9-b0f4-2b317f2c4410))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "Net-(R4-Pad1)") (pintype "passive") (tstamp bb7e0dda-51f2-4167-a5b5-daede60cd1cc))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 15 "Net-(J6-Pad4)") (pintype "passive") (tstamp f5009c7c-d99c-4ba1-9292-fe9bd0ee358c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-220F-3_Horizontal_TabDown" (layer "F.Cu")
    (tstamp 733641bc-affc-45c8-bec9-2bb667df108c)
    (at 50.96 88.9 90)
    (descr "TO-220F-3, Horizontal, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf")
    (tags "TO-220F-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/f27fdfd6-3fe3-49f4-aa87-1fd3cb02d496")
    (attr through_hole)
    (fp_text reference "Q1" (at 2.54 -20.22 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9074b8a4-b838-4126-ab93-327e22a72ae9)
    )
    (fp_text value "IRF540N" (at 2.54 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b7c86368-c38d-4bd5-a043-7aab4bc5d64f)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -20.22 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8e69e457-e018-43b6-8d13-f6f68a5c26c0)
    )
    (fp_line (start -2.71 -19.22) (end -2.71 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 41caa78e-890d-4a82-88ca-48da37860d18))
    (fp_line (start -2.71 -19.22) (end 7.79 -19.22)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 99489398-b155-4cf1-a614-e91e1d2e5e3a))
    (fp_line (start -2.71 -3.11) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6fcfb407-05d2-415f-91c6-e32dbd20b1e4))
    (fp_line (start 0 -3.11) (end 0 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e95e79b-bfb2-4f14-8da0-7fbda5829b79))
    (fp_line (start 2.54 -3.11) (end 2.54 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 908dd07b-7ee3-4ae1-be89-5d9fadcf3558))
    (fp_line (start 5.08 -3.11) (end 5.08 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f491adb7-b844-4a36-99c5-78db9cceef08))
    (fp_line (start 7.79 -19.22) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9fa589a-94f3-4480-8d15-56e046f3c09c))
    (fp_line (start -2.84 -19.35) (end -2.84 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3cb0a2d1-cb4e-4f2a-bad0-460494920d25))
    (fp_line (start -2.84 1.25) (end 7.92 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f6673cc7-cc72-41ee-bd2f-ddd2204601d5))
    (fp_line (start 7.92 -19.35) (end -2.84 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 065bda24-6699-4bd0-8e62-8995b3a1500c))
    (fp_line (start 7.92 1.25) (end 7.92 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 767f3e69-bee1-412f-888f-f7d1b8a64aaf))
    (fp_line (start -2.59 -19.1) (end 7.67 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 91d75f7f-cdd2-4771-a95d-781410b39d5f))
    (fp_line (start -2.59 -12.42) (end -2.59 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp de42d08b-aa44-4ee6-9a50-a8101725d91b))
    (fp_line (start -2.59 -12.42) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d8565841-e825-4057-b5c8-4726e8dc50ed))
    (fp_line (start -2.59 -3.23) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b8c9489-4e08-4e7e-a232-33f511d1fde5))
    (fp_line (start 0 -3.23) (end 0 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ac08ca18-909d-497d-9d80-4304b95f6456))
    (fp_line (start 2.54 -3.23) (end 2.54 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c36c136d-95c9-4428-98d3-e6c4345241ae))
    (fp_line (start 5.08 -3.23) (end 5.08 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4e810007-41c2-4691-95fc-92e24a55bddf))
    (fp_line (start 7.67 -19.1) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 82f3a002-d8a3-4e76-a924-eb5b99e22a9c))
    (fp_line (start 7.67 -12.42) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 953a072b-dc11-47d6-a071-0f841a1e1144))
    (fp_line (start 7.67 -12.42) (end 7.67 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7d44579d-56c7-4223-8911-8b29982023ce))
    (fp_line (start 7.67 -3.23) (end -2.59 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 639ad93e-01b1-46f4-bf2a-bd4dfebeacd0))
    (fp_circle (center 2.54 -15.8) (end 4.39 -15.8)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp da14ffe2-d068-4eed-a5a4-9fdafdf42040))
    (pad "" np_thru_hole oval (at 2.54 -15.8 90) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask") (tstamp 551d6617-44a0-48dc-936e-956f597aa2ac))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input") (tstamp bc376bcf-ad8e-4ea1-aa05-5ee89f4edffe))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(D1-Pad1)") (pinfunction "D") (pintype "passive") (tstamp e8b32254-46d6-45e2-8bec-c97221dd253d))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(C1-Pad2)") (pinfunction "S") (pintype "passive") (tstamp 09598763-9554-4a5d-89a9-ab181f7702f6))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220F-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm" (layer "F.Cu")
    (tstamp 78728fde-44bd-488b-bb7e-284047127998)
    (at 62.23 88.9 180)
    (descr "8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true")
    (tags "SSO Stretched SO SOIC 1.27")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/5ef7239f-ff2b-4b64-adc3-d394f8cf897c")
    (attr smd)
    (fp_text reference "U1" (at 0.1 -3.265) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1b53c504-df9a-44d2-9171-18ecb41cf59b)
    )
    (fp_text value "UCC23313" (at 0.05 3.385) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4366dd47-a822-4c1b-a655-c2212761834c)
    )
    (fp_text user "${REFERENCE}" (at 0 -0.065) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8228fec0-2ec9-4c1f-a6f0-cb1cb7d0fb61)
    )
    (fp_line (start -3.55 -2.465) (end -3.55 -1.815)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8321c67d-d7d2-4d05-93e3-1d46e908910b))
    (fp_line (start -3.55 -1.8) (end -5.3 -1.8)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e231f163-c521-4fb1-9901-fe214a025be8))
    (fp_line (start -3.5 1.785) (end -3.5 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6919c1f9-a017-4f49-9099-ab63d5ab7d1e))
    (fp_line (start -3.5 2.435) (end 3.55 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7f1465bc-220b-4065-839b-18c6ee7f11e5))
    (fp_line (start 3.5 -2.465) (end -3.55 -2.465)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a2e29b48-4cca-44e8-bb90-c599e478ee38))
    (fp_line (start 3.5 -2.465) (end 3.5 -1.815)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 969a57ad-1bff-4a55-989e-117091f85d50))
    (fp_line (start 3.55 1.785) (end 3.55 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d78895f-373a-4a10-96ca-fd58415da410))
    (fp_line (start -5.6 -2.56) (end -5.6 2.54)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b2bea1c4-3bbd-422c-88d0-7f58b8148819))
    (fp_line (start -5.6 -2.56) (end 5.6 -2.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c23533a6-02a0-4106-a477-8ebaaf83fa5c))
    (fp_line (start 5.6 2.54) (end -5.6 2.54)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 403f2813-1894-4306-9fd9-607bfc4705db))
    (fp_line (start 5.6 2.54) (end 5.6 -2.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0b34102b-5993-42b2-a167-88c76e09519e))
    (fp_line (start -3.4 2.285) (end -3.4 -1.265)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp ebd26c2d-f2be-49be-8589-106283e6ee9b))
    (fp_line (start -2.3 -2.315) (end -3.4 -1.215)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 3398c9ce-0445-4200-a9e9-10dc7a8aaa84))
    (fp_line (start 3.4 -2.315) (end -2.3 -2.315)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 2b3a59e1-253b-48ca-a3ef-da12ad9dea8c))
    (fp_line (start 3.4 -2.315) (end 3.4 2.285)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 0a57c4c3-ec9f-4d95-a318-e78e97a35c89))
    (fp_line (start 3.4 2.285) (end -3.4 2.285)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp b2d80bfa-675c-4847-aae0-dba7e4ca12b2))
    (pad "1" smd rect (at -4.27 -1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(R1-Pad1)") (pinfunction "A") (pintype "passive") (tstamp 2c4fc5ba-3ab2-46af-8391-900dc522bfe0))
    (pad "2" smd rect (at -4.27 0 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "unconnected-(U1-Pad2)") (pinfunction "NC") (pintype "no_connect") (tstamp 00860bf9-c8e3-4a56-ad72-7be37a4e2849))
    (pad "3" smd rect (at -4.27 1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive") (tstamp d145e37e-c08f-4657-80f5-77cc606a6ad9))
    (pad "4" smd rect (at 4.27 1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(C1-Pad2)") (pinfunction "VEE") (pintype "power_in") (tstamp 0fbc43ec-43c4-41bd-b321-f9fe367dc219))
    (pad "5" smd rect (at 4.27 0 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(Q1-Pad1)") (pinfunction "VO") (pintype "output") (tstamp 0cf4fd33-b545-4291-8391-9cbfa5af965e))
    (pad "6" smd rect (at 4.27 -1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(C1-Pad1)") (pinfunction "VCC") (pintype "power_in") (tstamp b1cb8543-c9e8-404b-b665-c68df83149a6))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-323" (layer "F.Cu")
    (tstamp 90136890-1b41-4fd9-a370-e845a09d9f31)
    (at 58.42 92.71)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/dc92bbb3-2215-498d-9573-47843642432e")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.85) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a29d845c-e89e-408f-8fce-f030fafb8e4b)
    )
    (fp_text value "1N4148WS" (at 0.1 1.9) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 04585ade-e905-4ea3-b67c-5c420c90f709)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.85) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8d41bdeb-8f28-4dc0-b245-2e16ae6365cc)
    )
    (fp_line (start -1.5 -0.85) (end -1.5 0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a1b83702-aeb5-450b-a862-6dfde4eda4de))
    (fp_line (start -1.5 -0.85) (end 1.05 -0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4f8cdeb0-4361-4044-b614-cfd77e742fe1))
    (fp_line (start -1.5 0.85) (end 1.05 0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e768831c-d304-448a-acee-f854d75fb0de))
    (fp_line (start -1.6 -0.95) (end -1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1b0b97e4-5dff-4c0c-98db-d7d5b845b99a))
    (fp_line (start -1.6 -0.95) (end 1.6 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 00767ee9-4043-4887-a2ea-b66732953aef))
    (fp_line (start -1.6 0.95) (end 1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6886ff2e-a747-4055-a49b-744a7179b577))
    (fp_line (start 1.6 -0.95) (end 1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2850b88e-292e-4442-941a-2972969c43c2))
    (fp_line (start -0.9 -0.7) (end 0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8839de2c-98be-41af-a970-6c2c205baa51))
    (fp_line (start -0.9 0.7) (end -0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fefcd923-875c-4a29-ac66-1eb30f7c8fbc))
    (fp_line (start -0.3 -0.35) (end -0.3 0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a86fabb5-c388-400a-83aa-feb9aca07ea2))
    (fp_line (start -0.3 0) (end -0.5 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a0889ac2-432a-4219-a924-5cfc743eca17))
    (fp_line (start -0.3 0) (end 0.2 -0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 90babfae-3ee4-4eac-afd6-c3d74d7abf1e))
    (fp_line (start 0.2 -0.35) (end 0.2 0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7bea006f-f030-4617-b3f7-d9731b0e1be5))
    (fp_line (start 0.2 0) (end 0.45 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2ad63a3f-37fa-44a1-9842-69726663bc01))
    (fp_line (start 0.2 0.35) (end -0.3 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 87f386ea-4a54-4b8c-8441-088b128bd4d8))
    (fp_line (start 0.9 -0.7) (end 0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0b7c6244-36e7-41b4-868c-4efa6971163b))
    (fp_line (start 0.9 0.7) (end -0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b3549472-1848-4e34-8328-7ed5da8ab5e2))
    (pad "1" smd rect (at -1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(C1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 0bf073ce-ad0f-4484-822a-5ebe1e9fe87b))
    (pad "2" smd rect (at 1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(D1-Pad1)") (pinfunction "A") (pintype "passive") (tstamp 44c30956-aed3-46e2-97ad-50d477d30d55))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tstamp 95e0e62d-068a-48c8-a653-c85e04a0da48)
    (at 66.04 60.325)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/93eb1227-ce5b-475b-8ec0-3a22879e6612")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.82) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c8931620-b7d1-4f64-800c-dc639e01584f)
    )
    (fp_text value "220" (at 0 1.82) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e19210c9-9f53-46bb-a835-7ccf0b55ff7b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp 5d3e30f6-bc0f-4467-a7ac-cff055282c24)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 08b157da-766c-4b51-8561-fc75a8b1c29a))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9d1f8690-52a3-4468-9a71-a88c051d0f1e))
    (fp_line (start -2.45 -1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f24c7427-e0a5-4215-b801-5a7fdae032e1))
    (fp_line (start -2.45 1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2063b26f-55a2-4980-8bb2-6650e4653188))
    (fp_line (start 2.45 -1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 845202ca-7007-4c8b-b0a8-2210d8a79e5c))
    (fp_line (start 2.45 1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f6e3a7c0-1a36-439d-853e-6cf7d207db73))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bb3b89ef-b2d1-40e2-8976-24fcc35ae991))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2bf4a677-a6f7-4857-9397-41b4071ef310))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 754f9ed8-3adb-413d-91eb-358fe79b5dd2))
    (fp_line (start 1.6 0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f7fae986-d222-49f7-9f24-d8027773ce65))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 9 "Net-(R1-Pad1)") (pintype "passive") (tstamp c84845d2-2f7e-47a1-8114-2a49a6b2013d))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 18 "Net-(J6-Pad1)") (pintype "passive") (tstamp 4310bd3b-5565-4eb4-bb3b-00be41947552))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-220F-3_Horizontal_TabDown" (layer "F.Cu")
    (tstamp 9e89f996-cf5c-4934-bd2c-d2d64aa3c447)
    (at 50.96 67.31 90)
    (descr "TO-220F-3, Horizontal, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf")
    (tags "TO-220F-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/bd89e833-d02e-4730-b42f-4ed1ea200c42")
    (attr through_hole)
    (fp_text reference "Q2" (at 2.54 -20.22 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp be526b42-257b-4aca-810e-9981cf059e6f)
    )
    (fp_text value "IRF540N" (at 2.54 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ff838cfb-b5d8-444d-a60a-fcc28767b5f0)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -20.22 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp eea39e02-a347-4434-97b3-225e033c054f)
    )
    (fp_line (start -2.71 -19.22) (end -2.71 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f52d63e4-f6b2-47f2-abc8-242815779bb4))
    (fp_line (start -2.71 -19.22) (end 7.79 -19.22)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9de5f914-c179-490c-90c0-b655608d243c))
    (fp_line (start -2.71 -3.11) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 72de0e39-2d42-46cf-9d1f-fec0f43f5df9))
    (fp_line (start 0 -3.11) (end 0 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6f6d9d94-541e-40ef-ae3b-629b4b0314df))
    (fp_line (start 2.54 -3.11) (end 2.54 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 41d403d7-e1ef-48a5-b6a5-e037e0cb42b5))
    (fp_line (start 5.08 -3.11) (end 5.08 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 360a9d49-f260-467b-8a1f-3890f82203e2))
    (fp_line (start 7.79 -19.22) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0409e8de-6290-4e1e-9742-9150342e7f47))
    (fp_line (start -2.84 -19.35) (end -2.84 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b3940e9b-dcb8-4212-8c02-cc5b9875e841))
    (fp_line (start -2.84 1.25) (end 7.92 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp aaed403d-b851-4a7d-aed1-e12e5217d95b))
    (fp_line (start 7.92 -19.35) (end -2.84 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4903ad12-9274-49e6-896a-0ba18048e9ec))
    (fp_line (start 7.92 1.25) (end 7.92 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fc28151b-9e88-4243-a483-f6ec13ce9ea2))
    (fp_line (start -2.59 -19.1) (end 7.67 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f3c3a0ec-208d-4912-a4aa-feeb9f111b70))
    (fp_line (start -2.59 -12.42) (end -2.59 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c50072e0-a05d-4580-9db6-fadd31652728))
    (fp_line (start -2.59 -12.42) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 28faec5d-5034-482e-892f-a5c01ca458aa))
    (fp_line (start -2.59 -3.23) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aec10ba3-c61b-4575-b3b5-e22a02671ccd))
    (fp_line (start 0 -3.23) (end 0 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7692b5fc-2f1f-462d-943a-018224942e05))
    (fp_line (start 2.54 -3.23) (end 2.54 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 33a4eeb1-2bea-40a2-8617-f68174223f91))
    (fp_line (start 5.08 -3.23) (end 5.08 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d062db05-1ea8-4cca-b443-eb2c8c53c150))
    (fp_line (start 7.67 -19.1) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 108d8c92-7968-4222-b6b6-fd7392ecb1dd))
    (fp_line (start 7.67 -12.42) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8075b37c-7514-4671-b658-7074ffaa9a4b))
    (fp_line (start 7.67 -12.42) (end 7.67 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 595f2e12-c82a-41a3-9c72-92a0a95c706f))
    (fp_line (start 7.67 -3.23) (end -2.59 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9ecb8678-b8e1-401c-bc52-4aba94a29f9f))
    (fp_circle (center 2.54 -15.8) (end 4.39 -15.8)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp dc7e6600-ee26-4ffd-94ed-ee540e751f99))
    (pad "" np_thru_hole oval (at 2.54 -15.8 90) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask") (tstamp 0035feff-fe19-4024-a1c9-f4bcf8cc5efe))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(Q2-Pad1)") (pinfunction "G") (pintype "input") (tstamp 87ffbfa4-af36-4ca6-9070-5b84b47b5c1e))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(C1-Pad2)") (pinfunction "D") (pintype "passive") (tstamp ff83b3a6-4d53-4701-934d-6e694b49d232))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(C2-Pad2)") (pinfunction "S") (pintype "passive") (tstamp 1ade1f8c-c9c8-41f2-b6f9-a28248362c99))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220F-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-323" (layer "F.Cu")
    (tstamp c715ba1d-772c-44e7-a835-e3b4cb39f8b2)
    (at 55.88 71.755)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/c62a68f6-5959-4e0d-add0-6725d0e22108")
    (attr smd)
    (fp_text reference "D5" (at 0 -1.85) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c8a719e9-5a60-4256-88e6-46309a6f2004)
    )
    (fp_text value "1N4148WS" (at 0.1 1.9) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 64ce93c4-34de-4f1e-a332-e5b65f4fd8b2)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.85) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 35d85d1f-cbf4-418c-a8e2-c754642f2785)
    )
    (fp_line (start -1.5 -0.85) (end -1.5 0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e5a27129-3301-4b3b-947a-140d7cc2883c))
    (fp_line (start -1.5 -0.85) (end 1.05 -0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9aa3c0ec-0ecc-47a3-aa99-f9c6ad245952))
    (fp_line (start -1.5 0.85) (end 1.05 0.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 42b86919-8d15-43b2-a3dd-3e32b120fb2f))
    (fp_line (start -1.6 -0.95) (end -1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp eab1edb4-4ddb-46ef-8ed8-68e5901615c8))
    (fp_line (start -1.6 -0.95) (end 1.6 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c745ca80-da42-4637-99ab-8d3131878536))
    (fp_line (start -1.6 0.95) (end 1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9f79c12c-00e9-4696-80c0-e28cb8e762de))
    (fp_line (start 1.6 -0.95) (end 1.6 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8fd291a0-2be1-4e31-baa6-903c749c4392))
    (fp_line (start -0.9 -0.7) (end 0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 757f5457-f31b-415d-b4ba-17697ca14e47))
    (fp_line (start -0.9 0.7) (end -0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a6ffe256-617d-421b-95d9-6f55927f5f53))
    (fp_line (start -0.3 -0.35) (end -0.3 0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ab6d212c-f040-4a8b-b094-f506eb75f2c5))
    (fp_line (start -0.3 0) (end -0.5 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1215aad5-d5c1-47f9-b5b5-3cd1a23f9c52))
    (fp_line (start -0.3 0) (end 0.2 -0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 18370893-99fc-4228-8b43-661cb90a284d))
    (fp_line (start 0.2 -0.35) (end 0.2 0.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 91aa9f2a-571b-4469-97d7-5cc7d4c2c37a))
    (fp_line (start 0.2 0) (end 0.45 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e0b7fa48-cad4-4eda-93cb-833d9048da91))
    (fp_line (start 0.2 0.35) (end -0.3 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8c8458a0-b31d-4d73-b8a3-6ac265a061d6))
    (fp_line (start 0.9 -0.7) (end 0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0b99653a-7ba7-48f4-a674-72e453b9b2c2))
    (fp_line (start 0.9 0.7) (end -0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ab3100e9-e4f5-4e70-ac1e-89880e51db6b))
    (pad "1" smd rect (at -1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(C2-Pad1)") (pinfunction "K") (pintype "passive") (tstamp d841aaaf-0234-4917-9004-b82d37082a7a))
    (pad "2" smd rect (at 1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 973cbdeb-0617-42c4-a9e8-cf7ef4a93fab))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_Pad_D4.0mm" (layer "F.Cu")
    (tstamp cb327948-66a2-43d2-a2dc-924c328b39ae)
    (at 51 93.345)
    (descr "SMD pad as test Point, diameter 4.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/050589bb-899f-4384-8e63-0c94b0a943cd")
    (attr exclude_from_pos_files)
    (fp_text reference "J1" (at 0 -2.898) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 18cc8f45-212b-4c3e-bee2-ff7a25299ef7)
    )
    (fp_text value "Vrail" (at 0 3.1) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 126bf3e8-30b1-45df-9f4d-dfb7065339e3)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.9) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5cb10700-2b13-4257-b24b-32f20824b0ff)
    )
    (fp_circle (center 0 0) (end 0 2.25)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 97204bf9-6a23-4a86-a411-c6535f15fc10))
    (fp_circle (center 0 0) (end 2.5 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 93c1080b-111f-4be5-919d-55f36de6004e))
    (pad "1" smd circle (at 0 0) (size 4 4) (layers "F.Cu" "F.Mask")
      (net 22 "Net-(D1-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 10708ad7-7e44-4bcb-aea6-72a668569847))
  )

  (footprint "Package_TO_SOT_THT:TO-220F-3_Horizontal_TabDown" (layer "F.Cu")
    (tstamp ccd95f00-d45e-451b-850d-826c11e4f8a0)
    (at 50.96 24.13 90)
    (descr "TO-220F-3, Horizontal, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf")
    (tags "TO-220F-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/bbc609db-d67c-42dc-a674-eb05a0c1600d")
    (attr through_hole)
    (fp_text reference "Q4" (at 2.54 -20.22 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 770c7500-9177-4f2d-a389-a92aed5fd2bb)
    )
    (fp_text value "IRF540N" (at 2.54 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp af67a863-5c89-4f0c-a82e-7d06f485fe68)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -20.22 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7f60a7f2-41ee-4da7-873c-97d632f6fb4a)
    )
    (fp_line (start -2.71 -19.22) (end -2.71 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8991c437-84fc-4add-8d0f-a6da22ca207e))
    (fp_line (start -2.71 -19.22) (end 7.79 -19.22)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 535a2712-cc05-4f86-8150-1bfd1236e1b6))
    (fp_line (start -2.71 -3.11) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fb17622e-914b-4f61-b924-58d9ad448438))
    (fp_line (start 0 -3.11) (end 0 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e8e2ca9-86d4-43f4-b395-17aeb535b8c0))
    (fp_line (start 2.54 -3.11) (end 2.54 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8aebae27-62b8-485a-aa23-4ebc9b236fdb))
    (fp_line (start 5.08 -3.11) (end 5.08 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d5559f92-7cc6-4a98-b1d3-cb40f312e72c))
    (fp_line (start 7.79 -19.22) (end 7.79 -3.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 63fddaab-1bd0-42a4-a232-64c3094d9932))
    (fp_line (start -2.84 -19.35) (end -2.84 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d7d315e9-2a7a-4b36-a258-51234a24a2bb))
    (fp_line (start -2.84 1.25) (end 7.92 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5458075a-95a7-4a57-8224-5a7973f11b64))
    (fp_line (start 7.92 -19.35) (end -2.84 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 79a7b1f6-018f-449d-bca1-d1d366464bd0))
    (fp_line (start 7.92 1.25) (end 7.92 -19.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3a9beaf0-4ab0-4bf9-a675-840cf20f9818))
    (fp_line (start -2.59 -19.1) (end 7.67 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 587c93cf-85b6-4c31-993c-742964f11fa8))
    (fp_line (start -2.59 -12.42) (end -2.59 -19.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b419b89-d2e9-4de8-8a4c-09071fdbd8b2))
    (fp_line (start -2.59 -12.42) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9bf83732-6f03-4f52-9b21-93c2b6d7e6da))
    (fp_line (start -2.59 -3.23) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5debe630-f246-421a-847c-9bb45f57ab75))
    (fp_line (start 0 -3.23) (end 0 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2d8c1618-b3bc-495a-9c2c-599e1d86e822))
    (fp_line (start 2.54 -3.23) (end 2.54 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9c3f044e-1eef-4249-ba1b-5eeba7652b2d))
    (fp_line (start 5.08 -3.23) (end 5.08 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1459cbb5-8339-4919-95a2-6d39afdaf991))
    (fp_line (start 7.67 -19.1) (end 7.67 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 79af50bf-2ff9-4ffe-9d56-c0d77f9d328e))
    (fp_line (start 7.67 -12.42) (end -2.59 -12.42)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp feae8c89-81f5-4192-8191-c1c326b04b0a))
    (fp_line (start 7.67 -12.42) (end 7.67 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dee454b7-a07f-44e3-a705-8dcb5532c655))
    (fp_line (start 7.67 -3.23) (end -2.59 -3.23)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b4a5157-7334-4048-9eaf-65a60005673c))
    (fp_circle (center 2.54 -15.8) (end 4.39 -15.8)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp e4e216d5-b42a-407f-818b-c04a34161fef))
    (pad "" np_thru_hole oval (at 2.54 -15.8 90) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask") (tstamp 4ae0896b-28eb-4333-8065-9326c5da95bd))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Q4-Pad1)") (pinfunction "G") (pintype "input") (tstamp fb6de705-4a04-4ab5-9e8a-8a8c916e8078))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(C3-Pad2)") (pinfunction "D") (pintype "passive") (tstamp c90c80f3-ff08-4df7-ada5-c700469919bc))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(C4-Pad2)") (pinfunction "S") (pintype "passive") (tstamp 20dc282b-b039-4f84-81b2-d608dcb04e8e))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220F-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tstamp d58e976c-321e-4e92-9bc4-0842de0ff6e0)
    (at 66.04 57.785)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/ffc1b322-1664-46b4-b4fb-ef1c82762c58")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.82) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 24d2246a-e09a-4731-814d-15998fd5916c)
    )
    (fp_text value "220" (at 0 1.82) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dc654af9-6b96-43be-8673-1342086a6eef)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp fab44d62-8170-466e-b5c8-dbec85aa62e1)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7441178d-aa53-4929-b5e9-6a8778e65c6a))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bafa4759-cb06-4ce5-9904-48256de2f6b8))
    (fp_line (start -2.45 -1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f1d039e7-c8f0-43f0-a2b5-440c1e31a848))
    (fp_line (start -2.45 1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 619f0093-2ed0-4e38-b536-dc232a1cf9c1))
    (fp_line (start 2.45 -1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8b8069c2-d145-4d4e-b8d2-4a1848de0814))
    (fp_line (start 2.45 1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b011786d-7a15-4802-a1d9-af7f6b09884e))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 402a5832-b070-4e1e-ba05-9c74fd156d02))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 69b53edb-faf4-4fc8-8c1b-60d75286c1ba))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e277b0b3-80c3-4d2a-9fe6-72be4467e6b7))
    (fp_line (start 1.6 0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2078e0f3-c65a-485d-ad8f-9b88e540b791))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 8 "Net-(R2-Pad1)") (pintype "passive") (tstamp 2bc107c5-264e-44d7-8dee-3531c85aef6a))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 17 "Net-(J6-Pad2)") (pintype "passive") (tstamp db2849b5-1b76-4d87-86dd-eda631eaeb75))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1812_4532Metric_Pad1.30x3.40mm_HandSolder" (layer "F.Cu")
    (tstamp e2ab00f7-5fd4-438b-8ebb-7752695859b5)
    (at 68.3 41.91)
    (descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/48b2513f-f38c-4176-af5d-1506d860931a")
    (attr smd)
    (fp_text reference "R5" (at 0 -2.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9bc77cf8-da98-46b9-8198-6a966e25f5ec)
    )
    (fp_text value "220" (at 0 2.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 508e5145-cb08-478e-9a92-09b8c3780fb4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7ddcb990-9399-4aed-b8c6-89db55814dd5)
    )
    (fp_line (start -1.386252 -1.71) (end 1.386252 -1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3734e5be-0877-46bc-ae5c-34ffcc753419))
    (fp_line (start -1.386252 1.71) (end 1.386252 1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5a8f17bc-ceb3-48d7-9ac9-6ea239bc5d57))
    (fp_line (start -3.12 -1.95) (end 3.12 -1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8149ef57-72c9-4d85-8324-94c964f08abb))
    (fp_line (start -3.12 1.95) (end -3.12 -1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 24f3d9a0-40f7-4c13-a779-27373953a1e2))
    (fp_line (start 3.12 -1.95) (end 3.12 1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 955ff49c-f456-4210-b449-1348b612a9bc))
    (fp_line (start 3.12 1.95) (end -3.12 1.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e1e2dab2-cd0b-44a6-9e45-04cb83e34842))
    (fp_line (start -2.25 -1.6) (end 2.25 -1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 66706b20-8927-47b6-8adb-0b2426d9e5b6))
    (fp_line (start -2.25 1.6) (end -2.25 -1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1c8d18fc-3130-4726-b334-353aeb2026a9))
    (fp_line (start 2.25 -1.6) (end 2.25 1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 62546863-11b1-42e7-9980-4f919d6293b8))
    (fp_line (start 2.25 1.6) (end -2.25 1.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 689f2882-0dd1-4283-9d1c-b40234ad8c59))
    (pad "1" smd roundrect (at -2.225 0) (size 1.3 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 1 "GND") (pintype "passive") (tstamp 5a7ea061-b3d7-4a6d-9e54-38372b63b63f))
    (pad "2" smd roundrect (at 2.225 0) (size 1.3 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 14 "Net-(J6-Pad5)") (pintype "passive") (tstamp 146b6dee-ca55-4360-9560-8a965f3b52d4))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm" (layer "F.Cu")
    (tstamp f3cc5bc7-ff5d-4414-b32f-051cab0d5f8c)
    (at 62.23 67.31 180)
    (descr "8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true")
    (tags "SSO Stretched SO SOIC 1.27")
    (property "Sheetfile" "squeow_mod.kicad_sch")
    (property "Sheetname" "")
    (path "/071894b9-a4fb-4962-a100-9be726162c17")
    (attr smd)
    (fp_text reference "U2" (at 0.1 -3.265) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 67929d4b-a75b-4094-a099-938ffed8162f)
    )
    (fp_text value "UCC23313" (at 0.05 3.385) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c2b0e8ed-c55a-468c-972a-16ad07c162c7)
    )
    (fp_text user "${REFERENCE}" (at 0 -0.065) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 443c2a0d-cbd6-4c30-a509-0bdde6def684)
    )
    (fp_line (start -3.55 -2.465) (end -3.55 -1.815)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7841857a-f066-413a-a976-0e3b0a2cec67))
    (fp_line (start -3.55 -1.8) (end -5.3 -1.8)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp be8a81ad-f538-44bc-9b60-65a8d740db65))
    (fp_line (start -3.5 1.785) (end -3.5 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b6ff1b8d-c21c-48ac-829b-1c71d1a8d5fd))
    (fp_line (start -3.5 2.435) (end 3.55 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e5dfbbf2-77b8-40d8-a56f-fd87f2596803))
    (fp_line (start 3.5 -2.465) (end -3.55 -2.465)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7c3fb679-ebf8-401f-800d-ec572417b185))
    (fp_line (start 3.5 -2.465) (end 3.5 -1.815)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1e44ae91-8fc7-48b8-afa7-8bb1cc9c650e))
    (fp_line (start 3.55 1.785) (end 3.55 2.435)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fea72355-6bbb-4787-b38f-8b0c5aa4c8be))
    (fp_line (start -5.6 -2.56) (end -5.6 2.54)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f9d0df7c-3091-458e-ac23-a22b79118297))
    (fp_line (start -5.6 -2.56) (end 5.6 -2.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 80998775-fd4f-4be9-a383-c9acb5b0f4bb))
    (fp_line (start 5.6 2.54) (end -5.6 2.54)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c9f216a2-b01e-4489-90c2-3546b799a480))
    (fp_line (start 5.6 2.54) (end 5.6 -2.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 38856f37-e523-477c-a78d-d659f95ae978))
    (fp_line (start -3.4 2.285) (end -3.4 -1.265)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 0f6e5ab4-bc55-4932-a288-b9c07e3d63d5))
    (fp_line (start -2.3 -2.315) (end -3.4 -1.215)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp b560417b-bbda-4270-9ef5-a7eb30d028b5))
    (fp_line (start 3.4 -2.315) (end -2.3 -2.315)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 1c035a41-f81c-4608-b72e-50ee0e2c598a))
    (fp_line (start 3.4 -2.315) (end 3.4 2.285)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 23a2d3b9-714f-48b0-a2f9-a491ba527c74))
    (fp_line (start 3.4 2.285) (end -3.4 2.285)
      (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp cca3404a-1e7b-485a-ae20-bcd9f7c1cfe7))
    (pad "1" smd rect (at -4.27 -1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(R2-Pad1)") (pinfunction "A") (pintype "passive") (tstamp 20e7c396-37e3-4319-b2ad-e03d6381750f))
    (pad "2" smd rect (at -4.27 0 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "unconnected-(U2-Pad2)") (pinfunction "NC") (pintype "no_connect") (tstamp 3b068ce1-d5fe-491d-b9aa-5c13423e92fd))
    (pad "3" smd rect (at -4.27 1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive") (tstamp 87a5d290-7ed6-48c4-b823-042d1ab6d1c0))
    (pad "4" smd rect (at 4.27 1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(C2-Pad2)") (pinfunction "VEE") (pintype "power_in") (tstamp 0deb5654-d051-4629-bda4-d01107ff20e7))
    (pad "5" smd rect (at 4.27 0 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(Q2-Pad1)") (pinfunction "VO") (pintype "output") (tstamp 53ad7123-afd8-4df8-a544-0226d13040a4))
    (pad "6" smd rect (at 4.27 -1.27 180) (size 2.16 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(C2-Pad1)") (pinfunction "VCC") (pintype "power_in") (tstamp 4910bbfc-a0a6-48cc-b0ec-f077fe750ead))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 46.9825 16.51) (end 73.0175 95.885)
    (stroke (width 0.1) (type solid)) (fill none) (layer "Edge.Cuts") (tstamp 496ae10a-9dc1-465b-8b7f-1b99fdd6e29e))

  (segment (start 64.135 41.91) (end 63.5 42.545) (width 1) (layer "F.Cu") (net 1) (tstamp 0d20a753-d080-491a-8fd9-42f4de522295))
  (segment (start 59.055 60.96) (end 63.5 65.405) (width 1) (layer "F.Cu") (net 1) (tstamp 176e265a-aaf1-415d-a50e-49d8fbe230e3))
  (segment (start 65.405 87.63) (end 66.5 87.63) (width 1) (layer "F.Cu") (net 1) (tstamp 21e55576-bc16-410d-ac63-3fe0efe63bb9))
  (segment (start 63.5 65.405) (end 63.5 66.675) (width 1) (layer "F.Cu") (net 1) (tstamp 223f330f-4606-4948-87cd-a70108d3bdcf))
  (segment (start 66.5 22.86) (end 64.87 22.86) (width 1) (layer "F.Cu") (net 1) (tstamp 282449a1-d1ca-4201-9602-8a1a3dc23aec))
  (segment (start 63.5 24.23) (end 63.5 42.545) (width 1) (layer "F.Cu") (net 1) (tstamp 2a41c0d6-3163-45b9-a849-a9961bb9d375))
  (segment (start 63.5 85.725) (end 65.405 87.63) (width 1) (layer "F.Cu") (net 1) (tstamp 2db282a7-6088-4229-9fbb-4284285dfc8c))
  (segment (start 59.055 53.34) (end 59.055 60.96) (width 1) (layer "F.Cu") (net 1) (tstamp 3a070fc1-20d3-459a-bf39-dcd486780604))
  (segment (start 63.5 44.45) (end 63.5 48.895) (width 1) (layer "F.Cu") (net 1) (tstamp 427259fc-0d52-4d9c-b352-5eb6c24f7289))
  (segment (start 63.5 48.895) (end 59.055 53.34) (width 1) (layer "F.Cu") (net 1) (tstamp 5d81611d-b3f6-4914-b669-b33e5e3976d7))
  (segment (start 63.5 66.04) (end 63.5 66.675) (width 1) (layer "F.Cu") (net 1) (tstamp 67dbd3d7-ef99-4ef1-990d-8a5a31a4c874))
  (segment (start 66.5 44.45) (end 63.5 44.45) (width 1) (layer "F.Cu") (net 1) (tstamp 785f0e05-b76f-44ca-8bd7-9ece313ce763))
  (segment (start 66.5 66.04) (end 63.5 66.04) (width 1) (layer "F.Cu") (net 1) (tstamp 873fde00-9ea3-4375-9d13-cebe0728e70a))
  (segment (start 64.87 22.86) (end 63.5 24.23) (width 1) (layer "F.Cu") (net 1) (tstamp 9721e885-a271-407d-b25b-d6860120056c))
  (segment (start 63.5 66.675) (end 63.5 85.725) (width 1) (layer "F.Cu") (net 1) (tstamp 97530bce-e1d7-4472-915f-ceed8459d5e8))
  (segment (start 66.075 41.91) (end 64.135 41.91) (width 1) (layer "F.Cu") (net 1) (tstamp b33992e7-fcc3-462c-958b-76361d1ba3ac))
  (segment (start 63.5 42.545) (end 63.5 44.45) (width 1) (layer "F.Cu") (net 1) (tstamp c4d8f845-8caf-4a52-8c93-4ffbc1fc425e))
  (segment (start 68.33 27.23) (end 66.5 25.4) (width 1) (layer "F.Cu") (net 6) (tstamp 1aa5eb28-2abd-4b3a-9f1b-90d186f05ab1))
  (segment (start 64.49 51.9) (end 68.33 48.06) (width 1) (layer "F.Cu") (net 6) (tstamp 31d1aebd-7cb3-486b-817e-6d5a56584266))
  (segment (start 64.49 52.705) (end 64.49 51.9) (width 1) (layer "F.Cu") (net 6) (tstamp 4cc3f6be-dd31-4d20-aa71-ff59cf27b256))
  (segment (start 68.33 48.06) (end 68.33 27.23) (width 1) (layer "F.Cu") (net 6) (tstamp f999e6db-83df-4552-acf2-d7be10b9b851))
  (segment (start 63 53.755) (end 64.49 55.245) (width 1) (layer "F.Cu") (net 7) (tstamp 70e50dbe-a61f-4f5b-b23f-37e92ad768f6))
  (segment (start 66.5 47.662766) (end 63 51.162766) (width 1) (layer "F.Cu") (net 7) (tstamp 8bff1444-4260-4f29-8a46-d8532a4891be))
  (segment (start 66.5 46.99) (end 66.5 47.662766) (width 1) (layer "F.Cu") (net 7) (tstamp 9423a92e-6ab7-43bb-9be8-2fdc586c7bbc))
  (segment (start 63 51.162766) (end 63 53.755) (width 1) (layer "F.Cu") (net 7) (tstamp 96c0ae32-6355-4d8c-acea-494edc9ec03c))
  (segment (start 68.13 68.58) (end 68.33 68.38) (width 1) (layer "F.Cu") (net 8) (tstamp 07267a88-0482-443d-b221-8ce33c72d7c6))
  (segment (start 66.500786 64) (end 65 64) (width 1) (layer "F.Cu") (net 8) (tstamp 4f868b49-e1dd-45cb-9243-717a2d07f5cf))
  (segment (start 63.215 57.785) (end 64.49 57.785) (width 1) (layer "F.Cu") (net 8) (tstamp 65cc0cf0-30e0-4b43-8654-73170824eca7))
  (segment (start 66.615786 64.115) (end 66.500786 64) (width 1) (layer "F.Cu") (net 8) (tstamp 83698258-5799-4a2a-b3a2-cf4b12ce3202))
  (segment (start 62 61) (end 62 59) (width 1) (layer "F.Cu") (net 8) (tstamp a542d1fc-64da-40fa-bdf7-8869c3e4f0ec))
  (segment (start 62 59) (end 63.215 57.785) (width 1) (layer "F.Cu") (net 8) (tstamp b0cfbef9-6232-4c27-acee-1ab6216943ec))
  (segment (start 65 64) (end 62 61) (width 1) (layer "F.Cu") (net 8) (tstamp cee7a0f4-1d51-4bfd-a786-cc292bcb8c8b))
  (segment (start 68.33 68.38) (end 68.33 65.155) (width 1) (layer "F.Cu") (net 8) (tstamp ee3403c5-9cc3-46f1-913d-d4f5a9d94a48))
  (segment (start 68.33 65.155) (end 67.29 64.115) (width 1) (layer "F.Cu") (net 8) (tstamp f2e67e03-faac-4bb6-8190-26c18407feb3))
  (segment (start 67.29 64.115) (end 66.615786 64.115) (width 1) (layer "F.Cu") (net 8) (tstamp fa062aad-817f-47ae-8830-69ea741421c5))
  (segment (start 66.5 68.58) (end 68.13 68.58) (width 1) (layer "F.Cu") (net 8) (tstamp fbe6a847-de7c-4703-a518-7b7e2df0be14))
  (segment (start 70.485 64.77) (end 68.58 62.865) (width 1) (layer "F.Cu") (net 9) (tstamp 58eff93c-d746-4c74-a427-3c88dc0da2dc))
  (segment (start 67.03 62.865) (end 64.49 60.325) (width 1) (layer "F.Cu") (net 9) (tstamp 6be44820-0f5e-4c02-8f70-7e5659c09fb4))
  (segment (start 68.58 62.865) (end 67.03 62.865) (width 1) (layer "F.Cu") (net 9) (tstamp 88c0938d-38dc-4a42-9d08-a8dd2b4c5699))
  (segment (start 68.13 90.17) (end 70.485 87.815) (width 1) (layer "F.Cu") (net 9) (tstamp a8dfaa9b-2559-4233-9dc0-077bdf840484))
  (segment (start 66.5 90.17) (end 68.13 90.17) (width 1) (layer "F.Cu") (net 9) (tstamp cf90e813-aef3-420e-94b9-39ce2da51e31))
  (segment (start 70.485 87.815) (end 70.485 64.77) (width 1) (layer "F.Cu") (net 9) (tstamp d95e18bf-74dd-4899-9864-bba6ded24db8))
  (segment (start 50.96 24.13) (end 57.96 24.13) (width 1) (layer "F.Cu") (net 10) (tstamp ff71fe09-a6b2-4fb6-912a-9962626a4ac6))
  (segment (start 57.96 45.72) (end 50.96 45.72) (width 1) (layer "F.Cu") (net 11) (tstamp 25f100ce-aa3d-4f8b-98c1-fdbc4accce2f))
  (segment (start 57.96 67.31) (end 50.96 67.31) (width 1) (layer "F.Cu") (net 12) (tstamp a1378cf0-e157-4ca0-8e1b-2300736a91b4))
  (segment (start 57.96 88.9) (end 50.96 88.9) (width 1) (layer "F.Cu") (net 13) (tstamp 8b726460-8885-405d-900d-f73b6c8b7e11))
  (segment (start 71.12 42.505) (end 70.525 41.91) (width 1) (layer "F.Cu") (net 14) (tstamp 159beb4b-6415-49fd-bf9b-9b3a94bbca0b))
  (segment (start 71.12 50.165) (end 71.12 42.505) (width 1) (layer "F.Cu") (net 14) (tstamp bb3cc94d-2d3f-4bdd-8ce2-d2849a3dba0b))
  (segment (start 67.04 52.705) (end 71.12 52.705) (width 1) (layer "F.Cu") (net 15) (tstamp 86172240-2bcd-4812-b0fd-1e3eaec60f96))
  (segment (start 71.12 55.245) (end 67.04 55.245) (width 1) (layer "F.Cu") (net 16) (tstamp 8a9859fa-c46a-4d9e-86c7-7d60b318dfde))
  (segment (start 71.12 57.785) (end 67.04 57.785) (width 1) (layer "F.Cu") (net 17) (tstamp 5d246eda-fc01-409f-a3ca-5203e0037609))
  (segment (start 71.12 60.325) (end 67.04 60.325) (width 1) (layer "F.Cu") (net 18) (tstamp 6a2118d8-35fe-4b94-9eb1-363ab5985787))
  (segment (start 53.975 32.385) (end 56.93 29.43) (width 1) (layer "F.Cu") (net 19) (tstamp 3b479abd-eb96-46ba-aa9a-89ebdfb90f98))
  (segment (start 56.93 29.43) (end 56.93 28.575) (width 1) (layer "F.Cu") (net 19) (tstamp 77626806-dc86-4a3a-a0af-73c4f1c3d389))
  (segment (start 53.975 32.385) (end 50.96 32.385) (width 2) (layer "F.Cu") (net 19) (tstamp c8e2d326-ba33-4d33-915e-9c40f99270ff))
  (segment (start 60.96 48.26) (end 58.1025 51.1175) (width 2) (layer "F.Cu") (net 20) (tstamp 049f3db9-d3f9-4f9d-8808-002a4917135e))
  (segment (start 52.07 34.925) (end 60.96 43.815) (width 2) (layer "F.Cu") (net 20) (tstamp 247a0435-591e-4515-8872-1849cac4d6bb))
  (segment (start 57.15 50.165) (end 58.1025 51.1175) (width 1) (layer "F.Cu") (net 20) (tstamp 2f3c8252-627f-487b-9a6c-4a531790084b))
  (segment (start 60.96 43.815) (end 60.96 48.26) (width 2) (layer "F.Cu") (net 20) (tstamp 764bab83-5995-4244-8ef3-da23f361392c))
  (segment (start 50.96 53.975) (end 55 53.975) (width 2) (layer "F.Cu") (net 20) (tstamp 896dad3b-af23-4a8b-889a-bedb0a5f8caa))
  (segment (start 50.96 34.925) (end 52.07 34.925) (width 2) (layer "F.Cu") (net 20) (tstamp aabf2c57-796a-456d-abcc-fa7056e39c5c))
  (segment (start 56.93 50.165) (end 57.15 50.165) (width 1) (layer "F.Cu") (net 20) (tstamp beb1b6d2-18ed-411f-8b5f-caf7ca127835))
  (segment (start 58.1025 51.1175) (end 55.245 53.975) (width 2) (layer "F.Cu") (net 20) (tstamp c30b65e3-0b6e-469c-9f11-531fab756f32))
  (segment (start 60.54 70.905) (end 59.3725 72.0725) (width 2) (layer "F.Cu") (net 21) (tstamp 066852fa-d36b-43bb-85f2-a6b4243f72ad))
  (segment (start 55.88 75.565) (end 53.975 75.565) (width 2) (layer "F.Cu") (net 21) (tstamp 249aa638-316d-46e0-a046-9962c8a0a7be))
  (segment (start 53.975 75.565) (end 50.96 75.565) (width 2) (layer "F.Cu") (net 21) (tstamp 6550f4da-61b0-4125-bc4a-5d9e6e1ee694))
  (segment (start 59.3725 72.0725) (end 55.88 75.565) (width 2) (layer "F.Cu") (net 21) (tstamp 7a0adfcb-e65f-45cd-b15f-1cd0ddbad5ca))
  (segment (start 52.07 56.515) (end 60.54 64.985) (width 2) (layer "F.Cu") (net 21) (tstamp 7fe58093-583d-41ef-9dc7-a5957b4719e6))
  (segment (start 56.93 71.755) (end 59.055 71.755) (width 1) (layer "F.Cu") (net 21) (tstamp 8618f475-191d-403f-a4fd-1320937d2b4b))
  (segment (start 59.055 71.755) (end 59.3725 72.0725) (width 1) (layer "F.Cu") (net 21) (tstamp ada321cb-1977-4a6e-9b00-4dee1ad55ca4))
  (segment (start 60.54 64.985) (end 60.54 70.905) (width 2) (layer "F.Cu") (net 21) (tstamp bdb89c98-635d-42c5-afac-fc6c3bf04e58))
  (segment (start 50.96 56.515) (end 52.07 56.515) (width 2) (layer "F.Cu") (net 21) (tstamp bf90ca37-2481-4af3-b6c2-dc7c47681280))
  (segment (start 50.96 78.105) (end 52.07 78.105) (width 2) (layer "F.Cu") (net 22) (tstamp 176faa20-226e-4809-bfb1-d56d6b11b41d))
  (segment (start 48.46 86.4475) (end 50.96 86.4475) (width 2) (layer "F.Cu") (net 22) (tstamp 3b3aef3e-d2c7-401a-aa6b-94164a612c90))
  (segment (start 59.69 93.345) (end 59.69 92.93) (width 1) (layer "F.Cu") (net 22) (tstamp 3cf020a4-8ba0-4c89-bc94-3bc6f70126f8))
  (segment (start 52.07 78.105) (end 60.54 86.575) (width 2) (layer "F.Cu") (net 22) (tstamp 472131de-a4c1-442e-9005-76726a09c32e))
  (segment (start 48.46 91.005) (end 48.46 86.4475) (width 2) (layer "F.Cu") (net 22) (tstamp 5efe1963-65ed-42f7-bb05-9861767e9ae5))
  (segment (start 60.54 92.495) (end 59.69 93.345) (width 2) (layer "F.Cu") (net 22) (tstamp 73a577d1-5784-4bdd-bf31-086f7ca7b4b7))
  (segment (start 58.5625 94.4725) (end 59.69 93.345) (width 2) (layer "F.Cu") (net 22) (tstamp 9744cd76-653a-405f-b4a6-9ba12f1c940c))
  (segment (start 51.9275 94.4725) (end 58.5625 94.4725) (width 2) (layer "F.Cu") (net 22) (tstamp a1a2b873-4ece-4f5f-bfe9-b67b85f75558))
  (segment (start 59.69 92.93) (end 59.47 92.71) (width 1) (layer "F.Cu") (net 22) (tstamp c6b98802-b8ef-470f-b8d6-8c2bfdd1d2fc))
  (segment (start 50.8 93.345) (end 51.9275 94.4725) (width 2) (layer "F.Cu") (net 22) (tstamp ccbef230-1dc7-477f-a3a1-35fe6c15af5a))
  (segment (start 60.54 86.575) (end 60.54 92.495) (width 2) (layer "F.Cu") (net 22) (tstamp f6725e05-bf1c-42ff-baef-dc746da76ad7))
  (segment (start 50.8 93.345) (end 48.46 91.005) (width 2) (layer "F.Cu") (net 22) (tstamp f9a0a125-dc7a-4051-a4e3-01cd11b548e9))
  (segment (start 54.61 21.9925) (end 54.61 19.44) (width 2) (layer "F.Cu") (net 23) (tstamp 4e34a65c-24f2-44a9-9552-5baa94a4bccc))
  (segment (start 54.61 21.9925) (end 55.4275 22.81) (width 1) (layer "F.Cu") (net 23) (tstamp 6269ec4c-c4bd-4d99-9ee1-6203d530342a))
  (segment (start 55.4275 22.81) (end 57.96 22.81) (width 1) (layer "F.Cu") (net 23) (tstamp a0424235-ff99-4902-8269-cfc67fb7b041))
  (segment (start 50.96 19.05) (end 55 19.05) (width 2) (layer "F.Cu") (net 23) (tstamp d25d37e2-afd4-4cf9-a7eb-8f632a713737))
  (segment (start 54.83 28.575) (end 54.83 26.4875) (width 1) (layer "F.Cu") (net 24) (tstamp 00424083-3a06-4fab-9227-0f6abbadc52b))
  (segment (start 54.61 26.2675) (end 55.4275 25.45) (width 1) (layer "F.Cu") (net 24) (tstamp e7d3ba02-c542-4a6e-819c-bac9b5d0f909))
  (segment (start 55.4275 25.45) (end 57.96 25.45) (width 1) (layer "F.Cu") (net 24) (tstamp f7c587d2-2fe0-4b26-90b1-2c74cd4612ba))
  (segment (start 48.895 21.59) (end 48.46 22.025) (width 2) (layer "F.Cu") (net 25) (tstamp 19306891-16af-4694-a828-7a789e8136e0))
  (segment (start 52.705 40.64) (end 54.61 42.545) (width 2) (layer "F.Cu") (net 25) (tstamp 1daf9f6b-b098-447c-88a4-e631efc860de))
  (segment (start 48.46 38.14) (end 50.96 40.64) (width 2) (layer "F.Cu") (net 25) (tstamp 28042122-8000-4ec2-ae63-450571a4b334))
  (segment (start 48.46 22.025) (end 48.46 30.28) (width 2) (layer "F.Cu") (net 25) (tstamp 355c503f-de6e-4a00-98ee-2bbd9c0a6ca5))
  (segment (start 54.61 42.545) (end 54.61 43.5825) (width 2) (layer "F.Cu") (net 25) (tstamp 3cab63ad-0b16-4209-bf66-3a55411dceca))
  (segment (start 54.61 43.5825) (end 55.4275 44.4) (width 1) (layer "F.Cu") (net 25) (tstamp 5020c4e3-eb92-4ff0-8d74-6a01d58b51cf))
  (segment (start 50.96 21.59) (end 48.895 21.59) (width 2) (layer "F.Cu") (net 25) (tstamp 5482ab7a-af5c-4ecf-b516-9bdce87f7d4c))
  (segment (start 55.4275 44.4) (end 57.96 44.4) (width 1) (layer "F.Cu") (net 25) (tstamp 7f89b7b3-24da-4986-85f1-97f0db66de9e))
  (segment (start 48.46 30.28) (end 48.46 38.14) (width 2) (layer "F.Cu") (net 25) (tstamp b1e443f4-5038-442a-ac34-45564cf16c6f))
  (segment (start 48.895 29.845) (end 48.46 30.28) (width 2) (layer "F.Cu") (net 25) (tstamp bfafb6d1-a623-4077-bd56-caf9a3536be9))
  (segment (start 50.96 29.845) (end 48.895 29.845) (width 2) (layer "F.Cu") (net 25) (tstamp e7703231-0a8e-4041-b591-d9ef39e9db9e))
  (segment (start 50.96 40.64) (end 52.705 40.64) (width 2) (layer "F.Cu") (net 25) (tstamp f71ca8fc-391b-4365-93f9-f6b7c5fb254f))
  (segment (start 54.61 47.8575) (end 55.4275 47.04) (width 1) (layer "F.Cu") (net 26) (tstamp 1c5019b1-46d4-4984-8a01-362d6a1cce82))
  (segment (start 55.4275 47.04) (end 57.96 47.04) (width 1) (layer "F.Cu") (net 26) (tstamp ad842466-9e46-4d2c-b2be-b97cbf14f3d6))
  (segment (start 54.83 50.165) (end 54.83 48.0775) (width 1) (layer "F.Cu") (net 26) (tstamp c8b38c04-ce26-4fd9-a95f-66a124ffb0f0))
  (segment (start 48.5475 43.18) (end 48.46 43.2675) (width 2) (layer "F.Cu") (net 27) (tstamp 0c39745f-cdb4-42f8-b2a0-8828be85cd21))
  (segment (start 50.96 62.23) (end 52.07 62.23) (width 2) (layer "F.Cu") (net 27) (tstamp 1b035314-2b9e-48f4-a7c9-c2deb7c9fe8a))
  (segment (start 50.96 43.18) (end 48.5475 43.18) (width 2) (layer "F.Cu") (net 27) (tstamp 404d0661-4068-479f-85a0-e5549993ad27))
  (segment (start 48.46 51.635) (end 48.46 59.73) (width 2) (layer "F.Cu") (net 27) (tstamp 4f685399-e74e-44a7-9eb8-d1805a649f0f))
  (segment (start 54.61 65.1725) (end 55.4275 65.99) (width 1) (layer "F.Cu") (net 27) (tstamp 5b597d12-ecc7-43ae-8199-fb2e04b96d6c))
  (segment (start 48.66 51.435) (end 48.46 51.635) (width 2) (layer "F.Cu") (net 27) (tstamp 5cadce4d-4a1e-4af7-baaf-5fbf78949932))
  (segment (start 54.61 64.77) (end 54.61 65.1725) (width 2) (layer "F.Cu") (net 27) (tstamp 8b1b0c40-69f0-46dc-8f62-91b54bcf03a1))
  (segment (start 55.4275 65.99) (end 57.96 65.99) (width 1) (layer "F.Cu") (net 27) (tstamp 951fb68f-e2bc-4382-8f95-1e5694566506))
  (segment (start 50.96 51.435) (end 48.66 51.435) (width 2) (layer "F.Cu") (net 27) (tstamp ba88c8e3-eae8-4bca-8bfa-47efcd9f1c3b))
  (segment (start 48.46 43.2675) (end 48.46 51.635) (width 2) (layer "F.Cu") (net 27) (tstamp d8bcf9cf-28c1-4fd8-9e5c-94ad91992ad7))
  (segment (start 48.46 59.73) (end 50.96 62.23) (width 2) (layer "F.Cu") (net 27) (tstamp dc977a5f-ff3a-4c79-8b77-bc66c38ff992))
  (segment (start 52.07 62.23) (end 54.61 64.77) (width 2) (layer "F.Cu") (net 27) (tstamp eaedefd9-a44c-48b8-8e51-4e41ee85108a))
  (segment (start 55.4275 68.63) (end 57.96 68.63) (width 1) (layer "F.Cu") (net 28) (tstamp 52408008-8c99-4d3a-9cc0-4f301362c612))
  (segment (start 54.83 71.755) (end 54.83 69.6675) (width 1) (layer "F.Cu") (net 28) (tstamp 638c05ac-8e53-4357-94c2-3a31cf9e8340))
  (segment (start 54.61 69.4475) (end 55.4275 68.63) (width 1) (layer "F.Cu") (net 28) (tstamp cb61fd3f-f65e-4d94-b40c-8cf45ce3cb72))
  (segment (start 48.895 73.025) (end 48.46 72.59) (width 2) (layer "F.Cu") (net 29) (tstamp 155c5b6d-851e-45e2-8bc4-624b20dbef77))
  (segment (start 49.809141 83.82) (end 50.96 83.82) (width 2) (layer "F.Cu") (net 29) (tstamp 412c3144-c50d-4330-91c6-05ed9a29f58a))
  (segment (start 54.61 86.7625) (end 55.4275 87.58) (width 1) (layer "F.Cu") (net 29) (tstamp 5fde0381-b7e6-4fcf-ac8d-a6e80ec20f14))
  (segment (start 52.07 83.82) (end 54.61 86.36) (width 2) (layer "F.Cu") (net 29) (tstamp 66cafd64-3853-4dfb-bf4b-0a40d2e59d33))
  (segment (start 48.46 72.59) (end 48.46 82.470859) (width 2) (layer "F.Cu") (net 29) (tstamp 6f8af218-1481-4864-93ed-a738bd48bf5b))
  (segment (start 50.96 83.82) (end 52.07 83.82) (width 2) (layer "F.Cu") (net 29) (tstamp 793a4950-89f2-4aaa-bb4d-069c8c2c5011))
  (segment (start 48.46 64.8575) (end 48.46 72.59) (width 2) (layer "F.Cu") (net 29) (tstamp 80987aca-2b41-4647-b329-ba7a5ca2cdab))
  (segment (start 55.4275 87.58) (end 57.96 87.58) (width 1) (layer "F.Cu") (net 29) (tstamp 8e0ac09b-ee86-4d70-87d2-5efb9ac08844))
  (segment (start 54.61 86.36) (end 54.61 86.7625) (width 2) (layer "F.Cu") (net 29) (tstamp 8f15f807-477e-4829-826e-850b1c7598bf))
  (segment (start 48.46 82.470859) (end 49.809141 83.82) (width 2) (layer "F.Cu") (net 29) (tstamp a78aebb5-23d6-4d94-9a2f-37f032bbafcc))
  (segment (start 48.5475 64.77) (end 48.46 64.8575) (width 2) (layer "F.Cu") (net 29) (tstamp dddc0e0f-c4d1-4231-aff0-92639633c58b))
  (segment (start 50.96 64.77) (end 48.5475 64.77) (width 2) (layer "F.Cu") (net 29) (tstamp e9a65852-edb9-4333-b6aa-01a494c660a2))
  (segment (start 50.96 73.025) (end 48.895 73.025) (width 2) (layer "F.Cu") (net 29) (tstamp f7a9ee9d-8e70-41a3-9db5-92382637ba31))
  (segment (start 57.3575 92.7225) (end 57.37 92.71) (width 1) (layer "F.Cu") (net 30) (tstamp 27534811-f109-4315-8e5c-3b3dc7002c04))
  (segment (start 55.4275 90.22) (end 57.96 90.22) (width 1) (layer "F.Cu") (net 30) (tstamp 49245ea2-dee1-4ab8-a8ae-15424dd3f1e1))
  (segment (start 54.61 91.0375) (end 55.4275 90.22) (width 1) (layer "F.Cu") (net 30) (tstamp 58f4ff1a-69cc-409b-97ce-470d60554d96))
  (segment (start 56.295 92.7225) (end 57.3575 92.7225) (width 1) (layer "F.Cu") (net 30) (tstamp 5f3be7c3-701f-4965-8e7c-af8244a59f7c))
  (segment (start 56.295 92.7225) (end 54.61 91.0375) (width 1) (layer "F.Cu") (net 30) (tstamp fa8c1536-6c27-4f8c-8745-bb65b787d840))

)
