(kicad_pcb (version 20171130) (host pcbnew 5.99.0+really5.1.12+dfsg1-1)

  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 167)
    (zones 0)
    (modules 20)
    (nets 15)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(SW1-Pad2)")
  (net 4 "Net-(U2-Pad10)")
  (net 5 "Net-(U2-Pad9)")
  (net 6 "Net-(U2-Pad3)")
  (net 7 "Net-(U2-Pad2)")
  (net 8 +12V)
  (net 9 "Net-(J1-Pad1)")
  (net 10 "Net-(J2-Pad1)")
  (net 11 "Net-(R1-Pad2)")
  (net 12 "Net-(R2-Pad2)")
  (net 13 "Net-(SW2-Pad2)")
  (net 14 "Net-(C1-Pad1)")

  (net_class Default "Questo è il gruppo di collegamenti predefinito"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U4-Pad3)")
  )

  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5A02FF57) (tstamp 61D3A92F)
    (at 70.575 32.525 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (path /61DBDBE5)
    (attr smd)
    (fp_text reference U5 (at 0 -4.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LD1117S33TR_SOT223 (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (fp_line (start 1.91 3.41) (end 1.91 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.91 -3.41) (end 1.91 -2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.4 -3.6) (end -4.4 -3.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.4 3.6) (end 4.4 -3.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.4 3.6) (end 4.4 3.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.4 -3.6) (end -4.4 3.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -2.35) (end -0.85 -3.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1.85 -2.35) (end -1.85 3.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1.85 3.41) (end 1.91 3.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.85 -3.35) (end 1.85 -3.35) (layer F.Fab) (width 0.1))
    (fp_line (start -4.1 -3.41) (end 1.91 -3.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 3.35) (end 1.85 3.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.85 -3.35) (end 1.85 3.35) (layer F.Fab) (width 0.1))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Button_Switch_SMD:SW_SPST_CK_RS282G05A3 (layer F.Cu) (tedit 5A7A67D2) (tstamp 61D3393E)
    (at 75.475 51.825 180)
    (descr https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf)
    (tags "SPST button tactile switch")
    (path /61D66A37)
    (attr smd)
    (fp_text reference SW2 (at 0 -2.6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.9 2.05) (end -4.9 -2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 2.05) (end -4.9 2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 -2.05) (end 4.9 2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.9 -2.05) (end 4.9 -2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1) (end 1.75 -1) (layer F.Fab) (width 0.1))
    (fp_line (start 1.75 -1) (end 1.75 1) (layer F.Fab) (width 0.1))
    (fp_line (start 1.75 1) (end -1.75 1) (layer F.Fab) (width 0.1))
    (fp_line (start -1.75 1) (end -1.75 -1) (layer F.Fab) (width 0.1))
    (fp_line (start -3.06 -1.85) (end 3.06 -1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 -1.85) (end 3.06 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 1.85) (end -3.06 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.06 1.85) (end -3.06 -1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.5 0.8) (end 1.5 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 -0.8) (end 1.5 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -0.8) (end 1.5 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 -0.8) (end -1.5 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3 1.8) (end 3 1.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -1.8) (end 3 -1.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -1.8) (end -3 1.8) (layer F.Fab) (width 0.1))
    (fp_line (start 3 -1.8) (end 3 1.8) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 3.9 0 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(SW2-Pad2)"))
    (pad 1 smd rect (at -3.9 0 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Button_Switch_SMD:SW_SPST_CK_RS282G05A3 (layer F.Cu) (tedit 5A7A67D2) (tstamp 61BD3C07)
    (at 64.8 41.25 90)
    (descr https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf)
    (tags "SPST button tactile switch")
    (path /61C14AD4)
    (attr smd)
    (fp_text reference SW1 (at 0 -2.6 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2.6 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.9 2.05) (end -4.9 -2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 2.05) (end -4.9 2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 -2.05) (end 4.9 2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.9 -2.05) (end 4.9 -2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1) (end 1.75 -1) (layer F.Fab) (width 0.1))
    (fp_line (start 1.75 -1) (end 1.75 1) (layer F.Fab) (width 0.1))
    (fp_line (start 1.75 1) (end -1.75 1) (layer F.Fab) (width 0.1))
    (fp_line (start -1.75 1) (end -1.75 -1) (layer F.Fab) (width 0.1))
    (fp_line (start -3.06 -1.85) (end 3.06 -1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 -1.85) (end 3.06 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 1.85) (end -3.06 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.06 1.85) (end -3.06 -1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.5 0.8) (end 1.5 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 -0.8) (end 1.5 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -0.8) (end 1.5 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 -0.8) (end -1.5 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3 1.8) (end 3 1.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -1.8) (end 3 -1.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -1.8) (end -3 1.8) (layer F.Fab) (width 0.1))
    (fp_line (start 3 -1.8) (end 3 1.8) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 3.9 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(SW1-Pad2)"))
    (pad 1 smd rect (at -3.9 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_SMD:D_3220_8050Metric_Pad2.65x5.15mm_HandSolder (layer F.Cu) (tedit 5F68FEF0) (tstamp 61D3822D)
    (at 86.575 32.625)
    (descr "Diode SMD 3220 (8050 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (path /61D9D085)
    (attr smd)
    (fp_text reference D1 (at 0 -3.52) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 0 3.52) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4 -2.5) (end -3 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.5) (end -4 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -4 -1.5) (end -4 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -4 2.5) (end 4 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 4 2.5) (end 4 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 4 -2.835) (end -4.86 -2.835) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.86 -2.835) (end -4.86 2.835) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.86 2.835) (end 4 2.835) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.85 2.82) (end -4.85 -2.82) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.85 -2.82) (end 4.85 -2.82) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.85 -2.82) (end 4.85 2.82) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.85 2.82) (end -4.85 2.82) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 3.275 0) (size 2.65 5.15) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09433999999999999)
      (net 8 +12V))
    (pad 1 smd roundrect (at -3.275 0) (size 2.65 5.15) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09433999999999999)
      (net 14 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_3220_8050Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F) (tstamp 61D34121)
    (at 94.325 44.65)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (path /61D73449)
    (attr virtual)
    (fp_text reference J5 (at 0 -2.898) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MOSFETGND (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 1 GND))
  )

  (module Crystal:Crystal_SMD_SeikoEpson_TSX3225-4Pin_3.2x2.5mm_HandSoldering (layer F.Cu) (tedit 5A0FD1B2) (tstamp 61D3179C)
    (at 77.75 40.2875)
    (descr "crystal Epson Toyocom TSX-3225 series https://support.epson.biz/td/api/doc_check.php?dl=brief_fa-238v_en.pdf, hand-soldering, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (path /61D4D30B)
    (attr smd)
    (fp_text reference Y1 (at 0 -2.95) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Crystal_GND24 (at 0 2.95) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.7 0.7) (thickness 0.105)))
    )
    (fp_line (start -1.5 -1.25) (end 1.5 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -1.25) (end 1.6 -1.15) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -1.15) (end 1.6 1.15) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 1.15) (end 1.5 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 1.25) (end -1.5 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 1.25) (end -1.6 1.15) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 1.15) (end -1.6 -1.15) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -1.15) (end -1.5 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.25) (end -0.6 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -2.7 -2.15) (end -2.7 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 2.15) (end 2.7 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.8 -2.2) (end -2.8 2.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 2.2) (end 2.8 2.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.8 2.2) (end 2.8 -2.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.8 -2.2) (end -2.8 -2.2) (layer F.CrtYd) (width 0.05))
    (pad 4 smd rect (at -1.45 -1.0875) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.45 -1.0875) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U2-Pad3)"))
    (pad 2 smd rect (at 1.45 1.0875) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.45 1.0875) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U2-Pad2)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_SeikoEpson_TSX3225-4Pin_3.2x2.5mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F) (tstamp 61D30632)
    (at 94.275 32.975)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (path /61D4A334)
    (attr virtual)
    (fp_text reference J4 (at 0 -2.898) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 8 +12V))
  )

  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1) (tstamp 61D39FB7)
    (at 85.3 39.69)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (path /6170CD01)
    (attr smd)
    (fp_text reference U3 (at 0 -3.4) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IXDN609PI (at 0 3.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 2.56) (end 1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 2.56) (end -1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end 1.95 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end -3.45 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 2.7) (end 3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.98 0.98) (thickness 0.15)))
    )
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C1-Pad1)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(J1-Pad1)"))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(J1-Pad1)"))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(U2-Pad10)"))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 61BD5655)
    (at 90.25 39.4625 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /617245F7)
    (attr smd)
    (fp_text reference C1 (at 0 -1.85 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220n (at 0 1.85 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 14 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1) (tstamp 61BD2D92)
    (at 85.05 50.255)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (path /6170DA36)
    (attr smd)
    (fp_text reference U4 (at 0 -3.4) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IXDN609PI (at 0 3.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 2.56) (end 1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 2.56) (end -1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end 1.95 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end -3.45 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 2.7) (end 3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.98 0.98) (thickness 0.15)))
    )
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C1-Pad1)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(J2-Pad1)"))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(U2-Pad9)"))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F) (tstamp 61D33C2A)
    (at 78.075 34.275)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (path /61D33D93)
    (attr virtual)
    (fp_text reference J3 (at 0 -2.898) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 1 GND))
  )

  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F) (tstamp 61D2EC39)
    (at 94.3 50.475)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (path /61C2A1B5)
    (attr virtual)
    (fp_text reference J2 (at 0 -2.898) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 10 "Net-(J2-Pad1)"))
  )

  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F) (tstamp 61D2ECD8)
    (at 94.325 39.475)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (path /61C293CA)
    (attr virtual)
    (fp_text reference J1 (at 0 -2.898) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 9 "Net-(J1-Pad1)"))
  )

  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 61D2D22D)
    (at 67.075 52.6)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /61BEE388)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 5k6 (at 0 1.82) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.45 1.12) (end -2.45 1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.45 -1.12) (end 2.45 1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.45 -1.12) (end 2.45 -1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.45 1.12) (end -2.45 -1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 12 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 61D2D21C)
    (at 67.125 50.05)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /61BED99B)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 5k6 (at 0 1.82) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.45 1.12) (end -2.45 1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.45 -1.12) (end 2.45 1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.45 -1.12) (end 2.45 -1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.45 1.12) (end -2.45 -1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 11 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 61D2D999)
    (at 73.75 40.5375 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /61C2AF29)
    (attr smd)
    (fp_text reference C4 (at 0 -1.85 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150n (at 0 1.85 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 61BD5677)
    (at 69.9625 39.525 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /61C2BA36)
    (attr smd)
    (fp_text reference C3 (at 0 -1.85) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150n (at 0 1.85) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 61BD5666)
    (at 90.225 50.0625 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /617264A4)
    (attr smd)
    (fp_text reference C2 (at 0 -1.85 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220n (at 0 1.85 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 14 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:MSOP-10_3x3mm_P0.5mm (layer F.Cu) (tedit 5A02F25C) (tstamp 61D2F9FE)
    (at 78.075 44.725)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (path /61BD2F46)
    (attr smd)
    (fp_text reference U2 (at 0 -2.6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Si5351A-B-GT (at 0 2.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.5 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.15))
    (fp_line (start -1.5 1.5) (end -1.5 -0.5) (layer F.Fab) (width 0.15))
    (fp_line (start -1.5 -0.5) (end -0.5 -1.5) (layer F.Fab) (width 0.15))
    (fp_line (start -3.15 -1.85) (end -3.15 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.15 -1.85) (end 3.15 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.15 -1.85) (end 3.15 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.15 1.85) (end 3.15 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.675 -1.675) (end -1.675 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.675 -1.675) (end 1.675 -1.375) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.675 1.675) (end 1.675 1.375) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.675 1.675) (end -1.675 1.375) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.675 -1.675) (end 1.675 -1.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.675 1.675) (end 1.675 1.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.675 -1.45) (end -2.9 -1.45) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.15)))
    )
    (pad 10 smd rect (at 2.2 -1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U2-Pad10)"))
    (pad 9 smd rect (at 2.2 -0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U2-Pad9)"))
    (pad 8 smd rect (at 2.2 0) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.2 0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 6 smd rect (at 2.2 1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.2 1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (pad 4 smd rect (at -2.2 0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R2-Pad2)"))
    (pad 3 smd rect (at -2.2 0) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U2-Pad3)"))
    (pad 2 smd rect (at -2.2 -0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U2-Pad2)"))
    (pad 1 smd rect (at -2.2 -1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:SO-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1) (tstamp 61BD2D3F)
    (at 69.845 44.9 270)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (path /61BD7233)
    (attr smd)
    (fp_text reference U1 (at 0 -3.4 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value STM32G031J6Mx (at 0 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 2.56) (end 1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 2.56) (end -1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end 1.95 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end -3.45 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 2.7) (end 3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.98 0.98) (thickness 0.15)))
    )
    (pad 8 smd roundrect (at 2.575 -1.905 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 2.575 -0.635 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(SW2-Pad2)"))
    (pad 6 smd roundrect (at 2.575 0.635 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R1-Pad2)"))
    (pad 5 smd roundrect (at 2.575 1.905 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R2-Pad2)"))
    (pad 4 smd roundrect (at -2.575 1.905 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -2.575 0.635 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -2.575 -0.635 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -2.575 -1.905 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 62.525 27.525) (end 97.5 27.475) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.525 55) (end 97.5 27.475) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 62.5 55) (end 97.525 55) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 62.525 27.525) (end 62.5 55) (layer Edge.Cuts) (width 0.05))

  (segment (start 87.525 41.595) (end 82.575 41.595) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 89.69 52.16) (end 90.225 51.625) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 87.525 52.16) (end 89.69 52.16) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 89.68 41.595) (end 90.25 41.025) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 87.525 41.595) (end 89.68 41.595) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 69.21 40.335) (end 68.4 39.525) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 69.21 42.325) (end 69.21 40.335) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 81.300001 46.135001) (end 81.060002 46.375) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.300001 44.814999) (end 81.300001 46.135001) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.210002 44.725) (end 81.300001 44.814999) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.275 44.725) (end 81.210002 44.725) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.060002 46.375) (end 80.4 46.375) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.4 46.375) (end 80.325 46.45) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.6 52.16) (end 82.575 52.16) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.325 50.885) (end 81.6 52.16) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.139998 47.025) (end 80.325 47.025) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 78.799989 45.684991) (end 80.139998 47.025) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 78.799989 41.900011) (end 78.799989 45.684991) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 79.35 41.35) (end 78.799989 41.900011) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.325 46.45) (end 80.325 47.025) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 90.4 41.025) (end 94.3 44.925) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 90.25 41.025) (end 90.4 41.025) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 80.325 50.225) (end 80.325 50.885) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.325 47.025) (end 80.325 50.225) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.325 50.225) (end 80.325 50.435) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 83.596758 48.99499) (end 84.085 49.483232) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 84.085 49.483232) (end 84.085 52.16) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.573222 48.99499) (end 83.596758 48.99499) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.27499 48.696758) (end 81.573222 48.99499) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.27499 48.003242) (end 81.27499 48.696758) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 82.575 46.703232) (end 81.27499 48.003242) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 82.575 41.595) (end 82.575 46.703232) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 84.085 52.16) (end 87.525 52.16) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 82.575 52.16) (end 84.085 52.16) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 77.47 34.88) (end 78.075 34.275) (width 1) (layer F.Cu) (net 1))
  (segment (start 73.875 34.88) (end 77.47 34.88) (width 1) (layer F.Cu) (net 1))
  (segment (start 78.075 34.275) (end 78.075 33.85) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 79.522502 41.375) (end 79.2 41.375) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.575001 40.322501) (end 79.522502 41.375) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.575001 36.775001) (end 80.575001 40.322501) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 78.075 34.275) (end 80.575001 36.775001) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 76.3 36.05) (end 76.3 39.2) (width 1) (layer F.Cu) (net 1))
  (segment (start 78.075 34.275) (end 76.3 36.05) (width 1) (layer F.Cu) (net 1))
  (segment (start 73.975 39.2) (end 73.75 38.975) (width 1) (layer F.Cu) (net 1))
  (segment (start 76.3 39.2) (end 73.975 39.2) (width 1) (layer F.Cu) (net 1))
  (segment (start 70.00001 37.92499) (end 68.4 39.525) (width 1) (layer F.Cu) (net 1))
  (segment (start 72.69999 37.92499) (end 70.00001 37.92499) (width 1) (layer F.Cu) (net 1))
  (segment (start 73.75 38.975) (end 72.69999 37.92499) (width 1) (layer F.Cu) (net 1))
  (segment (start 94.325 44.65) (end 94.325 43.375) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 70.48 41.45) (end 70.93001 40.99999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 70.48 42.325) (end 70.48 41.45) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 71.525 40.95) (end 71.47501 40.99999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 71.525 39.525) (end 71.525 40.95) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 70.93001 40.99999) (end 71.47501 40.99999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 73.875 32.6) (end 67.575 32.6) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 68.05 52.725) (end 68.025 52.75) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 70.48 42.778544) (end 70.48 42.325) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 67.18999 43.298534) (end 67.541466 43.65001) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 67.541466 43.65001) (end 69.608534 43.65001) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 67.28749 40.71248) (end 67.18999 40.80998) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 67.28749 32.88751) (end 67.28749 40.71248) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 69.608534 43.65001) (end 70.48 42.778544) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 67.575 32.6) (end 67.28749 32.88751) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 67.18999 43.18999) (end 67.18999 43.298534) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 67.18999 40.80998) (end 67.18999 43.18999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 64.8 49.275) (end 65.575 50.05) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 64.8 45.15) (end 64.8 49.275) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 65.575 52.55) (end 65.525 52.6) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 65.575 50.05) (end 65.575 52.55) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 66.85001 53.92501) (end 65.525 52.6) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 77.27499 53.92501) (end 66.85001 53.92501) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 79.375 51.825) (end 77.27499 53.92501) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 63.599999 43.949999) (end 64.8 45.15) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 63.599999 32.875001) (end 63.599999 43.949999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 63.875 32.6) (end 63.599999 32.875001) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 67.575 32.6) (end 63.875 32.6) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 79.339998 45.225) (end 80.275 45.225) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 80.002497 42.562501) (end 79.249999 43.314999) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 80.510001 42.562501) (end 80.002497 42.562501) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 79.249999 45.135001) (end 79.339998 45.225) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 81.02501 42.047492) (end 80.510001 42.562501) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 79.249999 43.314999) (end 79.249999 45.135001) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 80.335001 31.949999) (end 81.02501 32.640008) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 74.525001 31.949999) (end 80.335001 31.949999) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 81.02501 32.640008) (end 81.02501 42.047492) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 73.875 32.6) (end 74.525001 31.949999) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 74.7125 43.725) (end 75.875 43.725) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 73.75 42.7625) (end 74.7125 43.725) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 73.75 42.1) (end 73.75 42.7625) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 71.525 39.875) (end 73.75 42.1) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 71.525 39.525) (end 71.525 39.875) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 71.75 43.2) (end 71.75 42.325) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 70.59998 44.35002) (end 71.75 43.2) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 67.251513 44.35002) (end 70.59998 44.35002) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 66.000001 43.098508) (end 67.251513 44.35002) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 66.000001 38.550001) (end 66.000001 43.098508) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 64.8 37.35) (end 66.000001 38.550001) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 82.448232 39.055) (end 82.825 39.055) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 81.52499 39.978242) (end 82.448232 39.055) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 81.52499 43.42501) (end 81.52499 39.978242) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 81.225 43.725) (end 81.52499 43.42501) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 80.275 43.725) (end 81.225 43.725) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 80.824981 48.883159) (end 81.561822 49.62) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 80.82498 47.816842) (end 80.824981 48.883159) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 81.561822 49.62) (end 82.575 49.62) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 82.125 46.516822) (end 80.82498 47.816842) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 82.125 45.003588) (end 82.125 46.516822) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 81.346412 44.225) (end 82.125 45.003588) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 80.275 44.225) (end 81.346412 44.225) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 76.946412 44.725) (end 75.875 44.725) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 77.825001 43.846411) (end 76.946412 44.725) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 77.825001 39.399999) (end 77.825001 43.846411) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 78.05 39.175) (end 77.825001 39.399999) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 79.35 39.175) (end 78.05 39.175) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 76.900001 44.135001) (end 76.810002 44.225) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 76.900001 41.800001) (end 76.900001 44.135001) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 76.810002 44.225) (end 75.875 44.225) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 76.45 41.35) (end 76.900001 41.800001) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 87.525 48.35) (end 82.575 48.35) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 90.135 37.785) (end 90.25 37.9) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 87.525 37.785) (end 90.135 37.785) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 90.075 48.35) (end 90.225 48.5) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 87.525 48.35) (end 90.075 48.35) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 90.225 48.5) (end 90.6 48.5) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 90.6 48.5) (end 91.475 47.625) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 91.125001 37.024999) (end 90.25 37.9) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 96.685001 37.024999) (end 91.125001 37.024999) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 96.775001 37.114999) (end 96.685001 37.024999) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 96.775001 47.010001) (end 96.775001 37.114999) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 96.160002 47.625) (end 96.775001 47.010001) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 91.475 47.625) (end 96.160002 47.625) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 85.69 37.785) (end 82.575 37.785) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 87.525 37.785) (end 85.69 37.785) (width 0.5) (layer F.Cu) (net 14))
  (segment (start 93.925 32.625) (end 94.275 32.975) (width 1) (layer F.Cu) (net 8))
  (segment (start 89.85 32.625) (end 93.925 32.625) (width 1) (layer F.Cu) (net 8))
  (segment (start 94.3 39.85) (end 94.11249 39.66249) (width 1) (layer F.Cu) (net 9))
  (segment (start 94.11249 39.66249) (end 87.58749 39.66249) (width 1) (layer F.Cu) (net 9))
  (segment (start 87.525 39.6) (end 87.525 40.325) (width 0.5) (layer F.Cu) (net 9))
  (segment (start 87.58749 39.66249) (end 87.525 39.6) (width 1) (layer F.Cu) (net 9))
  (segment (start 87.525 39.055) (end 87.525 39.6) (width 0.5) (layer F.Cu) (net 9))
  (segment (start 87.66251 50.26249) (end 87.525 50.4) (width 1) (layer F.Cu) (net 10))
  (segment (start 94.08749 50.26249) (end 87.66251 50.26249) (width 1) (layer F.Cu) (net 10))
  (segment (start 94.3 50.475) (end 94.08749 50.26249) (width 1) (layer F.Cu) (net 10))
  (segment (start 87.525 50.4) (end 87.525 50.89) (width 0.5) (layer F.Cu) (net 10))
  (segment (start 87.525 49.62) (end 87.525 50.4) (width 0.5) (layer F.Cu) (net 10))
  (segment (start 69.53501 46.27499) (end 75.19999 46.27499) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 69.21 46.6) (end 69.53501 46.27499) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 69.21 47.475) (end 69.21 46.6) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 75.74998 45.725) (end 75.875 45.725) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 75.19999 46.27499) (end 75.74998 45.725) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 69.21 49.515) (end 69.21 47.475) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 68.675 50.05) (end 69.21 49.515) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 74.775 45.225) (end 75.875 45.225) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 74.17502 45.82498) (end 74.775 45.225) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 68.71502 45.82498) (end 74.17502 45.82498) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 67.94 46.6) (end 68.71502 45.82498) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 67.94 47.475) (end 67.94 46.6) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 67.57499 51.54999) (end 68.625 52.6) (width 0.5) (layer F.Cu) (net 12))
  (segment (start 67.57499 47.84001) (end 67.57499 51.54999) (width 0.5) (layer F.Cu) (net 12))
  (segment (start 67.94 47.475) (end 67.57499 47.84001) (width 0.5) (layer F.Cu) (net 12))
  (segment (start 70.48 50.73) (end 71.575 51.825) (width 0.5) (layer F.Cu) (net 13))
  (segment (start 70.48 47.475) (end 70.48 50.73) (width 0.5) (layer F.Cu) (net 13))
  (segment (start 80.995 30.32) (end 83.3 32.625) (width 1) (layer F.Cu) (net 14))
  (segment (start 73.875 30.32) (end 80.995 30.32) (width 1) (layer F.Cu) (net 14))
  (segment (start 83.3 32.625) (end 87.175 36.5) (width 1) (layer F.Cu) (net 14))
  (segment (start 88.85 36.5) (end 90.25 37.9) (width 1) (layer F.Cu) (net 14))
  (segment (start 87.175 36.5) (end 88.85 36.5) (width 1) (layer F.Cu) (net 14))

)
