(kicad_pcb (version 20171130) (host pcbnew 5.99.0+really5.1.12+dfsg1-1)

  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 163)
    (zones 0)
    (modules 21)
    (nets 16)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(SW1-Pad2)")
  (net 4 "Net-(U2-Pad10)")
  (net 5 "Net-(U2-Pad9)")
  (net 6 "Net-(U2-Pad3)")
  (net 7 "Net-(U2-Pad2)")
  (net 8 +12V)
  (net 9 "Net-(J1-Pad1)")
  (net 10 "Net-(J2-Pad1)")
  (net 11 "Net-(R1-Pad2)")
  (net 12 "Net-(R2-Pad2)")
  (net 13 "Net-(C1-Pad1)")
  (net 14 "Net-(J6-Pad4)")
  (net 15 "Net-(J6-Pad3)")

  (net_class Default "Questo è il gruppo di collegamenti predefinito"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad9)")
  )

  (module Capacitor_SMD:C_1812_4532Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 61D41F81)
    (at 86.85 45.075 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /61E06150)
    (attr smd)
    (fp_text reference C5 (at 0 -2.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220n (at 0 2.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.25 1.6) (end -2.25 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -2.25 -1.6) (end 2.25 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.25 -1.6) (end 2.25 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.25 1.6) (end -2.25 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1.161252 -1.71) (end 1.161252 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.161252 1.71) (end 1.161252 1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 1.95) (end -3 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 -1.95) (end 3 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3 -1.95) (end 3 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3 1.95) (end -3 1.95) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 2.05 0 180) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.178571)
      (net 13 "Net-(C1-Pad1)"))
    (pad 1 smd roundrect (at -2.05 0 180) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.178571)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 61D2D22D)
    (at 66.225 52.625)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /61BEE388)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 5k6 (at 0 1.82) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.45 1.12) (end -2.45 -1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.45 -1.12) (end 2.45 -1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.45 -1.12) (end 2.45 1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.45 1.12) (end -2.45 1.12) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 12 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 61BD5677)
    (at 69.7625 38.2 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /61C2BA36)
    (attr smd)
    (fp_text reference C3 (at 0 -1.85) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150n (at 0 1.85) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left (layer F.Cu) (tedit 59FED5CC) (tstamp 61D3F292)
    (at 75.245 51.23 270)
    (descr "surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x04 2.54mm single row style1 pin1 left")
    (path /61DE3E97)
    (attr smd)
    (fp_text reference J6 (at 0 -6.14 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04_Female (at 0 6.14 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 5.08) (end -1.27 5.08) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -5.08) (end 1.27 -5.08) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 5.08) (end -1.27 -4.13) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -4.13) (end -0.32 -5.08) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -5.08) (end 1.27 5.08) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -4.13) (end -2.54 -4.13) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -4.13) (end -2.54 -3.49) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -3.49) (end -1.27 -3.49) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 0.95) (end -2.54 0.95) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 0.95) (end -2.54 1.59) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 1.59) (end -1.27 1.59) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.59) (end 2.54 -1.59) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -1.59) (end 2.54 -0.95) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -0.95) (end 1.27 -0.95) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.49) (end 2.54 3.49) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 3.49) (end 2.54 4.13) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 4.13) (end 1.27 4.13) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 -5.14) (end 1.33 -5.14) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 5.14) (end 1.33 5.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -5.14) (end 1.33 -2.03) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -4.57) (end -2.85 -4.57) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -5.14) (end -1.33 -4.57) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 4.57) (end 1.33 5.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -0.51) (end 1.33 3.05) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -3.05) (end -1.33 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 2.03) (end -1.33 5.14) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.45 -5.6) (end -3.45 5.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.45 5.6) (end 3.45 5.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 5.6) (end 3.45 -5.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 -5.6) (end -3.45 -5.6) (layer F.CrtYd) (width 0.05))
    (pad 4 smd rect (at 1.655 3.81 270) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J6-Pad4)"))
    (pad 2 smd rect (at 1.655 -1.27 270) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at -1.655 1.27 270) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J6-Pad3)"))
    (pad 1 smd rect (at -1.655 -3.81 270) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5A02FF57) (tstamp 61D3A92F)
    (at 70.575 32.525 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (path /61DBDBE5)
    (attr smd)
    (fp_text reference U5 (at 0 -4.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LD1117S33TR_SOT223 (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.85 -3.35) (end 1.85 3.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1.85 3.35) (end 1.85 3.35) (layer F.Fab) (width 0.1))
    (fp_line (start -4.1 -3.41) (end 1.91 -3.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.85 -3.35) (end 1.85 -3.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1.85 3.41) (end 1.91 3.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 -2.35) (end -1.85 3.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1.85 -2.35) (end -0.85 -3.35) (layer F.Fab) (width 0.1))
    (fp_line (start -4.4 -3.6) (end -4.4 3.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.4 3.6) (end 4.4 3.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.4 3.6) (end 4.4 -3.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.4 -3.6) (end -4.4 -3.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.91 -3.41) (end 1.91 -2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.91 3.41) (end 1.91 2.15) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Button_Switch_SMD:SW_SPST_CK_RS282G05A3 (layer F.Cu) (tedit 5A7A67D2) (tstamp 61BD3C07)
    (at 64.8 41.25 90)
    (descr https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf)
    (tags "SPST button tactile switch")
    (path /61C14AD4)
    (attr smd)
    (fp_text reference SW1 (at 0 -2.6 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3 -1.8) (end 3 1.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -1.8) (end -3 1.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -1.8) (end 3 -1.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3 1.8) (end 3 1.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 -0.8) (end -1.5 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -0.8) (end 1.5 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 -0.8) (end 1.5 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 0.8) (end 1.5 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.06 1.85) (end -3.06 -1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 1.85) (end -3.06 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 -1.85) (end 3.06 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.06 -1.85) (end 3.06 -1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.75 1) (end -1.75 -1) (layer F.Fab) (width 0.1))
    (fp_line (start 1.75 1) (end -1.75 1) (layer F.Fab) (width 0.1))
    (fp_line (start 1.75 -1) (end 1.75 1) (layer F.Fab) (width 0.1))
    (fp_line (start -1.75 -1) (end 1.75 -1) (layer F.Fab) (width 0.1))
    (fp_line (start -4.9 -2.05) (end 4.9 -2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 -2.05) (end 4.9 2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 2.05) (end -4.9 2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.9 2.05) (end -4.9 -2.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -2.6 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.9 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(SW1-Pad2)"))
    (pad 1 smd rect (at -3.9 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_SMD:D_3220_8050Metric_Pad2.65x5.15mm_HandSolder (layer F.Cu) (tedit 5F68FEF0) (tstamp 61D3822D)
    (at 86.575 32.625)
    (descr "Diode SMD 3220 (8050 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (path /61D9D085)
    (attr smd)
    (fp_text reference D1 (at 0 -3.52) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 0 3.52) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.85 2.82) (end -4.85 2.82) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.85 -2.82) (end 4.85 2.82) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.85 -2.82) (end 4.85 -2.82) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.85 2.82) (end -4.85 -2.82) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.86 2.835) (end 4 2.835) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.86 -2.835) (end -4.86 2.835) (layer F.SilkS) (width 0.12))
    (fp_line (start 4 -2.835) (end -4.86 -2.835) (layer F.SilkS) (width 0.12))
    (fp_line (start 4 2.5) (end 4 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -4 2.5) (end 4 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -4 -1.5) (end -4 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.5) (end -4 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 4 -2.5) (end -3 -2.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd roundrect (at 3.275 0) (size 2.65 5.15) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09433999999999999)
      (net 8 +12V))
    (pad 1 smd roundrect (at -3.275 0) (size 2.65 5.15) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09433999999999999)
      (net 13 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_3220_8050Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F) (tstamp 61D34121)
    (at 94.325 44.65)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (path /61D73449)
    (attr virtual)
    (fp_text reference J5 (at 0 -2.898) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MOSFETGND (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 1 GND))
  )

  (module Crystal:Crystal_SMD_SeikoEpson_TSX3225-4Pin_3.2x2.5mm_HandSoldering (layer F.Cu) (tedit 5A0FD1B2) (tstamp 61D3179C)
    (at 77.75 40.2875)
    (descr "crystal Epson Toyocom TSX-3225 series https://support.epson.biz/td/api/doc_check.php?dl=brief_fa-238v_en.pdf, hand-soldering, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (path /61D4D30B)
    (attr smd)
    (fp_text reference Y1 (at 0 -2.95) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Crystal_GND24 (at 0 2.95) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.8 -2.2) (end -2.8 -2.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.8 2.2) (end 2.8 -2.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 2.2) (end 2.8 2.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 -2.2) (end -2.8 2.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 2.15) (end 2.7 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -2.15) (end -2.7 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 0.25) (end -0.6 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -1.15) (end -1.5 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 1.15) (end -1.6 -1.15) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 1.25) (end -1.6 1.15) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 1.25) (end -1.5 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 1.15) (end 1.5 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -1.15) (end 1.6 1.15) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -1.25) (end 1.6 -1.15) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 -1.25) (end 1.5 -1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.7 0.7) (thickness 0.105)))
    )
    (pad 4 smd rect (at -1.45 -1.0875) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.45 -1.0875) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U2-Pad3)"))
    (pad 2 smd rect (at 1.45 1.0875) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.45 1.0875) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U2-Pad2)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_SeikoEpson_TSX3225-4Pin_3.2x2.5mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F) (tstamp 61D30632)
    (at 94.275 32.975)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (path /61D4A334)
    (attr virtual)
    (fp_text reference J4 (at 0 -2.898) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 8 +12V))
  )

  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1) (tstamp 61D39FB7)
    (at 85.3 39.69)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (path /6170CD01)
    (attr smd)
    (fp_text reference U3 (at 0 -3.4) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IXDN609PI (at 0 3.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.98 0.98) (thickness 0.15)))
    )
    (fp_line (start 0 2.56) (end 1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 2.56) (end -1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end 1.95 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end -3.45 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 2.7) (end 3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(U2-Pad10)"))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(J1-Pad1)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(J1-Pad1)"))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 61BD5655)
    (at 90.25 39.4625 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /617245F7)
    (attr smd)
    (fp_text reference C1 (at 0 -1.85 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220n (at 0 1.85 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 13 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1) (tstamp 61BD2D92)
    (at 85.05 50.255)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (path /6170DA36)
    (attr smd)
    (fp_text reference U4 (at 0 -3.4) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IXDN609PI (at 0 3.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.98 0.98) (thickness 0.15)))
    )
    (fp_line (start 0 2.56) (end 1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 2.56) (end -1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end 1.95 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end -3.45 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 2.7) (end 3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(U2-Pad9)"))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(J2-Pad1)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(J2-Pad1)"))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F) (tstamp 61D33C2A)
    (at 78.075 34.275)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (path /61D33D93)
    (attr virtual)
    (fp_text reference J3 (at 0 -2.898) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 1 GND))
  )

  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F) (tstamp 61D2EC39)
    (at 94.3 50.475)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (path /61C2A1B5)
    (attr virtual)
    (fp_text reference J2 (at 0 -2.898) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 10 "Net-(J2-Pad1)"))
  )

  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F) (tstamp 61D2ECD8)
    (at 94.325 39.475)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (path /61C293CA)
    (attr virtual)
    (fp_text reference J1 (at 0 -2.898) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 9 "Net-(J1-Pad1)"))
  )

  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 61D2D21C)
    (at 66.25 49.975)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /61BED99B)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 5k6 (at 0 1.82) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.45 1.12) (end -2.45 -1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.45 -1.12) (end 2.45 -1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.45 -1.12) (end 2.45 1.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.45 1.12) (end -2.45 1.12) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 11 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 61D2D999)
    (at 73.75 40.5375 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /61C2AF29)
    (attr smd)
    (fp_text reference C4 (at 0 -1.85 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150n (at 0 1.85 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 61BD5666)
    (at 90.225 50.0625 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /617264A4)
    (attr smd)
    (fp_text reference C2 (at 0 -1.85 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220n (at 0 1.85 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 13 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:MSOP-10_3x3mm_P0.5mm (layer F.Cu) (tedit 5A02F25C) (tstamp 61D2F9FE)
    (at 78.075 44.725)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (path /61BD2F46)
    (attr smd)
    (fp_text reference U2 (at 0 -2.6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Si5351A-B-GT (at 0 2.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.15)))
    )
    (fp_line (start -0.5 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.15))
    (fp_line (start -1.5 1.5) (end -1.5 -0.5) (layer F.Fab) (width 0.15))
    (fp_line (start -1.5 -0.5) (end -0.5 -1.5) (layer F.Fab) (width 0.15))
    (fp_line (start -3.15 -1.85) (end -3.15 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.15 -1.85) (end 3.15 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.15 -1.85) (end 3.15 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.15 1.85) (end 3.15 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.675 -1.675) (end -1.675 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.675 -1.675) (end 1.675 -1.375) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.675 1.675) (end 1.675 1.375) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.675 1.675) (end -1.675 1.375) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.675 -1.675) (end 1.675 -1.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.675 1.675) (end 1.675 1.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.675 -1.45) (end -2.9 -1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.2 -1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -2.2 -0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -2.2 0) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -2.2 0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R2-Pad2)"))
    (pad 5 smd rect (at -2.2 1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (pad 6 smd rect (at 2.2 1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.2 0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 8 smd rect (at 2.2 0) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.2 -0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 2.2 -1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U2-Pad10)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:SO-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1) (tstamp 61BD2D3F)
    (at 69.72 43.85 270)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (path /61BD7233)
    (attr smd)
    (fp_text reference U1 (at 0 -3.4 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value STM32G031J6Mx (at 0 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.98 0.98) (thickness 0.15)))
    )
    (fp_line (start 0 2.56) (end 1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 2.56) (end -1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end 1.95 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end -3.45 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 2.7) (end 3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd roundrect (at -2.575 -1.905 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(SW1-Pad2)"))
    (pad 2 smd roundrect (at -2.575 -0.635 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 3 smd roundrect (at -2.575 0.635 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -2.575 1.905 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at 2.575 1.905 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R2-Pad2)"))
    (pad 6 smd roundrect (at 2.575 0.635 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R1-Pad2)"))
    (pad 7 smd roundrect (at 2.575 -0.635 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(J6-Pad4)"))
    (pad 8 smd roundrect (at 2.575 -1.905 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 62.5 28.75) (end 97.5 28.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.525 55) (end 97.5 28.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 62.5 55) (end 97.525 55) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 62.5 28.75) (end 62.5 55) (layer Edge.Cuts) (width 0.05))

  (segment (start 87.525 41.595) (end 82.575 41.595) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 89.69 52.16) (end 90.225 51.625) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 87.525 52.16) (end 89.69 52.16) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 89.68 41.595) (end 90.25 41.025) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 87.525 41.595) (end 89.68 41.595) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 81.300001 46.135001) (end 81.060002 46.375) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.300001 44.814999) (end 81.300001 46.135001) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.210002 44.725) (end 81.300001 44.814999) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.275 44.725) (end 81.210002 44.725) (width 0.25) (layer F.Cu) (net 1) (status 10))
  (segment (start 81.060002 46.375) (end 80.4 46.375) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.4 46.375) (end 80.325 46.45) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.6 52.16) (end 82.575 52.16) (width 0.25) (layer F.Cu) (net 1) (status 30))
  (segment (start 80.325 50.885) (end 81.6 52.16) (width 0.25) (layer F.Cu) (net 1) (status 20))
  (segment (start 80.139998 47.025) (end 80.325 47.025) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 78.799989 45.684991) (end 80.139998 47.025) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 78.799989 41.900011) (end 78.799989 45.684991) (width 0.25) (layer F.Cu) (net 1) (status 10))
  (segment (start 79.35 41.35) (end 78.799989 41.900011) (width 0.25) (layer F.Cu) (net 1) (status 30))
  (segment (start 80.325 46.45) (end 80.325 47.025) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 90.4 41.025) (end 94.3 44.925) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 90.25 41.025) (end 90.4 41.025) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 80.325 50.225) (end 80.325 50.885) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.325 47.025) (end 80.325 50.225) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 80.325 50.225) (end 80.325 50.435) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 83.596758 48.99499) (end 84.085 49.483232) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 84.085 49.483232) (end 84.085 52.16) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.573222 48.99499) (end 83.596758 48.99499) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.27499 48.696758) (end 81.573222 48.99499) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.27499 48.003242) (end 81.27499 48.696758) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 82.575 46.703232) (end 81.27499 48.003242) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 82.575 41.595) (end 82.575 46.703232) (width 0.25) (layer F.Cu) (net 1) (status 10))
  (segment (start 84.085 52.16) (end 87.525 52.16) (width 0.5) (layer F.Cu) (net 1) (status 20))
  (segment (start 82.575 52.16) (end 84.085 52.16) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 77.47 34.88) (end 78.075 34.275) (width 1) (layer F.Cu) (net 1) (status 30))
  (segment (start 73.875 34.88) (end 77.47 34.88) (width 1) (layer F.Cu) (net 1) (status 30))
  (segment (start 78.075 34.275) (end 78.075 33.85) (width 0.25) (layer F.Cu) (net 1) (status 30))
  (segment (start 79.522502 41.375) (end 79.2 41.375) (width 0.25) (layer F.Cu) (net 1) (status 30))
  (segment (start 80.575001 40.322501) (end 79.522502 41.375) (width 0.25) (layer F.Cu) (net 1) (status 20))
  (segment (start 80.575001 36.775001) (end 80.575001 40.322501) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 78.075 34.275) (end 80.575001 36.775001) (width 0.25) (layer F.Cu) (net 1) (status 10))
  (segment (start 76.3 36.05) (end 76.3 39.2) (width 1) (layer F.Cu) (net 1) (status 30))
  (segment (start 78.075 34.275) (end 76.3 36.05) (width 1) (layer F.Cu) (net 1) (status 30))
  (segment (start 73.975 39.2) (end 73.75 38.975) (width 1) (layer F.Cu) (net 1) (status 30))
  (segment (start 76.3 39.2) (end 73.975 39.2) (width 1) (layer F.Cu) (net 1) (status 30))
  (segment (start 94.325 44.65) (end 94.325 43.375) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 69.085 39.085) (end 69.085 41.275) (width 0.5) (layer F.Cu) (net 1) (status 20))
  (segment (start 68.2 38.2) (end 69.085 39.085) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 71.575 34.825) (end 73.725 34.825) (width 0.5) (layer F.Cu) (net 1) (status 20))
  (segment (start 68.2 38.2) (end 71.575 34.825) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 79.215 49.775) (end 80.325 50.885) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 79.055 49.775) (end 79.215 49.775) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 93.9 45.075) (end 94.325 44.65) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 88.9 45.075) (end 93.9 45.075) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 73.875 32.6) (end 67.575 32.6) (width 0.5) (layer F.Cu) (net 2) (status 30))
  (segment (start 63.599999 43.949999) (end 64.8 45.15) (width 0.5) (layer F.Cu) (net 2) (status 20))
  (segment (start 63.599999 32.875001) (end 63.599999 43.949999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 63.875 32.6) (end 63.599999 32.875001) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 67.575 32.6) (end 63.875 32.6) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 74.7125 43.725) (end 75.875 43.725) (width 0.25) (layer F.Cu) (net 2) (status 20))
  (segment (start 73.75 42.7625) (end 74.7125 43.725) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 73.75 42.1) (end 73.75 42.7625) (width 0.25) (layer F.Cu) (net 2) (status 10))
  (segment (start 70.355 39.17) (end 71.325 38.2) (width 0.5) (layer F.Cu) (net 2) (status 20))
  (segment (start 70.355 41.275) (end 70.355 39.17) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 73.75 41.4375) (end 73.75 42.1) (width 0.5) (layer F.Cu) (net 2) (status 30))
  (segment (start 72.26249 39.94999) (end 73.75 41.4375) (width 0.5) (layer F.Cu) (net 2) (status 20))
  (segment (start 70.80501 39.94999) (end 72.26249 39.94999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 70.355 40.4) (end 70.80501 39.94999) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 70.355 41.275) (end 70.355 40.4) (width 0.5) (layer F.Cu) (net 2) (status 30))
  (segment (start 64.8 52.5) (end 64.675 52.625) (width 0.5) (layer F.Cu) (net 2) (status 30))
  (segment (start 64.8 45.15) (end 64.8 52.5) (width 0.5) (layer F.Cu) (net 2) (status 30))
  (segment (start 71.650029 44.199971) (end 73.75 42.1) (width 0.5) (layer F.Cu) (net 2) (status 20))
  (segment (start 65.750029 44.199971) (end 71.650029 44.199971) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 64.8 45.15) (end 65.750029 44.199971) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 66.515001 54.465001) (end 64.675 52.625) (width 0.25) (layer F.Cu) (net 2) (status 20))
  (segment (start 74.934999 54.465001) (end 66.515001 54.465001) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 76.515 52.885) (end 74.934999 54.465001) (width 0.25) (layer F.Cu) (net 2) (status 10))
  (segment (start 79.339998 45.225) (end 80.275 45.225) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 79.249999 45.135001) (end 79.339998 45.225) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 80.510001 42.562501) (end 79.249999 42.562501) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 79.249999 42.562501) (end 79.249999 45.135001) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 81.02501 42.047492) (end 80.510001 42.562501) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 81.02501 32.640008) (end 81.02501 42.047492) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 80.335001 31.949999) (end 81.02501 32.640008) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 74.300001 31.949999) (end 80.335001 31.949999) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 73.725 32.525) (end 74.300001 31.949999) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 71.625 41.551768) (end 71.625 41.275) (width 0.25) (layer F.Cu) (net 3) (status 30))
  (segment (start 67.468242 42.47501) (end 70.701758 42.47501) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 70.701758 42.47501) (end 71.625 41.551768) (width 0.25) (layer F.Cu) (net 3) (status 20))
  (segment (start 64.8 39.806768) (end 67.468242 42.47501) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 64.8 37.35) (end 64.8 39.806768) (width 0.25) (layer F.Cu) (net 3) (status 10))
  (segment (start 82.448232 39.055) (end 82.825 39.055) (width 0.25) (layer F.Cu) (net 4) (status 30))
  (segment (start 81.52499 39.978242) (end 82.448232 39.055) (width 0.25) (layer F.Cu) (net 4) (status 20))
  (segment (start 81.52499 43.42501) (end 81.52499 39.978242) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 81.225 43.725) (end 81.52499 43.42501) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 80.275 43.725) (end 81.225 43.725) (width 0.25) (layer F.Cu) (net 4) (status 10))
  (segment (start 80.824981 48.883159) (end 81.561822 49.62) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 80.82498 47.816842) (end 80.824981 48.883159) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 81.561822 49.62) (end 82.575 49.62) (width 0.25) (layer F.Cu) (net 5) (status 20))
  (segment (start 82.125 46.516822) (end 80.82498 47.816842) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 82.125 45.003588) (end 82.125 46.516822) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 81.346412 44.225) (end 82.125 45.003588) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 80.275 44.225) (end 81.346412 44.225) (width 0.25) (layer F.Cu) (net 5) (status 10))
  (segment (start 76.946412 44.725) (end 75.875 44.725) (width 0.25) (layer F.Cu) (net 6) (status 20))
  (segment (start 77.825001 43.846411) (end 76.946412 44.725) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 77.825001 39.399999) (end 77.825001 43.846411) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 78.05 39.175) (end 77.825001 39.399999) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 79.35 39.175) (end 78.05 39.175) (width 0.25) (layer F.Cu) (net 6) (status 10))
  (segment (start 76.900001 44.135001) (end 76.810002 44.225) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 76.900001 41.800001) (end 76.900001 44.135001) (width 0.25) (layer F.Cu) (net 7) (status 10))
  (segment (start 76.810002 44.225) (end 75.875 44.225) (width 0.25) (layer F.Cu) (net 7) (status 20))
  (segment (start 76.45 41.35) (end 76.900001 41.800001) (width 0.25) (layer F.Cu) (net 7) (status 30))
  (segment (start 93.925 32.625) (end 94.275 32.975) (width 1) (layer F.Cu) (net 8) (status 30))
  (segment (start 89.85 32.625) (end 93.925 32.625) (width 1) (layer F.Cu) (net 8) (status 30))
  (segment (start 94.3 39.85) (end 94.11249 39.66249) (width 1) (layer F.Cu) (net 9) (status 30))
  (segment (start 94.11249 39.66249) (end 87.58749 39.66249) (width 1) (layer F.Cu) (net 9) (status 10))
  (segment (start 87.525 39.6) (end 87.525 40.325) (width 0.5) (layer F.Cu) (net 9) (status 20))
  (segment (start 87.58749 39.66249) (end 87.525 39.6) (width 1) (layer F.Cu) (net 9))
  (segment (start 87.525 39.055) (end 87.525 39.6) (width 0.5) (layer F.Cu) (net 9) (status 10))
  (segment (start 87.66251 50.26249) (end 87.525 50.4) (width 1) (layer F.Cu) (net 10))
  (segment (start 94.08749 50.26249) (end 87.66251 50.26249) (width 1) (layer F.Cu) (net 10) (status 10))
  (segment (start 94.3 50.475) (end 94.08749 50.26249) (width 1) (layer F.Cu) (net 10) (status 30))
  (segment (start 87.525 50.4) (end 87.525 50.89) (width 0.5) (layer F.Cu) (net 10) (status 20))
  (segment (start 87.525 49.62) (end 87.525 50.4) (width 0.5) (layer F.Cu) (net 10) (status 10))
  (segment (start 74.925 45.725) (end 75.875 45.725) (width 0.25) (layer F.Cu) (net 11) (status 20))
  (segment (start 74.42499 45.22499) (end 74.925 45.725) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 69.41001 45.22499) (end 74.42499 45.22499) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 69.085 45.55) (end 69.41001 45.22499) (width 0.25) (layer F.Cu) (net 11) (status 10))
  (segment (start 69.085 46.425) (end 69.085 45.55) (width 0.25) (layer F.Cu) (net 11) (status 30))
  (segment (start 69.085 48.69) (end 69.085 46.425) (width 0.5) (layer F.Cu) (net 11) (status 20))
  (segment (start 67.8 49.975) (end 69.085 48.69) (width 0.5) (layer F.Cu) (net 11) (status 10))
  (segment (start 74.611391 44.774981) (end 75.06141 45.225) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 68.590021 44.77498) (end 74.611391 44.774981) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 75.06141 45.225) (end 75.875 45.225) (width 0.25) (layer F.Cu) (net 12) (status 20))
  (segment (start 67.815 45.55) (end 68.590021 44.77498) (width 0.25) (layer F.Cu) (net 12) (status 10))
  (segment (start 67.815 46.425) (end 67.815 45.55) (width 0.25) (layer F.Cu) (net 12) (status 30))
  (segment (start 66.69999 51.54999) (end 67.775 52.625) (width 0.5) (layer F.Cu) (net 12) (status 20))
  (segment (start 66.69999 47.54001) (end 66.69999 51.54999) (width 0.5) (layer F.Cu) (net 12))
  (segment (start 67.815 46.425) (end 66.69999 47.54001) (width 0.5) (layer F.Cu) (net 12) (status 10))
  (segment (start 90.135 37.785) (end 90.25 37.9) (width 0.5) (layer F.Cu) (net 13) (status 30))
  (segment (start 87.525 37.785) (end 90.135 37.785) (width 0.5) (layer F.Cu) (net 13) (status 30))
  (segment (start 90.075 48.35) (end 90.225 48.5) (width 0.5) (layer F.Cu) (net 13) (status 30))
  (segment (start 87.525 48.35) (end 90.075 48.35) (width 0.5) (layer F.Cu) (net 13) (status 30))
  (segment (start 90.225 48.5) (end 90.6 48.5) (width 0.5) (layer F.Cu) (net 13) (status 30))
  (segment (start 90.6 48.5) (end 91.475 47.625) (width 0.5) (layer F.Cu) (net 13) (status 10))
  (segment (start 91.125001 37.024999) (end 90.25 37.9) (width 0.5) (layer F.Cu) (net 13) (status 20))
  (segment (start 96.685001 37.024999) (end 91.125001 37.024999) (width 0.5) (layer F.Cu) (net 13))
  (segment (start 96.775001 37.114999) (end 96.685001 37.024999) (width 0.5) (layer F.Cu) (net 13))
  (segment (start 96.775001 47.010001) (end 96.775001 37.114999) (width 0.5) (layer F.Cu) (net 13))
  (segment (start 96.160002 47.625) (end 96.775001 47.010001) (width 0.5) (layer F.Cu) (net 13))
  (segment (start 91.475 47.625) (end 96.160002 47.625) (width 0.5) (layer F.Cu) (net 13))
  (segment (start 87.525 37.785) (end 82.575 37.785) (width 0.5) (layer F.Cu) (net 13) (status 30))
  (segment (start 80.995 30.32) (end 83.3 32.625) (width 1) (layer F.Cu) (net 13) (status 20))
  (segment (start 73.875 30.32) (end 80.995 30.32) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 83.3 32.625) (end 87.175 36.5) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 88.85 36.5) (end 90.25 37.9) (width 1) (layer F.Cu) (net 13) (status 20))
  (segment (start 87.175 36.5) (end 88.85 36.5) (width 1) (layer F.Cu) (net 13))
  (segment (start 84.8 48.15) (end 85 48.35) (width 0.5) (layer F.Cu) (net 13))
  (segment (start 84.8 45.075) (end 84.8 48.15) (width 0.5) (layer F.Cu) (net 13) (status 10))
  (segment (start 85 48.35) (end 82.575 48.35) (width 0.5) (layer F.Cu) (net 13) (status 20))
  (segment (start 87.525 48.35) (end 85 48.35) (width 0.5) (layer F.Cu) (net 13) (status 10))
  (segment (start 70.355 52.005) (end 71.435 53.085) (width 0.5) (layer F.Cu) (net 14) (status 20))
  (segment (start 70.355 46.425) (end 70.355 52.005) (width 0.5) (layer F.Cu) (net 14) (status 10))
  (segment (start 71.625 47.425) (end 73.975 49.775) (width 0.5) (layer F.Cu) (net 15) (status 20))
  (segment (start 71.625 46.425) (end 71.625 47.425) (width 0.5) (layer F.Cu) (net 15) (status 10))

)
